Project Name:	Regional
	Project Code:	REG	Site ID:	T148	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G. Smith	Locality:	5.4KM west of Thirlestone turnoff on new road 
	leading west from Yarrowmere:
	Date Desc.:	08/09/70	Elevation:	No Data
	Map Ref.:	Sheet No. : 8054   1:100000	Rainfall:	480
	Northing/Long.:	145.55	Runoff:	Moderately rapid
	Easting/Lat.:	-21.5333333333333	Drainage:	Well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qs	Substrate Material:	Undisturbed soil core, 3.8 m 
	deep,Sandstone 
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Plain
	Morph. Type:	Upper-slope	Relief:	15 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Mesotrophic Red Kandosol     	Principal Profile Form:	Gn2.14
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus setosa, Grevillea species
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.1 m	Dark reddish brown (5YR3/3-Moist); Brown (7.5YR5/4-Dry); ; Loamy sand (Heavy); Massive grade 
	of structure; Dry; Very strong consistence; Common, fine (1-2mm) roots; Clear change to - 
	A2	0.1 - 0.2 m	Red (2.5YR4/7-Moist); Red (2.5YR5/6-Dry); ; Sandy loam (Light); Massive grade of structure; Dry; 
	Strong consistence; Few, fine (1-2mm) roots; Gradual change to - 
	B1	0.2 - 0.3 m	Dark red (2.5YR3/8-Moist); Red (2.5YR5/8-Dry); ; Sandy loam; Massive grade of structure; Earthy 
	fabric; Dry; Very strong consistence; Gradual change to - 
	B1	0.3 - 0.4 m	Dark red (2.5YR3/8-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; Dry; Rigid 
	consistence; Gradual change to - 
	B21	0.4 - 0.5 m	Dark red (2.5YR3/8-Moist); ; Sandy clay loam (Light); Massive grade of structure; Earthy fabric; 
	Dry; Rigid consistence; Gradual change to - 
	B21	0.5 - 0.6 m	Dark red (2.5YR3/8-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; Dry; 
	Rigid consistence; Gradual change to - 
	B21	0.6 - 0.75 m	Dark red (2.5YR3/8-Moist); ; Sandy clay loam (Heavy); Massive grade of structure; Earthy fabric; 
	Dry; Rigid consistence; Gradual change to - 
	B22	0.75 - 0.9 m	Dark red (2.5YR3/8-Moist); ; Sandy medium clay; Massive grade of structure; Earthy fabric; Dry; 
	Rigid consistence; Gradual change to - 
	B22	0.9 - 1.05 m	Dark red (2.5YR3/8-Moist); ; Sandy medium clay; Massive grade of structure; Earthy fabric; Dry; 
	Very strong consistence; Gradual change to - 
	B22	1.05 - 1.2 m	Dark red (2.5YR3/8-Moist); ; Sandy medium clay; Massive grade of structure; Earthy fabric; Dry; 
	Very strong consistence; Gradual change to - 
	B22	1.2 - 1.5 m	Dark red (2.5YR3/8-Moist); ; Sandy medium clay; Massive grade of structure; Earthy fabric; Dry; 
	Very strong consistence; Gradual change to - 
	B22	1.5 - 1.8 m	Dark red (2.5YR3/8-Moist); ; Sandy medium clay; Massive grade of structure; Earthy fabric; Dry; 
	Strong consistence; Common (10 - 20 %), Argillaceous, , Nodules; Gradual change to - 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T148	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	1.8 - 2.1 m	Dark red (2.5YR3/8-Moist); ; Fine sandy clay loam (Heavy); Massive grade of structure; Very 
	strong consistence; , Argillaceous, Very coarse (20 - 60 mm), Nodules; Gradual change to - 
	2.1 - 2.4 m	Dark red (2.5YR3/8-Moist); ; Fine sandy clay loam; Massive grade of structure; Very strong 
	consistence; , Argillaceous, Very coarse (20 - 60 mm), Nodules; Gradual change to - 
	2.4 - 2.7 m	Dark red (2.5YR3/8-Moist); ; Fine sandy clay loam; Massive grade of structure; Rigid 
	consistence; Few (2 - 10 %), Argillaceous, , Nodules; Gradual change to - 
	2.7 - 3 m	Dark red (2.5YR3/8-Moist); ; Fine sandy clay loam (Light); Massive grade of structure; Rigid 
	consistence; Gradual change to - 
	3 - 3.3 m	Dark red (2.5YR3/8-Moist); ; Fine sandy clay loam; Massive grade of structure; Rigid 
	consistence; 2-10%, Sandstone, coarse fragments; Many (20 - 50 %), Ferruginous, Coarse (6 - 
	20 mm), Nodules; Gradual change to - 
	3.3 - 3.6 m	Red (2.5YR5/8-Moist); ; Fine sandy clay loam; Massive grade of structure; Rigid consistence; 0-
	2%, medium gravelly, 6-20mm, subrounded, Quartz, coarse fragments; Many (20 - 50 %), 
	Ferruginous, Coarse (6 - 20 mm), Nodules; Gradual change to - 
	3.6 - 3.75 m	Red (2.5YR5/8-Moist); ; Fine sandy clay loam; Massive grade of structure; Rigid consistence; 0-
	2%, medium gravelly, 6-20mm, subrounded, Quartz, coarse fragments; Many (20 - 50 %), 
	Ferruginous, Coarse (6 - 20 mm), Nodules; Abrupt change to - 
	3.75 - 3.8 m	; 
	Morphological Notes
	Purplish consolidated sandstone:
	Observation Notes
	150-270CM PSEUDONODULES HARDENED:                                      4YARROWMERE                                      
	Site Notes
	YARROWMERE

	Project Name:	Regional
	Project Code:	REG	Site ID:	T148	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.4A	 0.014A	 0.85B	 0.33	 0.06	 0.15	 1.7F	 3.1F
	0.1 - 0.2	6.4A	 0.014A	 0.75B	 0.27	 0.05	 0.15	 1.3F	 2.5F
	0.2 - 0.3	6.3A	 0.014A	 0.85B	 0.36	 0.03	 0.15	 1F	 2.4F
	0.3 - 0.4	6.5A	 0.014A	 0.57B	 0.39	 0.02	 0.15	 0.8F	 1.9F
	0.4 - 0.5	6.5A	 0.011A	 0.75B	 0.53	 0.01	 0.16	 1.2F	 2.7F
	0.5 - 0.6	6.5A	 0.011A
	0.6 - 0.75	6.6A	 0.014A
	0.75 - 0.9	6.6A	 0.017A	 1.1B	 1.1	 0.02	 0.16	 1.1F	 3.5F
	0.9 - 1.05	6.6A	 0.011A
	1.05 - 1.2	6.5A	 0.011A
	1.2 - 1.5	6.7A	 0.011A
	1.5 - 1.8	6.5A	 0.014A	 0.75B	 1.6	 0.04	 0.18	 1.2F	 3.8F
	1.8 - 2.1	6.6A	 0.014A
	2.1 - 2.4	6.7A	 0.014A	 0.5B	 1.7	 0.03	 0.19	 1F	 3.4F
	2.4 - 2.7	6.8A	 0.014A
	2.7 - 3	6.8A	 0.014A
	3 - 3.3	7A	 0.011A	 0.3B	 1.4	 0.02	 0.2	 0.9F	 2.8F
	3.3 - 3.6	7.4A	 0.011A
	3.6 - 3.75	7.5A	 0.014A	 0.2B	 0.8	 0.02	 0.2	 1F	 2.2F
	3.75 - 3.8	7.6A	 0.014A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.44D	 5.6B	 0.006A	 0.03A	 0.05A	<2	 49A	 40	 4	 7
	0.1 - 0.2	 0.23D	 0.006A	 0.02A	 0.04A	<2	 50A	 38	 3	 8
	0.2 - 0.3	 0.27D	 0.006A	 0.05A	<2	 47A	 40	 3	 10
	0.3 - 0.4	<2	 47A	 40	 3	 10
	0.4 - 0.5	<2	 50A	 35	 3	 12
	0.5 - 0.6
	0.6 - 0.75
	0.75 - 0.9	 0.005A	 0.07A	<2	 42A	 30	 3	 25
	0.9 - 1.05
	1.05 - 1.2
	1.2 - 1.5
	1.5 - 1.8	 0.006A	 0.08A	 2	 36A	 28	 3	 23
	1.8 - 2.1
	2.1 - 2.4	 2	 39A	 24	 3	 35
	2.4 - 2.7
	2.7 - 3
	3 - 3.3	 28	 42A	 33	 3	 22
	3.3 - 3.6
	3.6 - 3.75	 28	 57A	 27	 2	 14
	3.75 - 3.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1

	Project Name:	Regional
	Project Code:	REG	Site ID:	T148	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.75
	0.75 - 0.9
	0.9 - 1.05
	1.05 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2.1
	2.1 - 2.4
	2.4 - 2.7
	2.7 - 3
	3 - 3.3
	3.3 - 3.6
	3.6 - 3.75
	3.75 - 3.8

	Project Name:	Regional
	Project Code:	REG	Site ID:	T148	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_FE	Total element - Fe(%) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	MIN_EC	Exchange Capacity - Minerology
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_K2O	K2O - X-Ray Diffraction or Clay Fraction (air dry)
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction