Project Name:	Regional
	Project Code:	REG	Site ID:	T152	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G. Smith	Locality:	East of Yarrowmere on road to Mirtna and 
	highway:16KM west of west endof mirtna airstrip:
	Date Desc.:	12/09/70	Elevation:	No Data
	Map Ref.:	Sheet No. : 8155   1:100000	Rainfall:	560
	Northing/Long.:	146.108333333333	Runoff:	Moderately rapid
	Easting/Lat.:	-21.3833333333333	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qs	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	0 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Mesotrophic Brown Kandosol     	Principal Profile Form:	Gn2.21
	ASC Confidence:	Great Soil Group:	Yellow earth
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:
	Mid Strata - Tree, 1.01-3m, Very sparse. *Species includes - Melaleuca species, Grevillea species
	Tall Strata - Tree, 3.01-6m, Very sparse. *Species includes - Eucalyptus melanophloia, Eucalyptus polycarpa, 
	Eucalyptus papuana
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.05 m	Very dark greyish brown (10YR3/2-Moist); Greyish brown (10YR5/2-Dry); ; Loamy sand; Massive 
	grade of structure; Dry; Strong consistence; Many, fine (1-2mm) roots; Gradual change to - 
	A12	0.05 - 0.1 m	Dark brown (10YR3/3-Moist); Brown (10YR5/3-Dry); ; Loamy sand; Massive grade of structure; 
	Dry; Strong consistence; Many, fine (1-2mm) roots; Gradual change to - 
	A3	0.1 - 0.15 m	Brown (10YR4/3-Moist); Pale brown (10YR6/3-Dry); ; Loamy sand; Massive grade of structure; 
	Dry; Strong consistence; Few, medium (2-5mm) roots; Gradual change to - 
	A3	0.15 - 0.2 m	Dark yellowish brown (10YR4/4-Moist); Pale brown (10YR6/3-Dry); ; Loamy sand; Massive grade 
	of structure; Dry; Few, fine (1-2mm) roots; Gradual change to - 
	B1	0.2 - 0.3 m	Yellowish brown (10YR5/5-Moist); Light yellowish brown (10YR6/4-Dry); ; Loamy sand; Massive 
	grade of structure; Dry; Strong consistence; Gradual change to - 
	B1	0.3 - 0.4 m	Yellowish brown (10YR5/6-Moist); ; Loamy sand (Heavy); Massive grade of structure; Earthy 
	fabric; Dry; Very strong consistence; Gradual change to - 
	B1	0.4 - 0.5 m	Yellowish brown (10YR5/6-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; Dry; 
	Very strong consistence; Gradual change to - 
	B1	0.5 - 0.6 m	Yellowish brown (10YR5/6-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; Dry; 
	Rigid consistence; Gradual change to - 
	B21	0.6 - 0.7 m	Yellowish brown (10YR5/6-Moist); ; Sandy clay loam (Light); Massive grade of structure; Earthy 
	fabric; Dry; Strong consistence; Gradual change to - 
	B21	0.7 - 0.8 m	Yellowish brown (10YR5/6-Moist); , 7.5YR78, 0-2% , Distinct; , 0-2% , Distinct; Sandy clay loam 
	(Heavy); Massive grade of structure; Earthy fabric; Dry; Strong consistence; Gradual change to - 
	B22	0.8 - 0.9 m	Yellowish brown (10YR5/7-Moist); , 7.5YR78, 2-10% , 0-5mm, Distinct; , 2-10% , 0-5mm, 
	Distinct; Sandy medium clay; Massive grade of structure; Dry; Very strong consistence; Gradual 
	change to - 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T152	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B22	0.9 - 1 m	Yellowish brown (10YR5/6-Moist); , 7.5YR78, 2-10% , 15-30mm, Distinct; , 2-10% , 15-30mm, 
	Distinct; Sandy medium clay; Massive grade of structure; Earthy fabric; Dry; Rigid consistence; 
	Gradual change to - 
	B22	1 - 1.1 m	Yellowish brown (10YR5/6-Moist); , 7.5YR78, 2-10% , 15-30mm, Distinct; , 2-10% , 15-30mm, 
	Distinct; Sandy medium clay; Massive grade of structure; Earthy fabric; Dry; Very strong 
	consistence; Gradual change to - 
	1.1 - 1.2 m	Yellowish brown (10YR5/6-Moist); , 7.5YR78, 10-20% , 15-30mm, Distinct; , 10-20% , 15-30mm, 
	Distinct; Sandy medium clay; Massive grade of structure; Earthy fabric; Rigid consistence; 
	Gradual change to - 
	1.2 - 1.3 m	Yellowish brown (10YR5/6-Moist); , 7.5YR78, 10-20% , 15-30mm, Distinct; , 10-20% , 15-30mm, 
	Distinct; Sandy medium clay; Massive grade of structure; Rigid consistence; Gradual change to
	1.3 - 1.4 m	Brownish yellow (10YR6/5-Moist); ; Sandy medium clay (Light); Massive grade of structure; Very 
	strong consistence; Common (10 - 20 %), Ferromanganiferous, Coarse (6 - 20 mm), Nodules; 
	Gradual change to - 
	1.4 - 1.5 m	Light yellowish brown (10YR6/4-Moist); ; Sandy medium clay (Light); Massive grade of structure; 
	Very strong consistence; Many (20 - 50 %), Ferromanganiferous, Coarse (6 - 20 mm), Nodules; 
	Gradual change to - 
	1.5 - 1.8 m	Light yellowish brown (10YR6/4-Moist); ; Sandy clay loam (Light); Massive grade of structure; 
	Very strong consistence; Many (20 - 50 %), Ferromanganiferous, Very coarse (20 - 60 mm), 
	Nodules; Gradual change to - 
	1.8 - 2 m	Yellow (10YR7/5-Moist); ; Sandy clay loam (Light); Massive grade of structure; Very strong 
	consistence; Many (20 - 50 %), Ferromanganiferous, Coarse (6 - 20 mm), Nodules; 
	Morphological Notes
	Observation Notes
	0-90CM GRADUAL YELLOW MATRIX INCREASE:90-200CM GRADUAL YELLOW MATRIX DECREASE:                                    
	      
	Site Notes
	YARROWMERE

	Project Name:	Regional
	Project Code:	REG	Site ID:	T152	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.7A	 0.038A	 2.4B	 0.61	 0.19	 0.17	 0.8F	 4.2F
	0.05 - 0.1	6.9A	 0.029A	 1.7B	 0.48	 0.16	 0.17	 0.6F	 3.1F
	0.1 - 0.15	7A	 0.02A	 1.3B	 0.45	 0.12	 0.18
	0.15 - 0.2	7A	 0.017A	 0.86B	 0.38	 0.11	 0.17
	0.2 - 0.3	6.6A	 0.017A	 0.96B	 0.29	 0.1	 0.18	 0.5F	 2F
	0.3 - 0.4	7A	 0.017A
	0.4 - 0.5	7A	 0.017A	 0.76B	 0.26	 0.11	 0.17	 0.5F	 1.8F
	0.5 - 0.6	7.1A	 0.017A
	0.6 - 0.7	6.9A	 0.02A
	0.7 - 0.8	6.8A	 0.023A	 1.1B	 0.48	 0.15	 0.18	 0.5F	 2.4F
	0.8 - 0.9	6.8A	 0.02A
	0.9 - 1	6.4A	 0.026A
	1 - 1.1	6.4A	 0.023A	 0.96B	 0.8	 0.11	 0.17	 0.13F	 2.07A	 2.2F	8.21
	1.1 - 1.2	6.5A	 0.023A
	1.2 - 1.3	6.4A	 0.029A	 0.96B	 1.1	 0.09	 0.26
	1.3 - 1.4	6.4A	 0.026A
	1.4 - 1.5	6.5A	 0.026A
	1.5 - 1.8	6.4A	 0.041A
	1.8 - 2	6.8A	 0.026A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0.5D	 4.2B	 0.007A	 0.03A	 0.07A	 0	 53A	 36	 6	 5
	0.05 - 0.1	 0.4D	 3.1B	 0.005A	 0.02A	 0.07A	 0	 49A	 39	 6	 5
	0.1 - 0.15	 0.24D	 0.005A	 0.07A	 0	 55A	 22	 6	 7
	0.15 - 0.2	 0.16D	 0.004A	 0.07A	<2	 55A	 32	 6	 7
	0.2 - 0.3	 0.14D	 0.004A	 0.07A	<2	 52A	 35	 6	 7
	0.3 - 0.4
	0.4 - 0.5	 0.005A	 0.07A	<2	 49A	 37	 6	 8
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8	 0.006A	 0.1A	<2	 49A	 30	 5	 16
	0.8 - 0.9
	0.9 - 1
	1 - 1.1	 2	 40A	 31	 6	 23
	1.1 - 1.2
	1.2 - 1.3
	1.3 - 1.4
	1.4 - 1.5
	1.5 - 1.8
	1.8 - 2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.15

	Project Name:	Regional
	Project Code:	REG	Site ID:	T152	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	0.15 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1
	1 - 1.1
	1.1 - 1.2
	1.2 - 1.3
	1.3 - 1.4
	1.4 - 1.5
	1.5 - 1.8
	1.8 - 2

	Project Name:	Regional
	Project Code:	REG	Site ID:	T152	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_FE	Total element - Fe(%) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	MIN_EC	Exchange Capacity - Minerology
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)
	XRD_C_Hm	Hematite - X-Ray Diffraction
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_K2O	K2O - X-Ray Diffraction or Clay Fraction (air dry)
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction