Project Name:	Regional
	Project Code:	REG	Site ID:	T155	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G. Smith	Locality:	21.8KM east of Dunbar turn on Galbraith-Dunbar 
	Road:
	Date Desc.:	01/10/70	Elevation:	No Data
	Map Ref.:	Sheet No. : 7265   1:100000	Rainfall:	1020
	Northing/Long.:	141.777777777778	Runoff:	Very slow
	Easting/Lat.:	-16.4361111111111	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Czy	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	Simple-slope	Relief:	3 metres
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Surface crust
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Ferric Mesotrophic Grey Kandosol     	Principal Profile Form:	Gn2.74
	ASC Confidence:	Great Soil Group:	Yellow earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Mid Strata - Tree, 1.01-3m, Very sparse. *Species includes - None recorded
	Tall Strata - Tree, 3.01-6m, Very sparse. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.05 m	Dark greyish brown (10YR4/2-Moist); Light brownish grey (10YR6/2-Dry); , 10YR76, 2-10% , 0-
	5mm, Faint; , 2-10% , 0-5mm, Faint; Silty clay loam (Light); Massive grade of structure; Dry; 
	Rigid consistence; Clear change to - 
	AB	0.05 - 0.1 m	Brownish yellow (10YR6/5-Moist); Very pale brown (10YR7/4-Dry); , 5YR58, 10-20% , 0-5mm, 
	Distinct; , 10-20% , 0-5mm, Distinct; Silty medium clay; Massive grade of structure; Dry; Strong 
	consistence; Gradual change to - 
	B1	0.1 - 0.2 m	Brownish yellow (10YR6/5-Moist); , 10YR54, 10-20% , 0-5mm, Distinct; , 7.5YR56, 10-20% , 0-
	5mm, Distinct; Silty medium clay; Massive grade of structure; Dry; Strong consistence; Few (2 - 
	10 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Gradual change to - 
	0.2 - 0.3 m	Brownish yellow (10YR6/5-Moist); , 10YR76, 10-20% , 5-15mm, Faint; , 10-20% , 5-15mm, Faint; 
	Silty medium clay (Heavy); Massive grade of structure; Strong consistence; Many (20 - 50 %), 
	Ferruginous, Coarse (6 - 20 mm), Nodules; Gradual change to - 
	0.3 - 0.4 m	Pale red (2.5YR6/2-Moist); , 10YR76, 20-50% , 0-5mm, Distinct; , 20-50% , 0-5mm, Distinct; 
	Light clay; Massive grade of structure; Strong consistence; Many (20 - 50 %), Ferruginous, 
	Coarse (6 - 20 mm), Nodules; Gradual change to - 
	0.4 - 0.5 m	Pale red (2.5YR6/2-Moist); , 10YR76, 20-50% , 0-5mm, Distinct; , 20-50% , 0-5mm, Distinct; 
	Light clay; Massive grade of structure; Strong consistence; Many (20 - 50 %), Ferruginous, 
	Coarse (6 - 20 mm), Nodules; Gradual change to - 
	0.5 - 0.6 m	Pale red (2.5YR6/2-Moist); , 5YR78, 20-50% , 0-5mm, Distinct; , 20-50% , 0-5mm, Distinct; Light
	 clay (Heavy); Massive grade of structure; Strong consistence; Few (2 - 10 %), , , Nodules; 
	Gradual change to - 
	0.6 - 0.7 m	Pale red (2.5YR6/2-Moist); , 10YR65, 20-50% , 0-5mm, Distinct; , 10YR58, 20-50% , 0-5mm, 
	Distinct; Light medium clay; Weak grade of structure, Angular blocky; Strong consistence; 
	Common (10 - 20 %), , , Nodules; Gradual change to - 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T155	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	C	0.7 - 0.8 m	Pale red (2.5YR6/2-Moist); , 10YR66, 20-50% , 0-5mm, Distinct; , 10YR58, 20-50% , 0-5mm, 
	Distinct; Light medium clay; Moderate grade of structure, 10-20 mm, Angular blocky; Dry; Very 
	strong consistence; Few (2 - 10 %), Manganiferous, , Nodules; Gradual change to - 
	0.8 - 0.9 m	Grey (10YR6/1-Moist); , 10YR58, 20-50% , 15-30mm, Prominent; , 20-50% , 15-30mm, 
	Prominent; Medium heavy clay; Strong grade of structure, 20-50 mm, Angular blocky; Gradual 
	change to - 
	0.9 - 1 m	Grey (10YR6/1-Moist); Yellowish brown (10YR5/8-Dry); , 10YR58, 20-50% , 15-30mm, Prominent;
	 , 10YR58, 20-50% , 15-30mm, Prominent; Medium heavy clay; Strong grade of structure, 20-50 
	mm, Angular blocky; 
	Morphological Notes
	Observation Notes
	HORIZON 6A CONTINUES TO 130CM:>130CM 10YR 55(M) MODERATE COARSE BLOCKY HC:                                              
	Site Notes
	GALBRAITH

	Project Name:	Regional
	Project Code:	REG	Site ID:	T155	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.1A	 0.032A
	0.05 - 0.1	6.1A	 0.029A
	0.1 - 0.2	6.1A	 0.026A
	0.2 - 0.3	6.2A	 0.026A
	0.3 - 0.4	6.3A	 0.026A
	0.4 - 0.5	6.4A	 0.026A
	0.5 - 0.6	6.5A	 0.026A
	0.6 - 0.7	6.7A	 0.029A
	0.7 - 0.8	6.4A	 0.053A
	0.8 - 0.9	6.3A	 0.098A
	0.9 - 1	6.3A	 0.16A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1

	Project Name:	Regional
	Project Code:	REG	Site ID:	T155	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension