Project Name:	Regional
	Project Code:	REG	Site ID:	T165	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.F. Isbell	Locality:	.5KM along Boomerang Road from turnoff on Hann 
	Highway:turnoff is 6.5KMeast of Mt. Surprise Road:
	Date Desc.:	13/10/70	Elevation:	No Data
	Map Ref.:	Sheet No. : 7861   1:100000	Rainfall:	0
	Northing/Long.:	144.808333333333	Runoff:	Very slow
	Easting/Lat.:	-18.1958333333333	Drainage:	Moderately well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Czm	Substrate Material:	Undisturbed soil core, 5 m deep,Basalt 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	0 metres
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Ferrosol     	Principal Profile Form:	Gn3.12
	ASC Confidence:	Great Soil Group:	Euchrozem
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - None recorded
	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Grevillea pteridifolia
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus dichromophloia, Eucalyptus crebra, Eucalyptus 
	papuana
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.1 m	Dark reddish brown (5YR3/2-Moist); Dark reddish brown (5YR3/2-Dry); ; Clay loam; Weak grade of
	 structure, 5-10 mm, Angular blocky; Dry; Strong consistence; Common, fine (1-2mm) roots; 
	Gradual change to - 
	A12	0.1 - 0.2 m	Dark reddish brown (2.5YR3/3-Moist); Dark reddish brown (2.5YR3/4-Dry); ; Clay loam (Heavy); 
	Weak grade of structure, 5-10 mm, Angular blocky; Dry; Strong consistence; Few (2 - 10 %), 
	Argillaceous, Fine (0 - 2 mm), Nodules; Few, fine (1-2mm) roots; Gradual change to - 
	B1	0.2 - 0.3 m	Dark reddish brown (2.5YR3/4-Moist); Dark red (2.5YR3/5-Dry); ; Light clay; Weak grade of 
	structure, 5-10 mm, Angular blocky; Dry; Strong consistence; Few (2 - 10 %), Ferruginous, Fine 
	(0 - 2 mm), Nodules; 
	B1	0.3 - 0.6 m	Dark reddish brown (2.5YR3/4-Moist); Dark red (2.5YR3/5-Dry); ; Light clay; Weak grade of 
	structure, 5-10 mm, Angular blocky; Dry; Strong consistence; Few (2 - 10 %), Ferruginous, Fine 
	(0 - 2 mm), Nodules; Gradual change to - 
	B1	0.6 - 0.9 m	Dark red (2.5YR3/6-Moist); ; Light clay; Weak grade of structure, 5-10 mm, Angular blocky; Dry; 
	Strong consistence; Few (2 - 10 %), Ferruginous, Fine (0 - 2 mm), Nodules; Gradual change to - 
	B21	0.9 - 1.2 m	Dark red (2.5YR3/6-Moist); ; Light medium clay; Weak grade of structure, 5-10 mm, Angular 
	blocky; Smooth-ped fabric; Dry; Strong consistence; Few (2 - 10 %), Ferruginous, Fine (0 - 2 
	mm), Nodules; Gradual change to - 
	B21	1.2 - 1.5 m	Dark red (2.5YR3/6-Moist); ; Light medium clay; Moderate grade of structure, 2-5 mm, Angular 
	blocky; Smooth-ped fabric; Moderately moist; Very firm consistence; Few (2 - 10 %), 
	Ferruginous, Fine (0 - 2 mm), Nodules; Gradual change to - 
	B22	1.5 - 1.8 m	Dark red (2.5YR3/6-Moist); ; Medium clay; Moderate grade of structure, 2-5 mm, Angular blocky; 
	Smooth-ped fabric; Moderately moist; Very firm consistence; Few (2 - 10 %), Ferruginous, Fine 
	(0 - 2 mm), Nodules; Gradual change to - 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T165	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B22	1.8 - 2.1 m	Dark red (2.5YR3/6-Moist); ; Medium clay; Moderate grade of structure, 2-5 mm, Angular blocky; 
	Smooth-ped fabric; Moderately moist; Very firm consistence; Few (2 - 10 %), Ferruginous, Fine 
	(0 - 2 mm), Nodules; Gradual change to - 
	2.1 - 2.6 m	Dark red (2.5YR3/6-Moist); ; Medium heavy clay; Strong grade of structure, 2-5 mm, Angular 
	blocky; Smooth-ped fabric; Very firm consistence; Common (10 - 20 %), Argillaceous, , 
	Tubules; Gradual change to - 
	2.6 - 3.1 m	Dark red (2.5YR3/6-Moist); ; Medium heavy clay; Strong grade of structure, 2-5 mm, Angular 
	blocky; Smooth-ped fabric; Very firm consistence; Common (10 - 20 %), Argillaceous, , 
	Tubules; Gradual change to - 
	3.1 - 3.6 m	Yellowish red (5YR3/6-Moist); ; Medium heavy clay; Strong grade of structure, 2-5 mm, Angular 
	blocky; Smooth-ped fabric; Very firm consistence; Common (10 - 20 %), Argillaceous, , 
	3.6 - 4.1 m	Yellowish red (5YR3/6-Moist); ; Medium heavy clay; Strong grade of structure, 2-5 mm, Angular 
	blocky; Smooth-ped fabric; Very firm consistence; Common (10 - 20 %), Argillaceous, , 
	4.1 - 4.6 m	Yellowish red (5YR3/6-Moist); ; Medium heavy clay; Strong grade of structure, 2-5 mm, Angular 
	blocky; Smooth-ped fabric; Very firm consistence; Common (10 - 20 %), Argillaceous, , 
	4.6 - 4.8 m	Yellowish red (5YR3/6-Moist); ; Medium heavy clay; Strong grade of structure, 2-5 mm, Angular 
	blocky; Smooth-ped fabric; Very firm consistence; Common (10 - 20 %), Argillaceous, , 
	4.8 - 5 m	; 
	5 - 5.2 m	; 
	Morphological Notes
	Soft weathered basalt with small veins of red clay:
	Observation Notes
	480-500CM SOFT WEATHERED BASALT WITH AREAS OF RED MC:<10% BASALT FLOATERS IN PROFILE:120-121CM 
	STAINING ON PED FACES:   
	Site Notes
	BOOMERANG

	Project Name:	Regional
	Project Code:	REG	Site ID:	T165	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.1A	 0.065A	 16.2B	 4.66	 1.6	 0.05
	0.1 - 0.2	6A	 0.047A	 12.6B	 3.01	 1.23	 0.05
	0.2 - 0.3	6A	 0.035A	 10.3B	 2.59	 1.09	 0.04
	0.3 - 0.6	6.1A	 0.029A	 9.15B	 2.47	 1.1	 0.05
	0.6 - 0.9	6.4A	 0.02A
	0.9 - 1.2	6.4A	 0.023A
	1.2 - 1.5	6.6A	 0.02A
	1.5 - 1.8	6.6A	 0.023A
	1.8 - 2.1	6.7A	 0.02A
	2.1 - 2.6	6.7A	 0.02A	 6.28B	 5.17	 0.85	 0.07
	2.6 - 3.1	6.6A	 0.017A
	3.1 - 3.6	6.4A	 0.017A
	3.6 - 4.1	6.2A	 0.017A
	4.1 - 4.6	6.2A	 0.017A
	4.6 - 4.8	6.1A	 0.017A
	4.8 - 5	5.9A	 0.017A
	5 - 5.2	5.8A	 0.02A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 2.97D	 379B	 0.42A	 0.211A	 0.31A
	0.1 - 0.2	 1.51D	 312B	 0.4A	 0.153A	 0.3A
	0.2 - 0.3	 0.87D	 328B	 0.089A
	0.3 - 0.6	 0.67D	 128B	 0.28A	 0.064A	 0.25A
	0.6 - 0.9
	0.9 - 1.2	 0.18D	 57B	 0.036A
	1.2 - 1.5
	1.5 - 1.8	 0.15D	 39B	 0.027A
	1.8 - 2.1
	2.1 - 2.6	 58B	 0.27A	 0.19A
	2.6 - 3.1
	3.1 - 3.6
	3.6 - 4.1
	4.1 - 4.6
	4.6 - 4.8
	4.8 - 5	 0.29A	 0.18A
	5 - 5.2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.5

	Project Name:	Regional
	Project Code:	REG	Site ID:	T165	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	1.5 - 1.8
	1.8 - 2.1
	2.1 - 2.6
	2.6 - 3.1
	3.1 - 3.6
	3.6 - 4.1
	4.1 - 4.6
	4.6 - 4.8
	4.8 - 5
	5 - 5.2

	Project Name:	Regional
	Project Code:	REG	Site ID:	T165	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_FE	Total element - Fe(%) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)