Project Name:	Regional
	Project Code:	REG	Site ID:	T17	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.F. Isbell	Locality:	8KM east of Doongmabulla:5.4KM on Bygana Road 
	from Labona Road turnoff:
	Date Desc.:	06/07/64	Elevation:	 366 metres
	Map Ref.:	Sheet No. : 8153   1:100000	Rainfall:	560
	Northing/Long.:	146.316666666667	Runoff:	Rapid
	Easting/Lat.:	-22.0708333333333	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Rld	Substrate Material:	Sandstone 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	No Data	Relief:	15 metres
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Ferric Orthic Tenosol     	Principal Profile Form:	Gn2.22
	ASC Confidence:	Great Soil Group:	Yellow earth
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Plectrachne pungens
	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Acacia species
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus setosa, Melaleuca species
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.13 m	Yellowish brown (10YR5/4-Moist); ; Sand; Massive grade of structure; Weak consistence; 
	B11	0.13 - 0.38 m	Strong brown (7.5YR5/7-Moist); ; Loamy sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; Weak consistence; Few (2 - 10 %), Ferruginous, Medium (2 -6 mm), Nodules; 
	Gradual change to - 
	B12	0.38 - 0.61 m	Strong brown (7.5YR5/7-Moist); ; Loamy sand; Massive grade of structure; Weak consistence; 
	Very many (50 - 100 %), Ferruginous, Very coarse (20 - 60 mm), Nodules; Clear change to - 
	B21	0.61 - 0.86 m	Strong brown (7.5YR5/7-Moist); ; Sandy loam (Light); Massive grade of structure; Weak 
	consistence; Very many (50 - 100 %), Ferruginous, Very coarse (20 - 60 mm), Nodules; Gradual 
	change to - 
	B22	0.86 - 1.02 m	Brownish yellow (10YR6/6-Moist); ; Sandy loam (Heavy); Massive grade of structure; Weak 
	consistence; 2-10%, medium gravelly, 6-20mm, Sandstone, coarse fragments; Common (10 - 
	20 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 6.5 (pH meter); Gradual change to - 
	C	1.02 - 1.12 m	; 
	Morphological Notes
	C	Hard altered sandstone
	Observation Notes
	Site Notes
	DOONGMABULLA

	Project Name:	Regional
	Project Code:	REG	Site ID:	T17	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	5A	<0.03A	 0.6B	 0.14	 0.08	 0.2	 3C	6.67
	0.13 - 0.38	5A	<0.03A	 0.4B	 0.06	 0.05	 0.2	 1C	20.00
	0.38 - 0.61	5.4A	<0.03A
	0.61 - 0.86	5.7A	 0.029A	 0.4B	 0.2	 0.07	 0.3	 1C	30.00
	0.86 - 1.02	6.2A	 0.06A	 0.2B	 1.6	 0.04	 0.3
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13	 0.35D	 4B	 0.006A	 0.02A	 1	 43D	 47	 6	 5
	0.13 - 0.38	 0.1D	 3B
	0.38 - 0.61	 4B
	0.61 - 0.86	 4B
	0.86 - 1.02	 2B	 0.004A	 19	 45D	 40	 4	 11
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13
	0.13 - 0.38
	0.38 - 0.61
	0.61 - 0.86
	0.86 - 1.02

	Project Name:	Regional
	Project Code:	REG	Site ID:	T17	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance