Project Name:	Regional
	Project Code:	REG	Site ID:	T172	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.G. Murtha	Locality:	8.8KM north of Black Braes turnoff on Hann Highway:
	Date Desc.:	15/05/71	Elevation:	 831 metres
	Map Ref.:	Sheet No. : 7759   1:100000	Rainfall:	690
	Northing/Long.:	144.258333333333	Runoff:	Rapid
	Easting/Lat.:	-19.4833333333333	Drainage:	Well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Czc	Substrate Material:	Undisturbed soil core, 0.7 m deep,Basalt 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	No Data
	Morph. Type:	Flat	Relief:	0 metres
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Eutrophic Brown Ferrosol     	Principal Profile Form:	Gn3.2
	ASC Confidence:	Great Soil Group:	No suitable group
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	0-2%, , subrounded, Basalt
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (7.5YR3/2-Moist); ; Loam (Heavy); Weak grade of structure, 2-5 mm, Angular blocky; 
	Dry; Firm consistence; Very few (0 - 2 %), Ferromanganiferous, Fine (0 - 2 mm), Nodules; 
	Gradual change to - 
	B1	0.1 - 0.2 m	Brown (7.5YR4/4-Moist); ; Clay loam (Heavy); Weak grade of structure, 5-10 mm, Angular blocky; 
	Moist; Weak consistence; Gradual change to - 
	B1	0.2 - 0.3 m	Dark yellowish brown (10YR4/4-Moist); ; Light medium clay; Moderate grade of structure, 2-5 
	mm, Angular blocky; Moist; Weak consistence; Few (2 - 10 %), Manganiferous, Coarse (6 - 20 
	mm), Concretions; Gradual change to - 
	B2	0.3 - 0.45 m	Dark yellowish brown (10YR4/6-Moist); ; Medium clay; Moderate grade of structure, 5-10 mm, 
	Angular blocky; Moist; Weak consistence; Many (20 - 50 %), Ferromanganiferous, Coarse (6 - 20 
	mm), Nodules; 
	B2	0.45 - 0.6 m	Dark yellowish brown (10YR4/6-Moist); ; Medium clay; Moderate grade of structure, 5-10 mm, 
	Angular blocky; Moist; Weak consistence; Many (20 - 50 %), Ferromanganiferous, Coarse (6 - 20 
	mm), Nodules; 
	BC	0.6 - 0.75 m	Yellowish brown (10YR5/4-Moist); , 10YR58, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, 
	Distinct; Light medium clay; 
	Morphological Notes
	BC	On hard basalt:
	Observation Notes
	60-72CM MUCH SOFT WEATHERED BASALT:SOME BASALT FLOATERS ON SURFACE AND THROUGH PROFILE:              
	                   
	Site Notes
	LYNDHURST

	Project Name:	Regional
	Project Code:	REG	Site ID:	T172	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.7A	 0.041A	 9.2B	 8.7	 0.89	 0.06
	0.1 - 0.2	6.5A	 0.038A	 7.4B	 7.9	 0.46	 0.11
	0.2 - 0.3	6.4A	 0.038A	 7.3B	 9	 0.3	 0.17
	0.3 - 0.45	6.4A	 0.032A	 7.3B	 10.7	 0.28	 0.4
	0.45 - 0.6	6.9A	 0.044A
	0.6 - 0.72	 0.044A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.66D	 21B	 0.11A	 0	 15A	 21	 31	 34
	0.1 - 0.2	 0.74D	 5B	 0.07A	 0	 9A	 19	 25	 42
	0.2 - 0.3	 0.6D	 4B	 0.06A	 0	 16A	 15	 17	 52
	0.3 - 0.45	 0.49D	 4B	 0.05A	 0	 13A	 14	 19	 59
	0.45 - 0.6	 0.41D	 0	 8A	 12	 18	 65
	0.6 - 0.72	 0	 29A	 39	 18	 14
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.45
	0.45 - 0.6
	0.6 - 0.72

	Project Name:	Regional
	Project Code:	REG	Site ID:	T172	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_FE	Total element - Fe(%) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)