Project Name:	Regional
	Project Code:	REG	Site ID:	T173	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.G. Murtha	Locality:	On Hann Highway 14.9KM north of Conjuboy 4.2KM 
	south of Reedy Brook turnoff:
	Date Desc.:	16/05/71	Elevation:	 640 metres
	Map Ref.:	Sheet No. : 7860   1:100000	Rainfall:	710
	Northing/Long.:	144.7375	Runoff:	Rapid
	Easting/Lat.:	-18.5708333333333	Drainage:	Well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Czm	Substrate Material:	Undisturbed soil core, 1.1 m deep,Porous, 
	Basalt 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	0 metres
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melanic Eutrophic Brown Ferrosol     	Principal Profile Form:	Gn3.2
	ASC Confidence:	Great Soil Group:	No suitable group
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus crebra, Eucalyptus leptophleba, Eucalyptus 
	papuana
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Very dark brown (7.5YR2/2-Moist); ; Loam (Heavy); Moderate grade of structure, 2-5 mm, Angular 
	blocky; Moderately moist; Weak consistence; Very few (0 - 2 %), Ferromanganiferous, Fine (0 - 2 
	mm), Nodules; Many, fine (1-2mm) roots; Gradual change to - 
	B1	0.1 - 0.2 m	Very dark brown (7.5YR2/2-Moist); ; Clay loam (Heavy); Moderate grade of structure, 2-5 mm, 
	Angular blocky; Moist; Weak consistence; Few (2 - 10 %), Ferromanganiferous, Medium (2 -6 
	mm), Nodules; Gradual change to - 
	B1	0.2 - 0.3 m	Brown (7.5YR4/4-Moist); ; Light clay; Strong grade of structure, 2-5 mm, Angular blocky; Moist; 
	Weak consistence; , Manganiferous, , ; Gradual change to - 
	B21	0.3 - 0.45 m	Brown (7.5YR4/4-Moist); ; Medium clay; Strong grade of structure, 2-5 mm, Angular blocky; 
	Moist; Firm consistence; Few (2 - 10 %), Manganiferous, , Concretions; 
	B21	0.45 - 0.6 m	Brown (7.5YR4/4-Moist); , 7.5YR52, 10-20% , 5-15mm, Faint; , 10-20% , 5-15mm, Faint; Medium 
	clay; Strong grade of structure, 2-5 mm, Angular blocky; Moist; Firm consistence; 2-10%, Basalt,
	 coarse fragments; Few (2 - 10 %), Manganiferous, , Concretions; 
	B22	0.6 - 0.9 m	Reddish brown (5YR4/4-Moist); , 10YR54, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, 
	Distinct; Medium clay; Strong grade of structure, 2-5 mm, Angular blocky; Smooth-ped fabric; 
	Moist; Firm consistence; Many (20 - 50 %), Manganiferous, , Concretions; 
	B22	0.9 - 1.07 m	Reddish brown (5YR4/4-Moist); , 10YR54, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, 
	Distinct; Medium clay; Strong grade of structure, 2-5 mm, Angular blocky; Smooth-ped fabric; 
	Firm consistence; Many (20 - 50 %), , , Concretions; 
	Morphological Notes
	B22	On hard basalt probably a floater:
	Observation Notes
	Site Notes
	CONJUBOY

	Project Name:	Regional
	Project Code:	REG	Site ID:	T173	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)

	Project Name:	Regional
	Project Code:	REG	Site ID:	T173	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.7A	 0.059A	 15.8B	 7.4	 1.4	 0.06
	0.1 - 0.2	6.9A	 0.05A	 12.6B	 7.4	 1.2	 0.08
	0.2 - 0.3	6.7A	 0.044A	 13.7B	 9.1	 1.3	 0.12
	0.3 - 0.45	6.8A	 0.041A	 9.7B	 7.4	 1	 0.09
	0.45 - 0.6	6.9A	 0.044A
	0.6 - 0.9	6.8A	 0.053A	 7.9B	 8	 0.75	 0.17
	0.9 - 1.07	7.1A	 0.032A	 8.9B	 9.3	 0.91	 0.44
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 2.01D	 184B	 0.14A	 0	 15A	 20	 29	 38
	0.1 - 0.2	 0.85D	 70B	 0.08A	 0	 13A	 14	 23	 55
	0.2 - 0.3	 0.67D	 23B	 0.05A	 0	 5A	 9	 16	 75
	0.3 - 0.45	 0.42D	 17B	 0.04A	 0	 7A	 10	 19	 73
	0.45 - 0.6	 0.34D
	0.6 - 0.9	 36B	 10	 8A	 9	 15	 75
	0.9 - 1.07	 34B	 0	 8A	 17	 19	 62
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.45
	0.45 - 0.6
	0.6 - 0.9
	0.9 - 1.07

	Project Name:	Regional
	Project Code:	REG	Site ID:	T173	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_FE	Total element - Fe(%) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)