Project Name:	Regional
	Project Code:	REG	Site ID:	T176	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G. Smith	Locality:	25.9KM north of Laura Post Office on Kennedy 
	Highway:
	Date Desc.:	03/11/70	Elevation:	No Data
	Map Ref.:	Sheet No. : 7767   1:100000	Rainfall:	940
	Northing/Long.:	144.233333333333	Runoff:	Very slow
	Easting/Lat.:	-15.4638888888889	Drainage:	Well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Tf	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Simple-slope	Relief:	30 metres
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Regolithic Orthic Tenosol     	Principal Profile Form:	Gn2.64
	ASC Confidence:	Great Soil Group:	Yellow earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus species, Eucalyptus polycarpa, Grevillea species
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.1 m	Very dark greyish brown (10YR3/2-Moist); Grey (10YR5/1-Dry); ; Sand (Heavy); Massive grade of 
	structure; Dry; Strong consistence; Clear change to - 
	A21	0.05 - 0.1 m	Dark greyish brown (10YR4/2-Moist); Greyish brown (10YR5/2-Dry); ; Sand; Massive grade of 
	structure; Dry; Firm consistence; Gradual change to - 
	A22	0.1 - 0.2 m	Brown (10YR4/3-Moist); Pale brown (10YR6/3-Dry); ; Sand; Massive grade of structure; Dry; 
	Strong consistence; Gradual change to - 
	B1	0.2 - 0.3 m	Yellowish brown (10YR5/4-Moist); Pale brown (10YR6/3-Dry); ; Sand; Massive grade of structure;
	 Earthy fabric; Dry; Very strong consistence; Gradual change to - 
	B1	0.3 - 0.4 m	Yellowish brown (10YR5/4-Moist); Light yellowish brown (10YR6/4-Dry); ; Sand; Massive grade 
	of structure; Earthy fabric; Dry; Very strong consistence; Gradual change to - 
	B1	0.4 - 0.5 m	Yellowish brown (10YR5/5-Moist); ; Sand; Massive grade of structure; Earthy fabric; Dry; Very 
	strong consistence; Gradual change to - 
	B1	0.5 - 0.6 m	Yellowish brown (10YR5/6-Moist); ; Sand (Heavy); Massive grade of structure; Earthy fabric; Dry; 
	Very strong consistence; Gradual change to - 
	B1	0.6 - 0.75 m	Yellowish brown (10YR5/6-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; Dry; 
	Strong consistence; Gradual change to - 
	B2	0.75 - 0.9 m	Yellowish brown (10YR5/6-Moist); , 10YR68; Sandy clay loam; Massive grade of structure; 
	Earthy fabric; Dry; Strong consistence; Gradual change to - 
	B2	0.9 - 1.2 m	Strong brown (7.5YR5/6-Moist); , 2.5YR58, 2-10% , 15-30mm, Distinct; , 2-10% , 15-30mm, 
	Distinct; Sandy clay loam (Heavy); Massive grade of structure; Earthy fabric; Dry; Very strong 
	consistence; Gradual change to - 
	B2	1.2 - 1.5 m	Red (2.5YR5/8-Moist); , 10YR56, 20-50% , 5-15mm, Distinct; , 20-50% , 5-15mm, Distinct; 
	Sandy medium clay (Light); Massive grade of structure; Dry; Strong consistence; Gradual 
	change to - 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T176	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B2	1.5 - 1.8 m	Red (2.5YR5/8-Moist); , 10YR66, 20-50% , 5-15mm, Distinct; , 20-50% , 5-15mm, Distinct; 
	Sandy medium clay (Light); Massive grade of structure; Dry; Strong consistence; Gradual 
	change to - 
	1.8 - 2.1 m	Yellowish brown (10YR5/6-Moist); , 10YR66, 20-50% , 5-15mm, Distinct; , 10YR82, 20-50% , 5-
	15mm, Distinct; Sandy medium clay (Light); Massive grade of structure; Strong consistence; 
	Gradual change to - 
	B3	2.1 - 2.4 m	Yellow (10YR7/5-Moist); , 7.5YR56, 20-50% , 5-15mm, Distinct; , 20-50% , 5-15mm, Distinct; 
	Sandy medium clay (Light); Massive grade of structure; Dry; Strong consistence; Gradual 
	change to - 
	2.4 - 2.7 m	Light grey (10YR7/2-Moist); , 10YR56, 20-50% , 30-mm, Distinct; , 20-50% , 30-mm, Distinct; 
	Sandy medium clay (Light); Massive grade of structure; Strong consistence; Gradual change to - 
	2.7 - 2.85 m	Light grey (10YR7/2-Moist); , 10YR56, 20-50% , 30-mm, Distinct; , 20-50% , 30-mm, Distinct; 
	Sandy medium clay (Light); Massive grade of structure; Strong consistence; 0-2%, coarse 
	gravelly, 20-60mm, subrounded, Quartz, coarse fragments; 
	Morphological Notes
	Observation Notes
	Site Notes
	LAURA

	Project Name:	Regional
	Project Code:	REG	Site ID:	T176	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.9A	 0.029A	 1.1B	 0.56	 0.08	 0.17	 2.1F	 4F
	0.05 - 0.1	5.9A	 0.017A	 0.36B	 0.22	 0.03	 0.12	 1.3F	 2F
	0.1 - 0.2	5.9A	 0.014A	 0.22B	 0.15	 0.01	 0.1	 1F	 1.5F
	0.2 - 0.3	5.9A	 0.011A	 0.12B	 0.17	 0.02	 0.12	 1.3F	 1.7F
	0.3 - 0.4	6A	 0.008A
	0.4 - 0.5	6.1A	 0.008A	 0.18B	 0.14	 0.01	 0.12	 0.6F	 1.1F
	0.5 - 0.6	6.1A	 0.008A
	0.6 - 0.75	5.9A	 0.011A
	0.75 - 0.9	5.9A	 0.011A	 0.18B	 0.36	 0.01	 0.12	 0.8F	 1.5F
	0.9 - 1.2	6A	 0.014A
	1.2 - 1.5	6.2A	 0.008A	 0.18B	 0.61	 0.02	 0.12	 0.6F	 1.32A	 1.5F	9.09
	1.5 - 1.8	6.3A	 0.008A
	1.8 - 2.1	6.3A	 0.008A	 0.12B	 0.71	 0.01	 0.14	 0.4F	 1.4F
	2.1 - 2.4	5.8A	 0.026A
	2.4 - 2.7	6.2A	 0.011A	 0.12B	 0.19	 0.02	 0.07
	2.7 - 2.85	6.4A	 0.011A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0.8D	 5.6B	 0.011A	 0.07A	 0.03A	 0	 93A	 3	 4	 4
	0.05 - 0.1	 0.36D	 4.5B	 0.008A	 0.03A	 0.03A	<2	 92A	 3	 5	 5
	0.1 - 0.2	 0.25D	 14.8B	 0.008A	 0.03A	<2	 92A	 3	 6	 6
	0.2 - 0.3	 0.17D	<2	 91A	 2	 7	 6
	0.3 - 0.4
	0.4 - 0.5	 0.009A	 0.03A	<2	 90A	 2	 8	 7
	0.5 - 0.6
	0.6 - 0.75
	0.75 - 0.9	 6.6B	 0.013A	 0.04A	<2	 84A	 2	 14	 13
	0.9 - 1.2
	1.2 - 1.5	 2	 83A	 2	 15	 1
	1.5 - 1.8
	1.8 - 2.1	 2	 83A	 2	 14	 1
	2.1 - 2.4
	2.4 - 2.7
	2.7 - 2.85
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.75
	0.75 - 0.9

	Project Name:	Regional
	Project Code:	REG	Site ID:	T176	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2.1
	2.1 - 2.4
	2.4 - 2.7
	2.7 - 2.85

	Project Name:	Regional
	Project Code:	REG	Site ID:	T176	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	MIN_EC	Exchange Capacity - Minerology
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_K2O	K2O - X-Ray Diffraction or Clay Fraction (air dry)
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction