Project Name:	Regional
	Project Code:	REG	Site ID:	T177	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G. Smith	Locality:	25.9KM north of Laura Post Office on Kennedy 
	Highway:
	Date Desc.:	03/11/70	Elevation:	No Data
	Map Ref.:	Sheet No. : 7767   1:100000	Rainfall:	940
	Northing/Long.:	144.233333333333	Runoff:	Very slow
	Easting/Lat.:	-15.4638888888889	Drainage:	Well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Tf	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Upper-slope	Relief:	30 metres
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Mesotrophic Red Kandosol     	Principal Profile Form:	Gn2.14
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus tetrodonta, Eucalyptus polycarpa
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.05 m	Dark reddish brown (5YR2/2-Moist); Dark greyish brown (10YR4/2-Dry); ; Loamy sand; Massive 
	grade of structure; Dry; Firm consistence; Many, fine (1-2mm) roots; Clear change to - 
	A2	0.05 - 0.1 m	Dark reddish brown (5YR3/3-Moist); Reddish brown (5YR4/3-Dry); ; Loamy sand; Massive grade 
	of structure; Dry; Strong consistence; Common, fine (1-2mm) roots; Gradual change to - 
	A2	0.1 - 0.2 m	Dark reddish brown (5YR3/3-Moist); ; Sand; Massive grade of structure; Dry; Very strong 
	consistence; Gradual change to - 
	B1	0.2 - 0.3 m	Dark red (2.5YR3/5-Moist); ; Sand; Massive grade of structure; Dry; Rigid consistence; Gradual 
	change to - 
	B1	0.3 - 0.4 m	Dark red (2.5YR3/6-Moist); ; Sand (Heavy); Massive grade of structure; Earthy fabric; Dry; Very 
	strong consistence; Gradual change to - 
	B1	0.4 - 0.5 m	Dark red (2.5YR3/6-Moist); ; Sandy loam (Light); Massive grade of structure; Earthy fabric; Dry; 
	Very strong consistence; Gradual change to - 
	B21	0.5 - 0.6 m	Dark red (2.5YR3/6-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; Dry; Very
	 strong consistence; Gradual change to - 
	B22	0.6 - 0.75 m	Red (10R4/8-Moist); ; Sandy clay loam (Heavy); Massive grade of structure; Earthy fabric; Dry; 
	Very strong consistence; Gradual change to - 
	B22	0.75 - 0.9 m	Red (10R4/8-Moist); ; Sandy medium clay; Massive grade of structure; Earthy fabric; Dry; Very 
	strong consistence; 2-10%, fine gravelly, 2-6mm, Quartz, coarse fragments; Gradual change to - 
	B22	0.9 - 1.2 m	Red (10R4/8-Moist); ; Sandy medium clay; Massive grade of structure; Earthy fabric; Dry; Rigid 
	consistence; 2-10%, fine gravelly, 2-6mm, Quartz, coarse fragments; Gradual change to - 
	1.2 - 1.5 m	Red (10R4/8-Moist); ; Sandy medium clay; Massive grade of structure; Earthy fabric; Very strong 
	consistence; Gradual change to - 
	1.5 - 1.8 m	Red (10R4/8-Moist); ; Sandy medium clay; Massive grade of structure; Earthy fabric; Very strong 
	consistence; Gradual change to - 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T177	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	1.8 - 2.1 m	Red (10R4/8-Moist); ; Sandy medium clay; Massive grade of structure; Very strong consistence; 
	2-10%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; Gradual change to - 
	2.1 - 2.4 m	Red (10R4/8-Moist); ; Sandy medium clay; Massive grade of structure; Very strong consistence; 
	2-10%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; Gradual change to - 
	2.4 - 2.7 m	Red (10R4/8-Moist); ; Sandy medium clay; Massive grade of structure; Very strong consistence; 
	2-10%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; Gradual change to - 
	2.7 - 2.85 m	Red (10R4/8-Moist); ; Sandy medium clay; Massive grade of structure; Very strong consistence; 
	2-10%, medium gravelly, 6-20mm, subrounded, Quartz, coarse fragments; Clear change to - 
	C1	2.85 - 2.9 m	Red (10R4/8-Moist); ; Sandy medium clay; Massive grade of structure; Dry; Very strong 
	consistence; 90-100%, coarse gravelly, 20-60mm, subrounded, Quartz, coarse fragments; 
	Gradual change to - 
	2.9 - 3.05 m	Yellowish red (5YR4/8-Moist); ; Sandy medium clay; Gradual change to - 
	3.05 - 3.2 m	Yellowish red (5YR4/8-Moist); ; Sandy clay loam; Clear change to - 
	3.2 - 3.4 m	Yellowish red (5YR4/8-Moist); ; Sandy clay loam; Gradual change to - 
	3.4 - 3.55 m	; 
	Morphological Notes
	Soft consolidated yellow material:larger round pebbles:
	Observation Notes
	290-340CM YELLOW MATERIAL INCREASING DOWNWARDS:                                                                         
	Site Notes
	LAURA

	Project Name:	Regional
	Project Code:	REG	Site ID:	T177	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.2A	 0.032A	 2.4B	 1.3	 0.06	 0.1	 1.1F	 5F
	0.05 - 0.1	6.6A	 0.023A	 1.6B	 0.68	 0.03	 0.14	 0.2F	 2.7F
	0.1 - 0.2	6.6A	 0.02A	 1.1B	 0.48	 0.01	 0.1	 0.2F	 1.9F
	0.2 - 0.3	6.8A	 0.017A	 0.92B	 0.4	 0.01	 0.12	 0.3F	 1.8F
	0.3 - 0.4	6.9A	 0.014A	 0.8B	 0.33	 0.01	 0.17	 0.5F	 1.8F
	0.4 - 0.5	6.9A	 0.014A
	0.5 - 0.6	6.4A	 0.02A	 0.76B	 0.67	 0.02	 0.13	 0.7F	 2.3F
	0.6 - 0.75	6.6A	 0.02A
	0.75 - 0.9	6.5A	 0.014A	 0.86B	 0.84	 0.02	 0.14	 0.5F	 2.4F
	0.9 - 1.2	6.1A	 0.014A
	1.2 - 1.5	5.8A	 0.041A	 0.76B	 0.64	 0.02	 0.22	 0.6F	 2.2F
	1.5 - 1.8	6.1A	 0.014A
	1.8 - 2.1	6.2A	 0.011A	 3.8B	 0.84	 0.02	 0.17
	2.1 - 2.4	6.1A	 0.014A
	2.4 - 2.7	6.2A	 0.014A	 0.46B	 1	 0.02	 0.17	 0.8F	 2.5F
	2.7 - 2.85	6A	 0.02A
	2.85 - 2.9	5.7A	 0.047A	 0.26B	 1.2	 0.05	 0.29
	2.9 - 3.05	6A	 0.02A
	3.05 - 3.2	5.9A	 0.014A
	3.2 - 3.4	6A	 0.014A	 0.22B	 1.6	 0.04	 0.18
	3.4 - 3.55	6.2A	 0.014A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0.91D	 6.1B	 0.011A	 0.05A	 0.03A	 0	 72A	 19	 3	 6
	0.05 - 0.1	 0.37D	 4.5B	 0.01A	 0.03A	 0.03A	<2	 77A	 15	 3	 6
	0.1 - 0.2	 0.22D	 4.2B	 0.009A	 0.02A	 0	 74A	 17	 2	 7
	0.2 - 0.3	 0.17D	 4.2B	 0	 63A	 25	 3	 9
	0.3 - 0.4	 0	 68A	 20	 2	 10
	0.4 - 0.5
	0.5 - 0.6	<2	 60A	 20	 2	 18
	0.6 - 0.75
	0.75 - 0.9	 3.5B	 0.02A	 0.06A	<2	 56A	 16	 2	 26
	0.9 - 1.2
	1.2 - 1.5	 2	 50A	 18	 2	 30
	1.5 - 1.8
	1.8 - 2.1	 2	 54A	 18	 2	 26
	2.1 - 2.4
	2.4 - 2.7	 4	 47A	 22	 2	 29
	2.7 - 2.85
	2.85 - 2.9	 54	 52A	 19	 2	 27
	2.9 - 3.05
	3.05 - 3.2
	3.2 - 3.4	 44	 41A	 19	 3	 37
	3.4 - 3.55
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Regional
	Project Code:	REG	Site ID:	T177	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.75
	0.75 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2.1
	2.1 - 2.4
	2.4 - 2.7
	2.7 - 2.85
	2.85 - 2.9
	2.9 - 3.05
	3.05 - 3.2
	3.2 - 3.4
	3.4 - 3.55

	Project Name:	Regional
	Project Code:	REG	Site ID:	T177	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_FE	Total element - Fe(%) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)