Project Name:	Regional
	Project Code:	REG	Site ID:	T178	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G. Smith	Locality:	5.8KM north of Olive Vale on Lakefield Road running 
	north from Laura:7.8KM from Kennedy Highway:
	Date Desc.:	04/11/70	Elevation:	No Data
	Map Ref.:	Sheet No. : 7766   1:100000	Rainfall:	910
	Northing/Long.:	144.425	Runoff:	Very slow
	Easting/Lat.:	-15.5041666666667	Drainage:	Well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Tf	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Rises
	Morph. Type:	Crest	Relief:	15 metres
	Elem. Type:	Hillcrest	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Manganic Mesotrophic Red Kandosol     	Principal Profile Form:	Gn2.14
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus tetrodonta, Eucalyptus polycarpa
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.05 m	Dark reddish brown (5YR3/3-Moist); Reddish brown (5YR4/4-Dry); ; Loamy sand; Massive grade 
	of structure; Dry; Strong consistence; Clear change to - 
	A21	0.05 - 0.1 m	Dark red (2.5YR3/5-Moist); Red (2.5YR4/6-Dry); ; Loamy sand; Massive grade of structure; Dry; 
	Strong consistence; Gradual change to - 
	A22	0.1 - 0.2 m	Dark red (2.5YR3/8-Moist); Red (2.5YR4/6-Dry); ; Loamy sand; Massive grade of structure; Dry; 
	Very strong consistence; Gradual change to - 
	A22	0.2 - 0.3 m	Dark red (2.5YR3/8-Moist); ; Loamy sand; Massive grade of structure; Dry; Very strong 
	consistence; Gradual change to - 
	B1	0.3 - 0.4 m	Dark red (10R3/8-Moist); ; Loamy sand (Heavy); Massive grade of structure; Earthy fabric; Dry; 
	Rigid consistence; Gradual change to - 
	B1	0.4 - 0.5 m	Dark red (10R3/8-Moist); ; Sandy loam (Light); Massive grade of structure; Dry; Strong 
	consistence; Gradual change to - 
	B21	0.5 - 0.6 m	Dark red (10R3/8-Moist); ; Sandy clay loam (Light); Massive grade of structure; Dry; Strong 
	consistence; Gradual change to - 
	B21	0.6 - 0.75 m	Dark red (10R3/8-Moist); ; Sandy clay loam; Massive grade of structure; Dry; Very strong 
	consistence; Gradual change to - 
	B21	0.75 - 0.9 m	Dark red (10R3/8-Moist); ; Sandy clay loam; Massive grade of structure; Dry; Very strong 
	consistence; Gradual change to - 
	B22	0.9 - 1.2 m	Dark red (10R3/8-Moist); , 0-2% , 5-15mm, Distinct; , 0-2% , 5-15mm, Distinct; Sandy clay loam 
	(Heavy); Massive grade of structure; Earthy fabric; Dry; Very strong consistence; Gradual change
	 to - 
	B22	1.2 - 1.5 m	Dark red (10R3/8-Moist); ; Sandy clay loam (Heavy); Massive grade of structure; Dry; Rigid 
	consistence; Gradual change to - 
	B22	1.5 - 1.8 m	Dark red (10R3/8-Moist); ; Sandy clay loam (Heavy); Massive grade of structure; Dry; Rigid 
	consistence; Gradual change to - 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T178	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	1.8 - 2.1 m	Dark red (10R3/8-Moist); ; Sandy clay loam (Heavy); Massive grade of structure; Rigid 
	consistence; Gradual change to - 
	2.1 - 2.4 m	Dark red (10R3/8-Moist); ; Sandy clay loam (Heavy); Massive grade of structure; Rigid 
	consistence; Gradual change to - 
	2.4 - 2.7 m	Dark red (10R3/8-Moist); ; Sandy clay loam; Massive grade of structure; Rigid consistence; 
	Gradual change to - 
	2.7 - 3 m	Dark red (10R3/8-Moist); ; Sandy clay loam; Massive grade of structure; Rigid consistence; 
	Gradual change to - 
	3 - 3.3 m	Dark red (10R3/8-Moist); ; Sandy clay loam; Massive grade of structure; Very strong consistence;
	 Gradual change to - 
	3.3 - 3.6 m	Dark red (10R3/8-Moist); ; Sandy clay loam; Massive grade of structure; Very strong consistence;
	 Gradual change to - 
	3.6 - 3.9 m	Dark red (10R3/8-Moist); ; Sandy clay loam; Massive grade of structure; Very strong consistence;
	 Gradual change to - 
	3.9 - 4.2 m	Dark red (10R3/8-Moist); ; Sandy clay loam; Massive grade of structure; Very strong consistence;
	 0-2%, medium gravelly, 6-20mm, subrounded, Quartz, coarse fragments; Gradual change to - 
	4.2 - 4.3 m	Dark red (10R3/8-Moist); ; Sandy clay loam; Massive grade of structure; Very strong consistence;
	 20-50%, medium gravelly, 6-20mm, rounded, Quartz, coarse fragments; Many (20 - 50 %), 
	Manganiferous, Coarse (6 - 20 mm), Nodules; Clear change to - 
	4.3 - 4.45 m	Dark red (10R3/8-Moist); ; Sandy clay loam; Massive grade of structure; Very strong consistence;
	 50-90%, coarse gravelly, 20-60mm, Quartz, coarse fragments; Gradual change to - 
	4.45 - 4.55 m	Dark red (10R3/8-Moist); ; Sandy clay loam; Massive grade of structure; Very strong consistence; 
	Morphological Notes
	Observation Notes
	Site Notes
	LAURA

	Project Name:	Regional
	Project Code:	REG	Site ID:	T178	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.1A	 0.029A	 1.8B	 0.66	 0.09	 0.17	 1.9F	 4.6F
	0.05 - 0.1	6.3A	 0.017A	 1.2B	 0.42	 0.06	 0.12	 0.4F	 2.2F
	0.1 - 0.2	6.4A	 0.014A	 0.8B	 0.34	 0.08	 0.17	 0.4F	 1.8F
	0.2 - 0.3	6.5A	 0.011A	 0.4B	 0.31	 0.04	 0.14	 0.7F	 1.6F
	0.3 - 0.4	6.5A	 0.011A	 0.4B	 0.36	 0.04	 0.14	 0.4F	 1.3F
	0.4 - 0.5	6.3A	 0.017A
	0.5 - 0.6	6.4A	 0.011A
	0.6 - 0.75	6.3A	 0.011A	 0.56B	 0.84	 0.04	 0.12	 0.4F	 2F
	0.75 - 0.9	6.2A	 0.008A
	0.9 - 1.2	6.1A	 0.017A
	1.2 - 1.5	6.2A	 0.011A	 0.4B	 1.3	 0.03	 0.12	 0.7F	 2.6F
	1.5 - 1.8	6.3A	 0.011A
	1.8 - 2.1	6.4A	 0.011A	 0.22B	 2.09	 0.04	 0.14	 0.7F	 2.38A	 3.2F	5.88
	2.1 - 2.4	6.4A	 0.017A
	2.4 - 2.7	6.2A	 0.008A	 0.12B	 1.9	 0.03	 0.14	 0.7F	 2.9F
	2.7 - 3	6.4A	 0.011A
	3 - 3.3	6.4A	 0.011A
	3.3 - 3.6	6.4A	 0.011A
	3.6 - 3.9	6.4A	 0.008A	 0.12B	 1.8	 0.03	 0.12	 0.4F	 2.5F
	3.9 - 4.2	6.1A	 0.032A
	4.2 - 4.3	6.6A	 0.011A	 0.12B	 1.6	 0.04	 0.12
	4.3 - 4.45	6.5A	 0.011A
	4.45 - 4.55	6.4A	 0.014A	 0.12B	 1.6	 0.04	 0.17
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0.66D	 4.9B	 0.005A	 0.04A	 0.06A	 0	 58A	 35	 2	 5
	0.05 - 0.1	 0.33D	 5.5B	 0.007A	 0.03A	 0.06A	 0	 57A	 36	 2	 5
	0.1 - 0.2	 0.2D	 3.5B	 0.005A	 0.06A	 0	 54A	 38	 2	 6
	0.2 - 0.3	 0.12D	 4.2B	 0	 48A	 42	 2	 7
	0.3 - 0.4	 0	 54A	 35	 2	 9
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.75	 2.8B	 0.009A	 0.16A	<2	 47A	 30	 2	 21
	0.75 - 0.9
	0.9 - 1.2
	1.2 - 1.5	<2	 39A	 31	 2	 28
	1.5 - 1.8
	1.8 - 2.1	 2	 37A	 28	 2	 33
	2.1 - 2.4
	2.4 - 2.7	 2	 35A	 33	 2	 30
	2.7 - 3
	3 - 3.3
	3.3 - 3.6
	3.6 - 3.9	 2	 35A	 34	 2	 29
	3.9 - 4.2
	4.2 - 4.3
	4.3 - 4.45
	4.45 - 4.55

	Project Name:	Regional
	Project Code:	REG	Site ID:	T178	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.75
	0.75 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2.1
	2.1 - 2.4
	2.4 - 2.7
	2.7 - 3
	3 - 3.3
	3.3 - 3.6
	3.6 - 3.9
	3.9 - 4.2
	4.2 - 4.3
	4.3 - 4.45
	4.45 - 4.55

	Project Name:	Regional
	Project Code:	REG	Site ID:	T178	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_FE	Total element - Fe(%) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)