Project Name:	Regional
	Project Code:	REG	Site ID:	T18	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.G. Murtha	Locality:	Site in sewerage pit at Ritson's house:
	Date Desc.:	16/07/64	Elevation:	No Data
	Map Ref.:	Sheet No. : 8258   1:100000	Rainfall:	0
	Northing/Long.:	146.833333333333	Runoff:	Slow
	Easting/Lat.:	-19.6583333333333	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qa	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Sodic Calcic Brown Chromosol     	Principal Profile Form:	Dy3.43
	ASC Confidence:	Great Soil Group:	Solodic soil
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.13 m	Dark greyish brown (10YR4/2-Moist); , 0-0% ; , 0-0% ; Loam; Massive grade of structure; 
	Moderately moist; Weak consistence; 
	A2	0.13 - 0.38 m	Brown (10YR5/3-Moist); Very pale brown (10YR7/3-Dry); , 0-0% ; , 0-0% ; Sandy loam; Massive 
	grade of structure; Dry; Very strong consistence; Few (2 - 10 %), Ferromanganiferous, Medium (2
	 -6 mm), Nodules; Gradual change to - 
	B21	0.38 - 0.61 m	Yellowish brown (10YR5/4-Moist); , 0-0% ; , 0-0% ; Medium heavy clay; Moderate grade of 
	structure, 20-50 mm, Subangular blocky; Very coarse, (20 - 50) mm crack; Dry; Very strong 
	consistence; 0-2%, medium gravelly, 6-20mm, Gravel, coarse fragments; Very few (0 - 2 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules; Clear change to - 
	B22	0.61 - 0.91 m	Yellowish brown (10YR5/4-Moist); , 7.5YR56, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, 
	Distinct; Medium heavy clay; Moderate grade of structure, 100-200 mm, Prismatic; Very coarse, 
	(20 - 50) mm crack; Moderately moist; Very strong consistence; 0-2%, medium gravelly, 6-20mm,
	 Gravel, coarse fragments; Few (2 - 10 %), Ferromanganiferous, Medium (2 -6 mm), Nodules; 
	Very few (0 - 2 %), Calcareous, Coarse (6 - 20 mm), Concretions; Diffuse change to - 
	B23	0.91 - 1.22 m	Brown (10YR4/3-Moist); , 5YR44, 10-20% , 15-30mm, Distinct; , 10-20% , 15-30mm, Distinct; 
	Medium heavy clay; Moderate grade of structure, 50-100 mm, Prismatic; Very coarse, (20 - 50) 
	mm crack; Moderately moist; Very strong consistence; 2-10%, medium gravelly, 6-20mm, Gravel,
	 coarse fragments; Very few (0 - 2 %), Ferromanganiferous, Coarse (6 - 20 mm), Nodules; Very 
	few (0 - 2 %), Calcareous, Coarse (6 - 20 mm), Concretions; Diffuse change to - 
	B23	1.22 - 1.52 m	Brown (10YR4/3-Moist); , 5YR44, 10-20% , 15-30mm, Distinct; , 10-20% , 15-30mm, Distinct; 
	Medium heavy clay; Moderate grade of structure, 20-50 mm, Subangular blocky; Very coarse, (20
	 - 50) mm crack; Moderately moist; Very strong consistence; Very few (0 - 2 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules; Few (2 - 10 %), Calcareous, Extremely coarse 
	(> 60 mm), Concretions; 
	1.52 - 2.03 m	Reddish brown (5YR4/4-Moist); , 10YR42, 10-20% , 15-30mm, Distinct; , 10-20% , 15-30mm, 
	Distinct; Sandy medium clay; Moderate grade of structure, 20-50 mm, Subangular blocky; Very 
	strong consistence; 0-2%, coarse gravelly, 20-60mm, Gravel, coarse fragments; Very few (0 - 2 
	%), Ferromanganiferous, Fine (0 - 2 mm), Nodules; Few (2 - 10 %), Calcareous, Extremely 
	coarse (> 60 mm), Concretions; Diffuse change to - 
	Morphological Notes
	Observation Notes

	Project Name:	Regional
	Project Code:	REG	Site ID:	T18	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Notes
	LANDSDOWN

	Project Name:	Regional
	Project Code:	REG	Site ID:	T18	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	5.9A	 0.089A	 5.4E	 1.8	 0.6	 0.15	 4F	 12C	 12F	1.25
	0.13 - 0.38	6.2A	 0.059A
	0.38 - 0.61	6.5A	 0.059A	 6.6E	 3.6	 0.3	 0.1	 3.8F	 14.4C	 14.4F	0.69
	0.61 - 0.91	6.7A	 0.029A
	0.91 - 1.22	7.3A	 0.089A
	1.22 - 1.52	8.2A	 0.059A	 7.4E	 4.7	 0.27	 1.1	 0.6F	 14.1F
	1.52 - 2.03	8.6A	 0.148A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13	 1.2D	 8B	 0.008A	 0.1A	 15D	 54	 18	 14
	0.13 - 0.38	 4B
	0.38 - 0.61	 19D	 35	 11	 34
	0.61 - 0.91
	0.91 - 1.22
	1.22 - 1.52	 0.7A	 0.005A
	1.52 - 2.03	 0.006A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13
	0.13 - 0.38
	0.38 - 0.61
	0.61 - 0.91
	0.91 - 1.22
	1.22 - 1.52
	1.52 - 2.03

	Project Name:	Regional
	Project Code:	REG	Site ID:	T18	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, 
	pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble
	 salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble
	 salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble
	 salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	19A1	Carbonates - rapid titration
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance