Project Name:	Regional
	Project Code:	REG	Site ID:	T182	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.G. Murtha	Locality:	2.4KM north of Bluewater:
	Date Desc.:	19/11/70	Elevation:	 15 metres
	Map Ref.:	Sheet No. : 8259   1:100000	Rainfall:	1140
	Northing/Long.:	146.535555555556	Runoff:	Moderately rapid
	Easting/Lat.:	-19.1619444444444	Drainage:	Moderately well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qa	Substrate Material:	Undisturbed soil core, 1.2 m 
	deep,Unconsolidated material 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Stagnant alluvial plain
	Morph. Type:	No Data	Relief:	1 metres
	Elem. Type:	Prior stream	Slope Category:	No Data
	Slope:	0 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Class Undetermined Yellow Kandosol     	Principal Profile Form:	Gn2.74
	ASC Confidence:	Great Soil Group:	Yellow earth
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - None recorded
	Mid Strata - Tree, 1.01-3m, Very sparse. *Species includes - Acacia species, Melaleuca viridiflora
	Tall Strata - Tree, 3.01-6m, Very sparse. *Species includes - Eucalyptus alba, Eucalyptus polycarpa, Trigonella 
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.04 m	Very dark greyish brown (10YR3/2-Moist); ; Loamy sand; Massive grade of structure; Moist; Very 
	weak consistence; 20-50%, Charcoal, coarse fragments; Clear change to - 
	A2	0.04 - 0.1 m	Brown (10YR5/3-Moist); ; Sandy loam; Massive grade of structure; Moist; Weak consistence; 2-
	10%, fine gravelly, 2-6mm, Quartz, coarse fragments; Many, fine (1-2mm) roots; 
	A2	0.1 - 0.2 m	Brown (10YR5/3-Moist); ; Sandy loam; Massive grade of structure; Moist; Weak consistence; 2-
	10%, fine gravelly, 2-6mm, Quartz, coarse fragments; Gradual change to - 
	B1	0.2 - 0.3 m	Yellowish brown (10YR5/5-Moist); ; Sandy loam (Heavy); Massive grade of structure; Many (>5 
	per 100mm2) Fine (1-2mm) macropores, Moist; Weak consistence; 2-10%, fine gravelly, 2-6mm, 
	Quartz, coarse fragments; Very few (0 - 2 %), Ferromanganiferous, Medium (2 -6 mm), Nodules; 
	B1	0.3 - 0.45 m	Yellowish brown (10YR5/5-Moist); ; Sandy clay loam (Light); Massive grade of structure; Earthy 
	fabric; Moist; Weak consistence; 10-20%, fine gravelly, 2-6mm, Quartz, coarse fragments; Few 
	(2 - 10 %), Unidentified, Very coarse (20 - 60 mm), Concretions; 
	B2	0.45 - 0.6 m	Yellowish brown (10YR5/4-Moist); , 10YR58, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, 
	Distinct; Sandy clay loam; Massive grade of structure; Earthy fabric; Moderately moist; Firm 
	consistence; 0-2%, coarse gravelly, 20-60mm, rounded, Arkose, coarse fragments; Very few (0 - 
	2 %), Ferromanganiferous, Coarse (6 - 20 mm), Concretions; 
	B2	0.6 - 0.9 m	Light yellowish brown (10YR6/4-Moist); , 10YR58, 10-20% , 5-15mm, Distinct; , 10-20% , 5-
	15mm, Distinct; Sandy clay loam; Massive grade of structure; Earthy fabric; Common (1-5 per 
	0.01m2) Coarse (>5mm) macropores, Dry; Firm consistence; 20-50%, fine gravelly, 2-6mm, 
	Quartz, coarse fragments; Very few (0 - 2 %), Ferromanganiferous, Coarse (6 - 20 mm), 
	Concretions; 
	BC	0.9 - 1.2 m	Light yellowish brown (10YR6/4-Moist); , 10YR58, 10-20% , 5-15mm, Distinct; , 10-20% , 5-
	15mm, Distinct; Clayey sand; Massive grade of structure; Common (1-5 per 0.01m2) Coarse 
	(>5mm) macropores, Dry; Weak consistence; 20-50%, fine gravelly, 2-6mm, Quartz, coarse 
	fragments; Few (2 - 10 %), Ferruginous, Very coarse (20 - 60 mm), Concretions; 
	Morphological Notes

	Project Name:	Regional
	Project Code:	REG	Site ID:	T182	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	BEYOND 120CM IS WHITE COARSE SAND WITH SOME FE STAINED BANDING (TOP 30CM) OCCASIONAL ROUNDED GR 
	<60MM:                  
	Site Notes
	BLUEWATER
	Observation Notes

	Project Name:	Regional
	Project Code:	REG	Site ID:	T182	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04	6.1A	 0.017A
	0.04 - 0.1	5.7A	 0.014A
	0.1 - 0.2	5.6A	 0.011A
	0.2 - 0.3	5.7A	 0.014A
	0.3 - 0.45	5.7A	 0.041A
	0.45 - 0.6	5.8A	 0.017A	 0.2B	 1.4	 0.22	 0.18	 2.6C	6.92
	0.6 - 0.9	6A	 0.014A
	0.9 - 1.2	6.1A	 0.014A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04	 1.7D	<2A	 0.07A
	 5B
	0.04 - 0.1
	0.1 - 0.2	 0.43D	<2A	 0.04A
	 4B
	0.2 - 0.3
	0.3 - 0.45
	0.45 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.04
	0.04 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.45
	0.45 - 0.6
	0.6 - 0.9
	0.9 - 1.2

	Project Name:	Regional
	Project Code:	REG	Site ID:	T182	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)