Project Name:	Regional
	Project Code:	REG	Site ID:	T198	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.G. Murtha	Locality:	Opposite Upper Barron State School:
	Date Desc.:	21/01/71	Elevation:	 800 metres
	Map Ref.:	Sheet No. : 8063   1:100000	Rainfall:	1520
	Northing/Long.:	145.515277777778	Runoff:	Moderately rapid
	Easting/Lat.:	-17.3833333333333	Drainage:	Moderately well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Cza	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating hills 90-300m 3-	Pattern Type:	Hills
	Morph. Type:	Mid-slope	Relief:	100 metres
	Elem. Type:	Hillslope	Slope Category:	Moderately inclined
	Slope:	8.8 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Dystrophic Red Ferrosol     	Principal Profile Form:	Gn3.11
	ASC Confidence:	Great Soil Group:	Krasnozem
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Imperata cylindrica
	Tall Strata - Tree, 20.01-35m, Sparse. *Species includes - Eucalyptus grandifolia, Eucalyptus citriodora
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark reddish brown (5YR3/3-Moist); ; Clay loam (Heavy); Strong grade of structure, 2-5 mm, Cast;
	 Moist; Weak consistence; Many, fine (1-2mm) roots; 
	B1	0.1 - 0.2 m	Dark reddish brown (2.5YR3/4-Moist); ; Light clay; Moderate grade of structure, 5-10 mm, Angular
	 blocky; Moist; Weak consistence; Common, fine (1-2mm) roots; 
	B2	0.2 - 0.3 m	Dark red (2.5YR3/6-Moist); ; Light medium clay; Moderate grade of structure, 5-10 mm, Angular 
	blocky; Moist; Weak consistence; 
	B2	0.3 - 0.6 m	Dark red (2.5YR3/6-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, Angular blocky; 
	Moderately moist; Very firm consistence; 
	B2	0.6 - 0.9 m	Reddish brown (2.5YR4/4-Moist); ; Medium heavy clay; Strong grade of structure, <2 mm, 
	Polyhedral; Smooth-ped fabric; Moderately moist; Very firm consistence; 
	B2	0.9 - 1.2 m	Reddish brown (2.5YR4/4-Moist); ; Medium heavy clay; Strong grade of structure, <2 mm, 
	Polyhedral; Smooth-ped fabric; Moderately moist; Very firm consistence; 
	1.2 - 1.5 m	Reddish brown (2.5YR4/4-Moist); ; Heavy clay; Strong grade of structure, <2 mm, Polyhedral; 
	Smooth-ped fabric; Very firm consistence; 
	1.5 - 1.8 m	Reddish brown (2.5YR4/4-Moist); ; Heavy clay; Strong grade of structure, <2 mm, Polyhedral; 
	Smooth-ped fabric; Very firm consistence; 
	1.8 - 2.1 m	Reddish brown (2.5YR4/4-Moist); ; Heavy clay; Strong grade of structure, <2 mm, Polyhedral; 
	Smooth-ped fabric; Very firm consistence; 
	Morphological Notes
	Observation Notes
	10-20CM SOME A1 MATERIAL DOWN WORM CASTS:                                                                               
	Site Notes
	UPPER BARRON

	Project Name:	Regional
	Project Code:	REG	Site ID:	T198	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.2A	 0.127A	 5.04B	 4.24	 0.63	 0.33	 0.6F	 10.8F
	0.1 - 0.2	4.8A	 0.142A	 0.54B	 1.79	 0.24	 0.25
	0.2 - 0.3	4.8A	 0.049A	 0.34B	 1.48	 0.11	 0.25	 0.92F	 3.1F
	0.3 - 0.6	4.8A	 0.039A	 0.22B	 0.91	 0.07	 0.25	 0.8F	 2.3F
	0.6 - 0.9	4.8A	 0.059A
	0.9 - 1.2	5.2A	 0.03A	 0.21B	 0.78	 0.16	 0.23	 0.44F	 1.8F
	1.2 - 1.5	5A	 0.041A
	1.5 - 1.8	4.9A	 0.028A	 0.21B	 0.67	 0.09	 0.29	 0.6F	 1.9F
	1.8 - 2.1	4.8A	 0.047A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 5.45D	 123B	 0.32A	 0.328A	 0.12A	 0	 1A	 8	 15	 81
	0.1 - 0.2	 2.06D	 28B	 0.24A	 0.15A	 0.08A	 0	 1A	 5	 21	 78
	0.2 - 0.3	 0.99D	 19B	 0.22A	 0.121A	 0.06A
	0.3 - 0.6	 1.11D	 18B	 0.2A	 0.07A	 0.04A	 0	 0A	 6	 20	 78
	0.6 - 0.9
	0.9 - 1.2	 0.56D	 21B	 0.18A	 0.028A	 0.04A	 0	 0A	 13	 19	 71
	1.2 - 1.5
	1.5 - 1.8	 0.1D	 26B	 0.18A	 0.019A	 0.04A	 0	 1A	 6	 32	 61
	1.8 - 2.1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2.1

	Project Name:	Regional
	Project Code:	REG	Site ID:	T198	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	MIN_EC	Exchange Capacity - Minerology
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)
	XRD_C_Hm	Hematite - X-Ray Diffraction
	XRD_C_K2O	K2O - X-Ray Diffraction or Clay Fraction (air dry)
	XRD_C_Ka	Kaolin - X-Ray Diffraction