Project Name:	Regional
	Project Code:	REG	Site ID:	T199	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.F. Isbell	Locality:	1.1KM north east of Tarzali Post Office along Hogans
	 Road:
	Date Desc.:	28/09/71	Elevation:	 760 metres
	Map Ref.:	Sheet No. : 8063   1:100000	Rainfall:	2160
	Northing/Long.:	145.608333333333	Runoff:	Moderately rapid
	Easting/Lat.:	-17.1686111111111	Drainage:	Moderately well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Cza	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Low hills
	Morph. Type:	Ridge	Relief:	61 metres
	Elem. Type:	Hillcrest	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Dystrophic Red Ferrosol     	Principal Profile Form:	Gn3.11
	ASC Confidence:	Great Soil Group:	Krasnozem
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.1 m	Dark reddish brown (2.5YR3/4-Moist); Dark red (2.5YR3/6-Dry); ; Clay loam; Strong grade of 
	structure, 5-10 mm, Granular; Very firm consistence; 0-2%, coarse gravelly, 20-60mm, Quartz, 
	coarse fragments; Many, medium (2-5mm) roots; Gradual change to - 
	A12	0.1 - 0.2 m	Dark red (2.5YR3/5-Moist); Dark red (2.5YR3/6-Dry); ; Clay loam; Moderate grade of structure, 2-5 
	mm, Granular; Very firm consistence; Common, fine (1-2mm) roots; Gradual change to - 
	B1	0.2 - 0.3 m	Dark red (2.5YR3/6-Moist); ; Clay loam (Heavy); Weak grade of structure, 5-10 mm, Angular 
	blocky; Weak consistence; Few cutans, <10% of ped faces or walls coated; Few (2 - 10 %), 
	Unidentified, , Tubules; Few, fine (1-2mm) roots; Diffuse change to - 
	B1	0.3 - 0.6 m	Dusky red (10R3/4-Moist); ; Clay loam (Heavy); Weak grade of structure, 5-10 mm, Angular 
	blocky; Weak consistence; Few cutans, <10% of ped faces or walls coated; Few (2 - 10 %), 
	Unidentified, , Tubules; Few, fine (1-2mm) roots; Diffuse change to - 
	B2	0.6 - 0.9 m	Dusky red (10R3/4-Moist); ; Light clay; Moderate grade of structure, 5-10 mm, Angular blocky; 
	Weak consistence; Common cutans, 10-50% of ped faces or walls coated; Few (2 - 10 %), 
	Argillaceous, , Nodules; Few
	B2	0.9 - 1.2 m	Dusky red (10R3/4-Moist); ; Light clay; Moderate grade of structure, 5-10 mm, Angular blocky; 
	Weak consistence; Common cutans, 10-50% of ped faces or walls coated; Few (2 - 10 %), 
	Argillaceous, , Nodules; Diffuse change to - 
	B2	1.2 - 1.5 m	Dusky red (10R3/4-Moist); ; Light medium clay; Strong grade of structure, 5-10 mm, Angular 
	blocky; Weak consistence; Very few (0 - 2 %), Argillaceous, , Nodules; 
	1.5 - 1.8 m	Dusky red (10R3/4-Moist); ; Light medium clay; Strong grade of structure, 5-10 mm, Angular 
	blocky; Weak consistence; Very few (0 - 2 %), Argillaceous, , Nodules; Gradual change to - 
	1.8 - 2.1 m	Dark red (2.5YR3/5-Moist); ; Light medium clay; Strong grade of structure, 5-10 mm, Angular 
	blocky; Weak consistence; Very few (0 - 2 %), Argillaceous, , Nodules; 
	Morphological Notes
	Observation Notes
	Site Notes
	TARZALI

	Project Name:	Regional
	Project Code:	REG	Site ID:	T199	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)

	Project Name:	Regional
	Project Code:	REG	Site ID:	T199	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.1A	 0.089A	 2.99B	 1.31	 0.25	 0.22	 1.48F	 6.3F
	0.1 - 0.2	5A	 0.059A	 0.91B	 0.42	 0.13	 0.15
	0.2 - 0.3	4.8A	 0.118A	 0.77B	 0.18	 0.08	 0.14	 0.72F	 1.9F
	0.3 - 0.6	5A	 0.052A	 0.66B	 0.04	 0.01	 0.12	 0.24F	 1.1F
	0.6 - 0.9	5.1A	 0.02A
	0.9 - 1.2	5.2A	 0.024A	 0.13B	 0.11	 0.01	 0.11	 0.06F	 0.4F
	1.2 - 1.5	5.2A	 0.02A
	1.5 - 1.8	5.2A	 0.023A	 0.11B	 0.01	 0.11	 0.13	 0.04F	 0.4F
	1.8 - 2.1	5.3A	 0.02A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 4.18D	 0.326A	 0.445A	 0.077A	<2	 0A	 8	 23	 64
	0.1 - 0.2	 3.56D	 0.312A	 0.348A	 0.067A	 0	 2A	 7	 37	 61
	0.2 - 0.3	 2.57D	 0.305A	 0.261A	 0.06A
	0.3 - 0.6	 1.42D	 0.307A	 0.109A	 0.057A	 0	 2A	 8	 35	 60
	0.6 - 0.9
	0.9 - 1.2	 0.5D	 0.229A	 0.031A	 0.077A	 0	 2A	 7	 27	 71
	1.2 - 1.5
	1.5 - 1.8	 0.38D	 0.237A	 0.025A	 0.104A	 0	 3A	 5	 14	 83
	1.8 - 2.1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2.1

	Project Name:	Regional
	Project Code:	REG	Site ID:	T199	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	MIN_EC	Exchange Capacity - Minerology
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)
	XRD_C_Ch2	Chloritized 2:1 minerals - X-Ray Diffraction
	XRD_C_Gb	Gibbsite - X-Ray Diffraction
	XRD_C_Gt	Geothite - X-Ray Diffraction
	XRD_C_Hm	Hematite - X-Ray Diffraction
	XRD_C_K2O	K2O - X-Ray Diffraction or Clay Fraction (air dry)
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Mu	Muscovite - X-Ray Diffraction