Project Name:	Regional
	Project Code:	REG	Site ID:	T218	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.G. Murtha	Locality:	On boundary between Bentley and Cordingley`s:
	Date Desc.:	05/12/73	Elevation:	 15 metres
	Map Ref.:	Sheet No. : 8259   1:100000	Rainfall:	1140
	Northing/Long.:	146.953055555556	Runoff:	Slow
	Easting/Lat.:	-19.3858333333333	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qa	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	0 metres
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Sodic Eutrophic Brown Chromosol     	Principal Profile Form:	Dy3.42
	ASC Confidence:	Great Soil Group:	Solodic soil
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Heteropogon contortus
	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus drepanophylla, Eucalyptus polycarpa, Eucalyptus 
	tessellaris
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark grey (10YR4/1-Moist); ; Silty loam; Massive grade of structure; Dry; Very firm consistence; 
	Gradual change to - 
	A2	0.1 - 0.2 m	Greyish brown (10YR5/2-Moist); Light grey (10YR7/2-Dry); ; Silty loam; Massive grade of 
	structure; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Firm consistence; Few (2 -
	 10 %), Ferromanganiferous, Medium (2 -6 mm), Nodules; 
	A2	0.2 - 0.3 m	Greyish brown (10YR5/2-Moist); Light grey (10YR7/2-Dry); ; Silty loam; Massive grade of 
	structure; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Firm consistence; Few (2 -
	 10 %), Ferromanganiferous, Medium (2 -6 mm), Nodules; Gradual change to - 
	A3	0.3 - 0.35 m	Yellowish brown (10YR5/4-Moist); Very pale brown (10YR7/4-Dry); ; Silty clay loam; Massive 
	grade of structure; Dry; Firm consistence; Abrupt change to - 
	B2	0.35 - 0.5 m	Yellowish brown (10YR5/6-Moist); , 10YR62, 10-20% , 5-15mm, Faint; , 10-20% , 5-15mm, Faint;
	 Heavy clay; Moderate grade of structure, 10-20 mm, Angular blocky; Dry; Very strong 
	consistence; 0-2%, fine gravelly, 2-6mm, Quartz, coarse fragments; Few (2 - 10 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules; 
	B2	0.5 - 0.6 m	Yellowish brown (10YR5/6-Moist); , 10YR62, 10-20% , 5-15mm, Faint; , 10-20% , 5-15mm, Faint;
	 Heavy clay; Moderate grade of structure, 10-20 mm, Angular blocky; Dry; Very strong 
	consistence; 0-2%, fine gravelly, 2-6mm, Quartz, coarse fragments; Few (2 - 10 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules; 
	B2	0.6 - 0.9 m	Yellowish brown (10YR5/8-Moist); , 10YR62, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, 
	Distinct; Heavy clay; Moderate grade of structure, 10-20 mm, Angular blocky; Dry; Very strong 
	consistence; 0-2%, fine gravelly, 2-6mm, Quartz, coarse fragments; Few (2 - 10 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules; 
	BC	0.9 - 1.2 m	Yellowish brown (10YR5/6-Moist); , 10YR51, 10-20% , 0-5mm, Distinct; , 10-20% , 0-5mm, 
	Distinct; Heavy clay; Weak grade of structure, 20-50 mm, Angular blocky; Dry; Very strong 
	consistence; Common (10 - 20 %), Ferromanganiferous, Coarse (6 - 20 mm), Concretions; 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T218	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	BC	1.2 - 1.38 m	Yellowish brown (10YR5/6-Moist); , 10YR51, 10-20% , 0-5mm, Distinct; , 10-20% , 0-5mm, 
	Distinct; Heavy clay; Weak grade of structure, 20-50 mm, Angular blocky; Dry; Very strong 
	consistence; Common (10 - 20 %), Ferromanganiferous, Coarse (6 - 20 mm), Concretions; 
	Gradual change to - 
	D	1.38 - 1.5 m	Grey (10YR5/1-Moist); , 10YR43, 20-50% , 0-5mm, Faint; , 20-50% , 0-5mm, Faint; Heavy clay; 
	Strong grade of structure, 5-10 mm, Angular blocky; Dry; Very strong consistence; Few (2 - 10 
	%), Ferromanganiferous, Medium (2 -6 mm), Nodules; 
	D	1.5 - 1.8 m	Grey (10YR5/1-Moist); , 10YR43, 20-50% , 0-5mm, Faint; , 20-50% , 0-5mm, Faint; Heavy clay; 
	Strong grade of structure, 5-10 mm, Angular blocky; Dry; Very strong consistence; Few (2 - 10 
	%), Ferromanganiferous, Medium (2 -6 mm), Nodules; 
	D	1.8 - 2.05 m	Grey (10YR5/1-Moist); , 10YR43, 20-50% , 0-5mm, Faint; , 20-50% , 0-5mm, Faint; Heavy clay; 
	Strong grade of structure, 5-10 mm, Angular blocky; Dry; Very strong consistence; Few (2 - 10 
	%), Ferromanganiferous, Medium (2 -6 mm), Nodules; 
	Morphological Notes
	Observation Notes
	30-35CM SOME BLEACHED PATCHES THROUGHOUT:60-90CM FEW COARSE SLICKENSIDES:90-138CM MUCH 
	FELSPATHIC FLECKING:             
	Site Notes
	ALLIGATOR CK

	Project Name:	Regional
	Project Code:	REG	Site ID:	T218	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.8A	<0.05A	 3.5B	 1.6	 0.55	 0.03
	0.1 - 0.2	5.8A	<0.05A
	0.2 - 0.3	5.6A	<0.05A
	0.3 - 0.35	5.8A	<0.05A
	0.35 - 0.5	6.2A	<0.05A	 5.6B	 5.9	 0.11	 0.46
	0.5 - 0.6	6.5A	<0.05A	 5.5B	 5.6	 0.11	 0.72
	0.6 - 0.9	6.9A	<0.05A
	0.9 - 1.2	7.6A	<0.05A	 5.2B	 4.9	 0.11	 1.1
	1.2 - 1.38	8.3A	 0.092A
	1.38 - 1.5	8.5A	 0.151A	 7.7B	 6.3	 0.04	 2.7
	1.5 - 1.8	8.5A	 0.25A
	1.8 - 2.05	8.5A	 0.339A	 7.8B	 6.8	 0.04	 4
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.94D	 20.8B	 0.027A	 0.09A	 2.12A	 0	 13A	 41	 32	 12
	0.1 - 0.2
	0.2 - 0.3	 3.6B	 0	 13A	 41	 30	 16
	0.3 - 0.35
	0.35 - 0.5	 0.025A	 1.35A	 0	 7A	 22	 16	 56
	0.5 - 0.6
	0.6 - 0.9
	0.9 - 1.2	 0.024A	 2.12A	<2	 25A	 24	 21	 33
	1.2 - 1.38
	1.38 - 1.5	<2	 12A	 28	 27	 33
	1.5 - 1.8
	1.8 - 2.05	 0	 10A	 32	 23	 36
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.35
	0.35 - 0.5
	0.5 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.38
	1.38 - 1.5
	1.5 - 1.8
	1.8 - 2.05

	Project Name:	Regional
	Project Code:	REG	Site ID:	T218	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)