Project Name:	Regional
	Project Code:	REG	Site ID:	T221	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.G. Murtha	Locality:	2.1KM east along track from Rocky Springs 
	Homestead:
	Date Desc.:	06/12/73	Elevation:	 61 metres
	Map Ref.:	Sheet No. : 8259   1:100000	Rainfall:	1140
	Northing/Long.:	146.891666666667	Runoff:	Rapid
	Easting/Lat.:	-19.3791666666667	Drainage:	Well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	C-Pv	Substrate Material:	Undisturbed soil core, 1.2 m deep,Andesite 
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Mid-slope	Relief:	12 metres
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Eutrophic Red Dermosol     	Principal Profile Form:	Dr2.22
	ASC Confidence:	Great Soil Group:	Non-calcic brown 
	All necessary analytical data are available.	soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus drepanophylla, Eucalyptus alba, Eucalyptus 
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Very dark grey (5YR3/1-Moist); ; Loam (Heavy); Weak grade of structure, 5-10 mm, Angular 
	blocky; Dry; Very firm consistence; 0-2%, medium gravelly, 6-20mm, Gravel, coarse fragments; 
	Gradual change to - 
	A2	0.1 - 0.16 m	Dark reddish grey (5YR4/2-Moist); ; Loam (Heavy); Weak grade of structure, 5-10 mm, Angular 
	blocky; Moderately moist; Firm consistence; Many (20 - 50 %), Ferromanganiferous, Fine (0 - 2 
	mm), Nodules; Clear change to - 
	B21	0.16 - 0.2 m	Dark red (2.5YR3/6-Moist); ; Light medium clay; Moderate grade of structure, 10-20 mm, Angular 
	blocky; Moist; Very firm consistence; Very few (0 - 2 %), Ferromanganiferous, Medium (2 -6 mm), 
	Nodules; 
	B21	0.2 - 0.3 m	Dark red (2.5YR3/6-Moist); ; Light medium clay; Moderate grade of structure, 10-20 mm, Angular 
	blocky; Moist; Very firm consistence; Very few (0 - 2 %), Ferromanganiferous, Medium (2 -6 mm), 
	Nodules; 
	B22	0.3 - 0.6 m	Dark red (2.5YR3/6-Moist); ; Medium heavy clay; Strong grade of structure, 10-20 mm, Angular 
	blocky; Moist; Very firm consistence; 0-2%, subrounded, Andesite, coarse fragments; Very few 
	(0 - 2 %), Ferromanganiferous, Medium (2 -6 mm), Nodules; 
	B22	0.6 - 0.9 m	Yellowish red (5YR5/6-Moist); , 10YR63, 2-10% , 0-5mm, Faint; , 2-10% , 0-5mm, Faint; Medium 
	heavy clay; Moderate grade of structure, 10-20 mm, Angular blocky; Moist; Very firm 
	consistence; 
	BC	0.9 - 1.13 m	Yellowish red (5YR5/6-Moist); , 10YR62, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, 
	Distinct; Medium heavy clay; Moderate grade of structure, 20-50 mm, Angular blocky; Moist; Very
	 firm consistence; 
	C	1.13 - 1.2 m	; 
	C	1.2 - 1.5 m	; 
	Morphological Notes
	C	Soft weathered parent material (113-150CM):

	Project Name:	Regional
	Project Code:	REG	Site ID:	T221	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	16-30CM A HORIZON MATERIAL DOWN WORM CASTS:60-113CM W`D PARENT MATERIALINCREASING DOWN PROFILE:  
	                       
	Site Notes
	ROCKY SPRINGS
	Observation Notes

	Project Name:	Regional
	Project Code:	REG	Site ID:	T221	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.4A	<0.05A	 15.1B	 5.4	 1.2	 0.07
	0.1 - 0.16	6.2A	<0.05A
	0.16 - 0.2	6.2A	<0.05A
	0.2 - 0.3	6.3A	<0.05A	 9B	 3.1	 0.47	 0.06
	0.3 - 0.6	6.7A	<0.05A
	0.6 - 0.9	7A	<0.05A	 10.9B	 7.1	 0.09	 0.16
	0.9 - 1.13	7.2A	<0.05A
	1.13 - 1.2	7.3A	<0.05A
	1.2 - 1.5	7.2A	<0.05A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 3.75D	 153B	 0.13A	 0.21A	 1.38A	 0	 15A	 27	 27	 31
	0.1 - 0.16	 0	 13A	 29	 26	 31
	0.16 - 0.2	 0	 16A	 28	 24	 32
	0.2 - 0.3	 12B	 0.058A	 1.46A	 0	 14A	 27	 23	 37
	0.3 - 0.6
	0.6 - 0.9	 4	 6A	 12	 18	 63
	0.9 - 1.13
	1.13 - 1.2	 652B	 0.082A	 1.13A
	1.2 - 1.5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.16
	0.16 - 0.2
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.9
	0.9 - 1.13
	1.13 - 1.2
	1.2 - 1.5

	Project Name:	Regional
	Project Code:	REG	Site ID:	T221	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)