Project Name:	Regional
	Project Code:	REG	Site ID:	T228	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.J. Coventry	Locality:	18 Km E. of Torrens Ck.
	Date Desc.:	16/11/76	Elevation:	No Data
	Map Ref.:	Sheet No. : 7956   1:100000	Rainfall:	600
	Northing/Long.:	145.194444444444	Runoff:	No Data
	Easting/Lat.:	-20.7277777777778	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	N/A
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Sodic Magnesic Yellow Kandosol     	Principal Profile Form:	Gn2.64
	ASC Confidence:	Great Soil Group:	Yellow earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - None recorded
	Tall Strata - Tree, 3.01-6m, Very sparse. *Species includes - Eucalyptus similis, Grevillea pteridifolia
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Very dark greyish brown (10YR3/2-Moist); Brown (10YR5/3-Dry); , 7.5YR58, 0-2% , 0-5mm, 
	Distinct; , 0-2% , 0-5mm, Distinct; Fine sandy clay loam; Massive grade of structure; Dry; Strong 
	consistence; Common, fine (1-2mm) roots; Diffuse change to - 
	A3	0.1 - 0.2 m	Yellowish brown (10YR5/4-Moist); Very pale brown (10YR7/4-Dry); , 7.5YR58, 0-2% , 0-5mm, 
	Distinct; , 0-2% , 0-5mm, Distinct; Fine sandy clay loam; Massive grade of structure; Dry; Strong 
	consistence; Common, fine (1-2mm) roots; Gradual change to - 
	B1	0.2 - 0.3 m	Brownish yellow (10YR6/6-Moist); Yellow (10YR7/6-Dry); , 10YR68, 2-10% , 0-5mm, Distinct; , 2-
	10% , 0-5mm, Distinct; Fine sandy clay loam; Massive grade of structure; Dry; Strong 
	consistence; Common, fine (1-2mm) roots; 
	B1	0.3 - 0.4 m	Brownish yellow (10YR6/6-Moist); Yellow (10YR7/6-Dry); , 10YR68, 2-10% , 0-5mm, Distinct; , 2-
	10% , 0-5mm, Distinct; Fine sandy clay loam (Heavy); Massive grade of structure; Dry; Strong 
	consistence; Common, fine (1-2mm) roots; Diffuse change to - 
	B2	0.4 - 0.6 m	Brownish yellow (10YR6/6-Moist); Very pale brown (10YR7/4-Dry); , 7.5YR58, 20-50% , 5-15mm, 
	Faint; , 20-50% , 5-15mm, Faint; Sandy light clay; Massive grade of structure; Dry; Strong 
	consistence; Few (2 - 10 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Common, fine (1-2mm) 
	roots; Clear change to - 
	BC	0.6 - 0.7 m	Yellowish brown (10YR5/4-Moist); , 2.5YR36, 20-50% , 5-15mm, Distinct; , 20-50% , 5-15mm, 
	Distinct; Sandy medium clay; Massive grade of structure; Dry; Strong consistence; Very many 
	(50 - 100 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Common, fine (1-2mm) roots; Clear 
	change to - 
	C1	0.7 - 0.9 m	Dark red (2.5YR3/6-Moist); , 7.5YR58, 20-50% , 15-30mm, Prominent; , 5Y71, 20-50% , 15-
	30mm, Prominent; Sandy medium clay; Massive grade of structure; Dry; Very strong 
	consistence; 2-10%, coarse gravelly, 20-60mm, rounded, Quartz, coarse fragments; Very many 
	(50 - 100 %), Ferruginous, Coarse (6 - 20 mm), Nodules; 
	C1	0.9 - 1.2 m	Dark red (2.5YR3/6-Moist); , 7.5YR58, 20-50% , 15-30mm, Prominent; , 5Y71, 20-50% , 15-
	30mm, Prominent; Sandy medium clay; Massive grade of structure; Dry; Very strong 
	consistence; 2-10%, coarse gravelly, 20-60mm, rounded, Quartz, coarse fragments; Very many 
	(50 - 100 %), Ferruginous, Coarse (6 - 20 mm), Nodules; 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T228	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	C1	1.2 - 1.5 m	Dark red (2.5YR3/6-Moist); , 7.5YR58, 20-50% , 15-30mm, Prominent; , 5Y71, 20-50% , 15-
	30mm, Prominent; Sandy medium clay; Massive grade of structure; Dry; Very strong 
	consistence; 2-10%, coarse gravelly, 20-60mm, rounded, Quartz, coarse fragments; Many (20 - 
	50 %), Ferruginous, Coarse (6 - 20 mm), Nodules; 
	C1	1.5 - 1.8 m	Dark red (2.5YR3/6-Moist); , 7.5YR58, 20-50% , 15-30mm, Prominent; , 5Y71, 20-50% , 15-
	30mm, Prominent; Sandy medium clay; Massive grade of structure; Dry; Very strong 
	consistence; 2-10%, coarse gravelly, 20-60mm, rounded, Quartz, coarse fragments; Many (20 - 
	50 %), Ferruginous, Coarse (6 - 20 mm), Nodules; 
	C1	1.8 - 2.1 m	Dark red (2.5YR3/6-Moist); , 7.5YR58, 20-50% , 15-30mm, Prominent; , 5Y71, 20-50% , 15-
	30mm, Prominent; Sandy medium clay; Massive grade of structure; Dry; Very strong 
	consistence; 2-10%, coarse gravelly, 20-60mm, rounded, Quartz, coarse fragments; Many (20 - 
	50 %), Ferruginous, Coarse (6 - 20 mm), Nodules; 
	C1	2.1 - 2.4 m	Dark red (2.5YR3/6-Moist); , 7.5YR58, 20-50% , 15-30mm, Prominent; , 5Y71, 20-50% , 15-
	30mm, Prominent; Sandy medium clay; Massive grade of structure; Dry; Very strong 
	consistence; 2-10%, coarse gravelly, 20-60mm, rounded, Quartz, coarse fragments; Many (20 - 
	50 %), Ferruginous, Coarse (6 - 20 mm), Nodules; 
	C1	2.4 - 2.5 m	Dark red (2.5YR3/6-Moist); , 7.5YR58, 20-50% , 15-30mm, Prominent; , 5Y71, 20-50% , 15-
	30mm, Prominent; Sandy medium clay; Massive grade of structure; Dry; Very strong 
	consistence; 2-10%, coarse gravelly, 20-60mm, rounded, Quartz, coarse fragments; Many (20 - 
	50 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Diffuse change to - 
	C2	2.5 - 2.7 m	Light grey (10YR7/1-Moist); , 7.5YR56, 20-50% , 15-30mm, Prominent; , 2.5YR36, 20-50% , 15-
	30mm, Prominent; Sandy light clay; Massive grade of structure; Dry; Very strong consistence; 
	20-50%, cobbly, 60-200mm, rounded, Quartz, coarse fragments; 
	C2	2.7 - 3 m	Light grey (10YR7/1-Moist); , 7.5YR56, 20-50% , 15-30mm, Prominent; , 2.5YR36, 20-50% , 15-
	30mm, Prominent; Sandy light clay; Massive grade of structure; Dry; Very strong consistence; 
	20-50%, cobbly, 60-200mm, rounded, Quartz, coarse fragments; 
	C2	3 - 3.3 m	Light grey (10YR7/1-Moist); , 7.5YR56, 20-50% , 15-30mm, Prominent; , 2.5YR36, 20-50% , 15-
	30mm, Prominent; Sandy medium clay; Massive grade of structure; Dry; Very strong 
	consistence; 2-10%, coarse gravelly, 20-60mm, rounded, Quartz, coarse fragments; 
	C2	3.3 - 3.46 m	Light grey (10YR7/1-Moist); , 7.5YR56, 20-50% , 15-30mm, Prominent; , 2.5YR36, 20-50% , 15-
	30mm, Prominent; Sandy medium clay; Massive grade of structure; Dry; Very strong 
	consistence; 0-2%, medium gravelly, 6-20mm, rounded, Quartz, coarse fragments; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Regional
	Project Code:	REG	Site ID:	T228	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.5A	 0.024A	 0.41H	 0.89	 0.06	 0.16	 0.25F	 2.06A	 1.8F	7.77
	0.1 - 0.2	5.5A	 0.023A
	0.2 - 0.3	5.5A	 0.021A	<0.02H	 1.28	 0.04	 0.3	 0.4F	 2.45A	 2F	12.24
	0.3 - 0.4	5.3A	 0.032A
	0.4 - 0.6	5.9A	 0.021A	<0.02H	 1.58	 0.04	 0.3	 0.36F	 2.81A	 2.3F	10.68
	0.6 - 0.7	6.1A	 0.019A
	0.7 - 0.9	5.7A	 0.018A	<0.02H	 2.12	 0.04	 0.4	 0.19F	 3.38A	 2.8F	11.83
	0.9 - 1.2	5.9A	 0.021A
	1.2 - 1.5	6A	 0.024A
	1.5 - 1.8	6A	 0.029A
	1.8 - 2.1	5.8A	 0.021A
	2.1 - 2.4	5.9A	 0.028A
	2.4 - 2.5	6A	 0.026A
	2.5 - 2.7	5.6A	 0.029A
	2.7 - 3	5.2A	 0.028A
	3 - 3.3	5.2A	 0.035A
	3.3 - 3.46	5.8A	 0.023A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.49D	 8B	 0.007A	 0.041A	 0.04A	 2	 33A	 40	 8	 19
	0.1 - 0.2	 0.34D	 6B	 0.028A	 2	 30A	 39	 8	 23
	0.2 - 0.3	 0.2D	 6B	 0.005A	 0.014A	 0.05A	 1	 29A	 37	 7	 27
	0.3 - 0.4	 4	 30A	 35	 7	 29
	0.4 - 0.6	 9	 31A	 31	 6	 32
	0.6 - 0.7	 61	 34A	 29	 6	 30
	0.7 - 0.9	 0.009A	 0.06A	 74	 34A	 27	 6	 33
	0.9 - 1.2	 58	 51A	 22	 6	 21
	1.2 - 1.5	 50	 34A	 26	 8	 22
	1.5 - 1.8	 51	 28A	 25	 8	 39
	1.8 - 2.1	 49	 29A	 23	 7	 41
	2.1 - 2.4	 45	 33A	 19	 6	 42
	2.4 - 2.5	 49	 36A	 19	 6	 39
	2.5 - 2.7	 47	 35A	 16	 5	 43
	2.7 - 3	 23	 42A	 14	 5	 39
	3 - 3.3	 7	 45A	 16	 6	 33
	3.3 - 3.46	 3	 43A	 14	 6	 38
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.6
	0.6 - 0.7
	0.7 - 0.9

	Project Name:	Regional
	Project Code:	REG	Site ID:	T228	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2.1
	2.1 - 2.4
	2.4 - 2.5
	2.5 - 2.7
	2.7 - 3
	3 - 3.3
	3.3 - 3.46

	Project Name:	Regional
	Project Code:	REG	Site ID:	T228	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)