Project Name:	Regional
	Project Code:	REG	Site ID:	T236	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.G. Murtha	Locality:	On road to TV stations 7.3KM from Flinders Highway:
	Date Desc.:	18/01/78	Elevation:	 442 metres
	Map Ref.:	Sheet No. : 8259   1:100000	Rainfall:	1200
	Northing/Long.:	146.791666666667	Runoff:	No Data
	Easting/Lat.:	-19.35	Drainage:	No Data
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	C-Pv	Substrate Material:	Existing vertical exposure, 0.8 m 
	deep,Andesite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Mountains
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Chromosol     	Principal Profile Form:	Dr2.12
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus drepanophylla, Eucalyptus polycarpa
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Very dark brown (10YR2/2-Moist); ; Loam; Moderate grade of structure, 5-10 mm, Angular blocky; 
	Moist; Weak consistence; 2-10%, coarse gravelly, 20-60mm, Gravel, coarse fragments; 
	Abundant
	B1	0.1 - 0.2 m	Reddish brown (5YR4/4-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, Angular 
	blocky; Moist; Very firm consistence; 2-10%, coarse gravelly, 20-60mm, Gravel, coarse 
	fragments; CommonClear change to - 
	B2	0.2 - 0.3 m	Yellowish red (5YR4/6-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, Angular 
	blocky; Moist; Very firm consistence; 2-10%, coarse gravelly, 20-60mm, Gravel, coarse 
	fragments; Few (2 - 10 %), Unidentified, Fine (0 - 2 mm), Nodules; 
	B2	0.3 - 0.45 m	Yellowish red (5YR4/6-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, Angular 
	blocky; Moist; Very firm consistence; 
	BC	0.45 - 0.6 m	Reddish brown (5YR4/4-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, Angular 
	blocky; Moist; Very firm consistence; 20-50%, fine gravelly, 2-6mm, Andesite, coarse fragments;
	 Gradual change to - 
	BC	0.6 - 0.8 m	Reddish brown (5YR4/4-Moist); ; Medium clay; 50-90%, large Boulders, >2m, Andesite, coarse 
	fragments; 
	Morphological Notes
	Observation Notes
	WEATHERED PM STARTING AT 40CM:60-80CM (.5CM-4CM) ANDESITE GV SET IN MATRIX OF rB MC:                                    
	Site Notes
	MT STUART

	Project Name:	Regional
	Project Code:	REG	Site ID:	T236	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.1A	 0.08A	 10.8H	 5.02	 0.6	 0.09	 0.5F	 15.2A	 17F	0.59
	0.1 - 0.2	5.7A	<0.05A
	0.2 - 0.3	5.9A	<0.05A	 2.13H	 6.65	 0.11	 0.17	 0.4F	 16.2A	 9.5F	1.05
	0.3 - 0.45	<0.05A	 2.43H	 7.66	 0.08	 0.24	 0.3F	 17.5A	 10.7F	1.37
	0.45 - 0.6	6.5A	<0.05A
	0.6 - 0.8	6.7A	<0.05A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 3.05D	 0.16A	 6	 9A	 23	 24	 40
	0.1 - 0.2	 1.94D	 5A	 0.113A	 4	 3A	 9	 20	 68
	 4B
	0.2 - 0.3	 1.19D	 0.03A	 4	 2A	 5	 18	 76
	0.3 - 0.45	 12	 3A	 7	 22	 68
	0.45 - 0.6	 24	 4A	 11	 30	 55
	0.6 - 0.8	 52	 6A	 12	 30	 51
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.45
	0.45 - 0.6
	0.6 - 0.8

	Project Name:	Regional
	Project Code:	REG	Site ID:	T236	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)