Project Name:	Regional
	Project Code:	REG	Site ID:	T242	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.F. Isbell	Locality:	On road 1KM south of Stager Road 2.6KM from 
	highway:
	Date Desc.:	20/08/75	Elevation:	 40 metres
	Map Ref.:	Sheet No. : 8063   1:100000	Rainfall:	410
	Northing/Long.:	145.891666666667	Runoff:	Moderately rapid
	Easting/Lat.:	-17.3666666666667	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Pgm	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Upper-slope	Relief:	40 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	0 % 	Aspect:	23 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Dystrophic Red Kandosol     	Principal Profile Form:	Gn3.14
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.1 m	Brown (7.5YR4/3-Moist); ; Sandy clay loam (Light); Moderate grade of structure, 2-5 mm, 
	Granular; Weak consistence; 0-2%, Gravel, coarse fragments; Abundant
	0.1 - 0.2 m	Strong brown (7.5YR4/5-Moist); ; Sandy clay loam (Light); Moderate grade of structure, 2-5 mm, 
	Granular; Weak consistence; ManyClear change to - 
	A2	0.2 - 0.3 m	Yellowish red (5YR5/6-Moist); ; Sandy clay loam; Weak grade of structure, 2-5 mm, Granular; 
	Weak consistence; CommonGradual change to - 
	A2/B1	0.3 - 0.45 m	Yellowish red (5YR5/6-Moist); ; Sandy clay loam; Weak grade of structure, 5-10 mm, Angular 
	blocky; Weak consistence; 0-2%, Gravel, coarse fragments; FewDiffuse change to - 
	B1	0.45 - 0.6 m	Yellowish red (5YR4/8-Moist); ; Sandy medium clay (Light); Massive grade of structure; Weak 
	consistence; FewDiffuse change to - 
	B1	0.6 - 0.9 m	Yellowish red (5YR4/8-Moist); ; Sandy medium clay; Massive grade of structure; Firm 
	consistence; Diffuse change to - 
	B21	0.9 - 1.2 m	Red (2.5YR4/7-Moist); ; Sandy medium clay; Weak grade of structure, 10-20 mm, Angular 
	blocky; Very firm consistence; 0-2%, Gravel, coarse fragments; Diffuse change to - 
	B22	1.2 - 1.5 m	Red (2.5YR4/7-Moist); ; Medium clay; Weak grade of structure, 10-20 mm, Angular blocky; 
	Smooth-ped fabric; Very firm consistence; FewDiffuse change to - 
	B22	1.5 - 1.8 m	Red (2.5YR4/7-Moist); ; Medium clay; Weak grade of structure, 10-20 mm, Angular blocky; 
	Smooth-ped fabric; Very firm consistence; Diffuse change to - 
	B3	1.8 - 2.1 m	Red (2.5YR4/7-Moist); ; Sandy medium clay; Weak grade of structure, 10-20 mm, Angular 
	blocky; Firm consistence; Diffuse change to - 
	BC	2.1 - 2.4 m	Red (2.5YR4/7-Moist); ; Sandy medium clay; Weak grade of structure, 10-20 mm, Angular 
	blocky; Weak consistence; Diffuse change to - 
	BC	2.4 - 2.7 m	Red (2.5YR4/7-Moist); ; Sandy medium clay; Massive grade of structure; Weak consistence; 
	Diffuse change to - 
	BC	2.7 - 3 m	Red (2.5YR4/7-Moist); ; Sandy medium clay (Light); Massive grade of structure; Weak 
	consistence; 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T242	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Morphological Notes
	Observation Notes
	0-20CM MANY WORM CASTS:180-270CM LESS AGGREGATED + MORE W`D ROCK FRAGMENTS:270-300 MUCH ROCK 
	FABRIC VISIBLE:            
	Site Notes
	BABINDA CK.

	Project Name:	Regional
	Project Code:	REG	Site ID:	T242	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5A	 0.48B	 0.45	 0.09	 0.1	 1.41F	 2.5F
	0.1 - 0.2	4.9A
	0.2 - 0.3	4.8A	 0.08B	 0.13	 0.09	 0.06	 1.82F	 2.2F
	0.3 - 0.45	4.8A
	0.45 - 0.6	4.8A	 0.08B	 0.09	 0.02	 0.03	 1.57F	 1.8F
	0.6 - 0.9	4.9A	 0.08B	 0.05	 0.01	 0.03	 1.68F	 1.9F
	0.9 - 1.2	4.9A	 0.08B	 0.09	 0.005	 0.02	 2.23F	 2.4F
	1.2 - 1.5	4.9A
	1.5 - 1.8	4.9A	 0.08B	 0.13	 0.005	 0.03	 3.05F	 3.3F
	1.8 - 2.1	4.9A
	2.1 - 2.4	4.9A
	2.4 - 2.7	4.8A
	2.7 - 3	4.8A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.47D	 11B	 0.02A	 0.128A	 0.24A	 14	 57A	 8	 10	 25
	0.1 - 0.2	 1.11D	 8B	 0.105A
	0.2 - 0.3	 0.97D	 4B	 0.012A	 0.09A	 0.24A	 16	 51A	 8	 11	 30
	0.3 - 0.45	 0.62D	 0.06A
	0.45 - 0.6	 0.45D	 1B	 0.009A	 0.038A	 0.91A	 14	 42A	 10	 13	 35
	0.6 - 0.9	 0.31D	 14	 37A	 11	 16	 33
	0.9 - 1.2	 0.007A	 1.1A	 10	 32A	 12	 25	 31
	1.2 - 1.5
	1.5 - 1.8	 0.008A	 1.36A	 12	 32A	 15	 28	 25
	1.8 - 2.1
	2.1 - 2.4
	2.4 - 2.7
	2.7 - 3
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.45
	0.45 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2.1
	2.1 - 2.4
	2.4 - 2.7
	2.7 - 3

	Project Name:	Regional
	Project Code:	REG	Site ID:	T242	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_FE	Total element - Fe(%) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)