Project Name:	Regional
	Project Code:	REG	Site ID:	T250	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.F. Isbell	Locality:	Road cut 28M SSE from track SE along power 
	line:Millaa Millaa/Tully Geoge Road ~ 27KM SE of 
	Millaa Millaa:
	Date Desc.:	03/07/76	Elevation:	 640 metres
	Map Ref.:	Sheet No. : 8062   1:100000	Rainfall:	2540
	Northing/Long.:	145.6625	Runoff:	Moderately rapid
	Easting/Lat.:	-17.6833333333333	Drainage:	Moderately well drained
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Pgb	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Hills
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Moderately inclined
	Slope:	12.3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Mesotrophic Red Dermosol     	Principal Profile Form:	Gn3.14
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (10YR3/3-Moist); ; Clay loam; Strong grade of structure, 5-10 mm, Cast; Moist; Weak 
	consistence; AbundantClear change to - 
	A2	0.1 - 0.2 m	Brown (7.5YR4/4-Moist); ; Light clay; Strong grade of structure, 5-10 mm, Granular; Moist; Weak 
	consistence; ManyClear change to - 
	B1	0.2 - 0.3 m	Yellowish red (5YR4/8-Moist); ; Light medium clay; Moderate grade of structure, 10-20 mm, 
	Angular blocky; Moist; Very firm consistence; ManyGradual change to - 
	B1	0.3 - 0.45 m	Red (2.5YR4/8-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, Angular blocky; 
	Smooth-ped fabric; Moist; Very firm consistence; FewGradual change to - 
	B2	0.45 - 0.6 m	Red (2.5YR4/7-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, Angular blocky; 
	Smooth-ped fabric; Moist; Firm consistence; FewGradual change to - 
	B2	0.6 - 0.9 m	Red (2.5YR4/7-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, Angular blocky; 
	Smooth-ped fabric; Moist; Firm consistence; FewGradual change to - 
	B3	0.9 - 1.2 m	Red (2.5YR4/6-Moist); ; Light medium clay; Weak grade of structure, 10-20 mm, Angular blocky; 
	Smooth-ped fabric; Moist; Firm consistence; FewGradual change to - 
	B3	1.2 - 1.5 m	Red (2.5YR4/8-Moist); ; Light clay; Weak grade of structure, 10-20 mm, Angular blocky; Smooth-
	ped fabric; Moist; Weak consistence; Few
	B3	1.5 - 1.8 m	Red (2.5YR4/8-Moist); ; Light clay; Weak grade of structure, 10-20 mm, Angular blocky; Smooth-
	ped fabric; Moist; Weak consistence; Few
	B3	1.8 - 2.1 m	Red (2.5YR4/7-Moist); , 7.5YR57, 0-2% , 15-30mm; , 0-2% , 15-30mm; Light clay; Weak grade of 
	structure, 20-50 mm, Angular blocky; Common (1-5 per 100mm2) Fine (1-2mm) macropores, 
	Moist; Very firm consistence; Gradual change to - 
	2.1 - 2.4 m	Red (2.5YR4/7-Moist); , 7.5YR57, 0-2% , 15-30mm; , 0-2% , 15-30mm; Light clay; Weak grade of 
	structure, 20-50 mm, Angular blocky; Common (1-5 per 100mm2) Fine (1-2mm) macropores, 
	Very firm consistence; 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T250	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	2.4 - 2.7 m	Red (2.5YR4/7-Moist); , 7.5YR57, 0-2% , 15-30mm; , 0-2% , 15-30mm; Light clay; Weak grade of 
	structure, 20-50 mm, Angular blocky; Common (1-5 per 100mm2) Fine (1-2mm) macropores, 
	Very firm consistence; 
	2.7 - 3 m	Red (2.5YR4/7-Moist); , 7.5YR57, 0-2% , 15-30mm; , 0-2% , 15-30mm; Light clay; Weak grade of 
	structure, 20-50 mm, Angular blocky; Common (1-5 per 100mm2) Fine (1-2mm) macropores, 
	Very firm consistence; Gradual change to - 
	3 - 3.3 m	Red (2.5YR4/6-Moist); , 7.5YR57, 0-2% ; , 0-2% ; Clay loam; Weak consistence; 
	3.3 - 3.6 m	Red (2.5YR4/6-Moist); , 7.5YR57, 0-2% ; , 0-2% ; Clay loam; Weak consistence; 
	3.6 - 4 m	Red (2.5YR4/6-Moist); , 7.5YR57, 0-2% ; , 0-2% ; Clay loam; Weak consistence; 
	Morphological Notes
	Observation Notes
	60-400CM SMALL MICA FLAKES:180-400CM W`D FELSPAR GRADING FROM RARE TO FEW:300-400CM INCREASING ROCK
	 FABRIC:             
	Site Notes
	MAALAN

	Project Name:	Regional
	Project Code:	REG	Site ID:	T250	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.6A	 4.08B	 1.58	 0.34	 0.05
	0.1 - 0.2	5.6A
	0.2 - 0.3	5.6A	 2.12B	 0.9	 0.24
	0.3 - 0.45	5.6A
	0.45 - 0.6	5.6A	 2.12B	 0.94	 0.18	 0.04
	0.6 - 0.9	5.4A	 1.7B	 0.9	 0.18	 0.05
	0.9 - 1.2	5.2A	 0.56B	 0.6	 0.12	 0.1
	1.2 - 1.5	5.3A
	1.5 - 1.8	5.1A
	1.8 - 2.1	5A	 0.22B	 0.38	 0.11	 0.06
	2.1 - 2.4	5A
	2.4 - 2.7	5.1A
	2.7 - 3	5A
	3 - 3.3	5A
	3.3 - 3.6	5A
	3.6 - 4	5.1A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 2.54D	 5B	 0.197A	<2	 34A	 18	 13	 35
	0.1 - 0.2	 1.35D	 3B	 0.128A	<2	 27A	 19	 15	 39
	0.2 - 0.3	 0.76D	 1B	 0.075A	 0	 24A	 14	 14	 5
	0.3 - 0.45	 0.65D	 0.068A	 0	 16A	 14	 15	 54
	0.45 - 0.6	 0.41D	 1B	 0.053A	 0	 13A	 14	 13	 56
	0.6 - 0.9	 0.31D	 0	 15A	 17	 19	 49
	0.9 - 1.2	<2	 16A	 21	 22	 40
	1.2 - 1.5
	1.5 - 1.8	 2	 27A	 24	 20	 30
	1.8 - 2.1
	2.1 - 2.4
	2.4 - 2.7
	2.7 - 3
	3 - 3.3
	3.3 - 3.6
	3.6 - 4
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.45
	0.45 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2.1

	Project Name:	Regional
	Project Code:	REG	Site ID:	T250	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	2.1 - 2.4
	2.4 - 2.7
	2.7 - 3
	3 - 3.3
	3.3 - 3.6
	3.6 - 4

	Project Name:	Regional
	Project Code:	REG	Site ID:	T250	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_FE	Total element - Fe(%) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)