Project Name:	Regional
	Project Code:	REG	Site ID:	T256	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.J. Coventry	Locality:	120M east of Redlands plots:
	Date Desc.:	31/08/77	Elevation:	No Data
	Map Ref.:	Sheet No. : 8057   1:100000	Rainfall:	620
	Northing/Long.:	145.883333333333	Runoff:	No Data
	Easting/Lat.:	-20.225	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Tf	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Red Kandosol     	Principal Profile Form:	Gn2.11
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus drepanophylla
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.05 m	Dark reddish brown (2.5YR3/4-Moist); Red (2.5YR4/5-Dry); ; Sandy loam (Heavy); Massive grade 
	of structure; Earthy fabric; Dry; Firm consistence; Common, fine (1-2mm) roots; Diffuse change 
	to - 
	A12	0.05 - 0.1 m	Dark red (2.5YR3/6-Moist); Red (2.5YR4/6-Dry); ; Sandy loam (Heavy); Massive grade of structure;
	 Earthy fabric; Dry; Very firm consistence; Few, fine (1-2mm) roots; Diffuse change to - 
	A3	0.1 - 0.2 m	Dark red (10R3/6-Moist); Dark red (2.5YR3/6-Dry); ; Sandy clay loam; Massive grade of structure; 
	Earthy fabric; Dry; Very firm consistence; Few, fine (1-2mm) roots; Diffuse change to - 
	B11	0.2 - 0.3 m	Dark red (10R3/6-Moist); Red (10R4/6-Dry); ; Sandy medium clay (Light); Massive grade of 
	structure; Earthy fabric; Dry; Very firm consistence; Few, fine (1-2mm) roots; Diffuse change to - 
	B12	0.3 - 0.4 m	Dark red (10R3/6-Moist); Red (10R4/6-Dry); ; Sandy medium clay; Massive grade of structure; 
	Earthy fabric; Dry; Very firm consistence; Diffuse change to - 
	B21	0.4 - 0.6 m	Red (10R4/6-Moist); Red (10R4/8-Dry); ; Light clay; Massive grade of structure; Earthy fabric; Dry;
	 Strong consistence; Diffuse change to - 
	B22	0.6 - 0.9 m	Red (10R4/6-Moist); Red (10R4/8-Dry); ; Light clay; Massive grade of structure; Earthy fabric; Dry;
	 Strong consistence; Few (2 - 10 %), Argillaceous, Coarse (6 - 20 mm), Nodules; Diffuse 
	change to - 
	B23	0.9 - 1.2 m	Red (10R4/6-Moist); Red (10R4/8-Dry); ; Light clay; Massive grade of structure; Earthy fabric; Dry;
	 Strong consistence; Few (2 - 10 %), Argillaceous, Coarse (6 - 20 mm), Nodules; 
	Morphological Notes
	Observation Notes
	Site Notes
	REDLANDS

	Project Name:	Regional
	Project Code:	REG	Site ID:	T256	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.3A	<0.05A	 2.24B	 1.05	 0.29	 0.03	 0.08F	 3.7F
	0.05 - 0.1	6.4A	<0.05A	 1.76B	 0.85	 0.23	 0.02	 0.08F	 2.9F
	0.1 - 0.2
	0.2 - 0.3	6.33A	<0.05A	 1.44B	 0.73	 0.18	 0.02	 0.1F	 2.5F
	0.3 - 0.4
	0.4 - 0.6	6.2A	<0.05A	 1.52B	 1.13	 0.18	 0.02	 0.06F	 2.9F
	0.6 - 0.9
	0.9 - 1.2	6.4A	<0.05A	 1.04B	 1.96	 0.11	 0.02	 0.06F	 3.2F
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0.62D	 0.036A	 0	 40A	 37	 9	 15
	0.05 - 0.1	 0.33D	 0.045A	 0	 40A	 36	 7	 17
	0.1 - 0.2	 1	 39A	 34	 7	 21
	0.2 - 0.3	 0.22D	 0.018A	 1	 42A	 29	 5	 24
	0.3 - 0.4	 1	 36A	 25	 5	 34
	0.4 - 0.6	 0.12D	 1	 31A	 23	 6	 41
	0.6 - 0.9	 1	 26A	 20	 5	 48
	0.9 - 1.2	 0.05D	 1	 21A	 22	 11	 47
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.6
	0.6 - 0.9
	0.9 - 1.2

	Project Name:	Regional
	Project Code:	REG	Site ID:	T256	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9H1	Phosphate retention
	MIN_EC	Exchange Capacity - Minerology
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)
	XRD_C_Hm	Hematite - X-Ray Diffraction
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_K2O	K2O - X-Ray Diffraction or Clay Fraction (air dry)
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction