Project Name:	Regional
	Project Code:	REG	Site ID:	T262	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.G. Murtha	Locality:	In quarry 7.5KM from highway on Mission Beach 
	Road:
	Date Desc.:	02/06/78	Elevation:	 40 metres
	Map Ref.:	Sheet No. : 8162   1:100000	Rainfall:	4000
	Northing/Long.:	146	Runoff:	Moderately rapid
	Easting/Lat.:	-17.9166666666667	Drainage:	Well drained
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  QA	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Alluvial fan
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Fan	Slope Category:	Gently inclined
	Slope:	5 % 	Aspect:	20 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melacic Dystrophic Red Kandosol     	Principal Profile Form:	Gn2.14
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - None recorded
	Tall Strata - Tree, 20.01-35m, Sparse. *Species includes - Acacia mangium, Eucalyptus pellita
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark reddish brown (5YR3/2-Moist); ; Sandy loam; Weak grade of structure, 5-10 mm, Cast; 
	Moist; Weak consistence; Abundant, fine (1-2mm) roots; 
	A1	0.1 - 0.2 m	Dark reddish brown (5YR3/2-Moist); ; Sandy loam; Weak grade of structure, 5-10 mm, 
	Subangular blocky; Moist; Weak consistence; Many, fine (1-2mm) roots; Gradual change to - 
	A2	0.2 - 0.3 m	Dark reddish brown (5YR3/4-Moist); ; Sandy loam (Heavy); Massive grade of structure; Moist; 
	Weak consistence; Common, fine (1-2mm) roots; Gradual change to - 
	B1	0.3 - 0.45 m	Dark red (2.5YR3/6-Moist); ; Sandy clay loam (Light); Massive grade of structure; Earthy fabric; 
	Moist; Weak consistence; 
	B2	0.45 - 0.6 m	Dark red (2.5YR3/6-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; Moist; 
	Weak consistence; 
	B2	0.6 - 0.9 m	Dark red (2.5YR3/6-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; Moist; 
	Weak consistence; 
	B2	0.9 - 1.2 m	Dark red (2.5YR3/6-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; Moist; 
	Weak consistence; 
	1.2 - 1.5 m	Dark red (2.5YR3/8-Moist); ; Sandy clay loam (Heavy); Massive grade of structure; Earthy fabric; 
	Weak consistence; 
	1.5 - 1.8 m	Dark red (2.5YR3/8-Moist); ; Sandy clay loam (Heavy); Massive grade of structure; Earthy fabric; 
	Weak consistence; 
	1.8 - 2.1 m	Dark red (2.5YR3/8-Moist); ; Sandy clay loam (Heavy); Massive grade of structure; Earthy fabric; 
	Weak consistence; 
	Morphological Notes
	Observation Notes
	IN QUARRY FACE THE SOIL CONTINUES TO 450CM WITH LITTLE CHANGE                                                           
	Site Notes

	Project Name:	Regional
	Project Code:	REG	Site ID:	T262	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)

	Project Name:	Regional
	Project Code:	REG	Site ID:	T262	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.2A	 0.184A	 0.71H	 0.41	 0.08	 0.01	 1.7F	 2.4A	 2.9F	0.42
	0.1 - 0.2	5.1A	 0.13A	 0.31H	 0.11	 0.02	 0.01	 1.5F	 2A	 2F	0.50
	0.2 - 0.3	5.1A	 0.101A
	0.3 - 0.45	5.2A	 0.187A	 0.13H	<0.01	<0.01	<0.01	 0.48F	 1.7A	 0.6F
	0.45 - 0.6	5.1A	 0.113A	 0.13H	 0.04	<0.01	<0.01	 0.24F	 1.4A	 0.4F
	0.6 - 0.9	5.1A	 0.154A
	0.9 - 1.2	4.8A	 0.11A	 0.08H	 0.1	<0.01	<0.01	 0.2F	 1.5A	 0.4F
	1.2 - 1.5	4.8A	 0.113A
	1.5 - 1.8	5A	 0.083A
	1.8 - 2.1	4.9A	 0.065A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 3.4D	 9B	 0.022A	 0.13A	 0.14A	 0	 46A	 12	 7	 36
	0.1 - 0.2	 1.88D	 5B	 0.1A	 10	 50A	 9	 6	 35
	0.2 - 0.3	 1.04D	 2B	 0.1A	 8	 44A	 10	 8	 38
	0.3 - 0.45	 0.71D	 3B	 0.81A	 5	 39A	 9	 8	 44
	0.45 - 0.6	 0.3D	 3B	 0.47A	 8	 39A	 9	 4	 47
	0.6 - 0.9
	0.9 - 1.2	 0.15D	 1B	 0.011A	 0.02A	 0.08A	 0	 30A	 11	 7	 52
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2.1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.45
	0.45 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2.1

	Project Name:	Regional
	Project Code:	REG	Site ID:	T262	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)