Project Name:	Regional
	Project Code:	REG	Site ID:	T263	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.F. Isbell	Locality:	Charappa Creek Forestry Road south west of 
	Johnstone River crossing:3.5KM south west of Mena 
	Creek turnoff:
	Date Desc.:	07/08/78	Elevation:	 600 metres
	Map Ref.:	Sheet No. : 8062   1:100000	Rainfall:	3000
	Northing/Long.:	145.7	Runoff:	Rapid
	Easting/Lat.:	-17.6958333333333	Drainage:	No Data
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Pgb	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Hills
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Steep
	Slope:	21.3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Magnesic Red Dermosol     	Principal Profile Form:	Gn3.14
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:	2-10%, , , Granite
	Profile Morphology
	A1	0 - 0.1 m	Dark reddish brown (5YR3/4-Moist); ; Sandy clay loam (Heavy); Moderate grade of structure, 5-10 
	mm, Cast; Weak consistence; 2-10%, Granite, coarse fragments; Many, medium (2-5mm) roots; 
	A2	0.1 - 0.2 m	Yellowish red (5YR4/8-Moist); ; Clay loam; Strong grade of structure, 5-10 mm, Granular; Weak 
	consistence; Few, medium (2-5mm) roots; Clear change to - 
	B1	0.2 - 0.3 m	Yellowish red (5YR4/6-Moist); ; Clay loam; Moderate grade of structure, 50-100 mm, Subangular 
	blocky; Firm consistence; FewGradual change to - 
	B21	0.3 - 0.45 m	Yellowish red (5YR4/6-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, Subangular 
	blocky; Smooth-ped fabric; Firm consistence; 0-2%, Gravel, coarse fragments; Common cutans,
	 10-50% of ped faces or walls coated, distinct; Gradual change to - 
	0.45 - 0.6 m	Yellowish red (5YR4/6-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, Subangular 
	blocky; Smooth-ped fabric; Firm consistence; 0-2%, Gravel, coarse fragments; Common cutans,
	 10-50% of ped faces or walls coated, distinct; 
	B22	0.6 - 0.9 m	Dark red (2.5YR3/6-Moist); ; Light medium clay; Moderate grade of structure, 10-20 mm, 
	Subangular blocky; Smooth-ped fabric; Weak consistence; 0-2%, Quartz, coarse fragments; 
	Common cutans, 10-50% of ped faces or walls coated, distinct; Gradual change to - 
	B23	0.9 - 1.2 m	Red (2.5YR4/6-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, Subangular 
	blocky; Smooth-ped fabric; Weak consistence; Common cutans, 10-50% of ped faces or walls 
	coated, distinct; 
	B24	1.2 - 1.5 m	Red (2.5YR4/7-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, Subangular 
	blocky; Smooth-ped fabric; Weak consistence; Common cutans, 10-50% of ped faces or walls 
	coated, distinct; 
	B31	1.5 - 1.8 m	Red (2.5YR4/7-Moist); , 10YR68, 2-10% , 5-15mm, Faint; , 2-10% , 5-15mm, Faint; Light clay; 
	Moderate grade of structure, 10-20 mm, Subangular blocky; Smooth-ped fabric; Weak 
	consistence; 0-2%, Gravel, coarse fragments; Common cutans, 10-50% of ped faces or walls 
	coated, distinct; 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T263	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B32	1.8 - 2 m	Red (2.5YR4/7-Moist); , 10YR68, 10-20% , 15-30mm, Distinct; , 10-20% , 15-30mm, Distinct; 
	Light clay; Smooth-ped fabric; Weak consistence; 0-2%, Gravel, coarse fragments; Common 
	cutans, 10-50% of ped faces or walls coated, distinct; 
	Morphological Notes
	Observation Notes
	150-200CM OCCASIONAL W'D ROCK FRAGMENT:                                                                                 
	Site Notes
	STH JOHNSTONE

	Project Name:	Regional
	Project Code:	REG	Site ID:	T263	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.9A	 0.086A	 0.76B	 1.08	 0.17	 0.05	 2.32F	 3.6A	 4.4F	1.39
	0.1 - 0.2	5.1A	 0.044A	 2.3A
	0.2 - 0.3	5.1A	 0.029A	 0.04B	 0.66	 0.09	 0.02	 1.16F	 2.69A	 2F	0.74
	0.3 - 0.45	5.1A	 0.029A
	0.45 - 0.6	5.1A	 0.029A
	0.6 - 0.9	5.2A	 0.02A	 0.01B	 0.16	 0.13	 0.02	 1.64F	 2.8A	 2F	0.71
	0.9 - 1.2	5.1A	 0.014A
	1.2 - 1.5	5A	 0.017A	 0.01B	 0.27	 0.09	 0.02	 6.96F	 8.67A	 7.4F	0.23
	1.5 - 1.8	5.1A	 0.017A
	1.8 - 2	5A	 0.017A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 4.53D	 44B	 0.222A	 30	 48A	 11	 7	 34
	0.1 - 0.2	 2.15D	 1B	 0.105A	 30	 44A	 12	 10	 34
	0.2 - 0.3	 1.48D	<1B	 16	 34A	 13	 8	 45
	0.3 - 0.45	 1.26D	 16	 31A	 12	 8	 48
	0.45 - 0.6	 1.1D	 1B	 14	 32A	 12	 9	 47
	0.6 - 0.9	 0.62D	 16	 32A	 13	 11	 44
	0.9 - 1.2	 22	 30A	 14	 19	 36
	1.2 - 1.5	 20	 27A	 18	 24	 31
	1.5 - 1.8	 25	 32A	 18	 22	 28
	1.8 - 2	 25	 29A	 20	 23	 28
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.45
	0.45 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2

	Project Name:	Regional
	Project Code:	REG	Site ID:	T263	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)