Project Name:	Regional
	Project Code:	REG	Site ID:	T29	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.F. Isbell	Locality:	Manton paddock approx. 5 chain's north east of stock 
	yards:
	Date Desc.:	10/09/64	Elevation:	No Data
	Map Ref.:	Sheet No. : 8258   1:100000	Rainfall:	870
	Northing/Long.:	146.820833333333	Runoff:	No Data
	Easting/Lat.:	-19.65	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qa	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Mottled-Subnatric Grey Sodosol     	Principal Profile Form:	Dy3.43
	ASC Confidence:	Great Soil Group:	Solodized solonetz
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Heteropogon contortus, Stylosanthes humilis
	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus drepanophylla, Eucalyptus alba, Eucalyptus papuana
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.06 m	Very dark greyish brown (10YR3/2-Moist); Grey (10YR5/1-Dry); , 0-0% ; , 0-0% ; Sandy loam 
	(Light); Massive grade of structure; Dry; Very firm consistence; Clear change to - 
	A21	0.06 - 0.2 m	Yellowish brown (10YR5/4-Moist); Very pale brown (10YR7/3-Dry); , 0-0% ; , 0-0% ; Sandy loam 
	(Light); Massive grade of structure; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; 
	Very firm consistence; Gradual change to - 
	A22	0.2 - 0.38 m	Yellowish brown (10YR5/4-Moist); Very pale brown (10YR7/3-Dry); , 10YR56, 2-10% , 0-5mm, 
	Distinct; , 2-10% , 0-5mm, Distinct; Sandy loam (Heavy); Massive grade of structure; Common 
	(1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Strong consistence; 0-2%, fine gravelly, 2-
	6mm, Gravel, coarse fragments; Gradual change to - 
	A23	0.38 - 0.53 m	Yellowish brown (10YR5/4-Moist); Very pale brown (10YR7/3-Dry); , 10YR56, 2-10% , 0-5mm, 
	Distinct; , 2-10% , 0-5mm, Distinct; Sandy loam (Heavy); Massive grade of structure; Common 
	(1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Strong consistence; 2-10%, coarse gravelly, 
	20-60mm, rounded, Gravel, coarse fragments; Few (2 - 10 %), Ferruginous, Medium (2 -6 mm), 
	Nodules; Abrupt change to - 
	B21	0.53 - 0.69 m	Greyish brown (10YR5/2-Moist); , 10YR56, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, 
	Distinct; Sandy medium clay; Moderate grade of structure, 50-100 mm, Prismatic; Weak grade 
	of structure, 50-100 mm, Columnar; Dry; Rigid consistence; 0-2%, medium gravelly, 6-20mm, 
	Gravel, coarse fragments; Few (2 - 10 %), Ferromanganiferous, Medium (2 -6 mm), Nodules; 
	Gradual change to - 
	B22	0.69 - 0.84 m	Yellowish brown (10YR5/6-Moist); , 10YR52, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, 
	Distinct; Sandy medium clay; Weak grade of structure, 20-50 mm, Angular blocky; Dry; Rigid 
	consistence; Few (2 - 10 %), Ferromanganiferous, , Nodules; Gradual change to - 
	Bk	0.84 - 1.02 m	Yellowish brown (10YR5/6-Moist); , 10YR52, 2-10% , 5-15mm, Distinct; , 2-10% , 5-15mm, 
	Distinct; Sandy medium clay; Weak grade of structure, 20-50 mm, Angular blocky; Dry; Rigid 
	consistence; Few (2 - 10 %), Ferromanganiferous, , Nodules; Few (2 - 10 %), Calcareous, , 
	Nodules; Gradual change to - 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T29	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	C	1.02 - 1.17 m	Dark greyish brown (10YR4/2-Moist); ; Medium clay; Very firm consistence; 2-10%, fine gravelly, 
	2-6mm, Gravel, coarse fragments; Very few (0 - 2 %), Calcareous, , Concretions; Clear change 
	to - 
	D	1.17 - 1.32 m	Very dark grey (10YR3/1-Moist); , 10YR52; Medium clay; , Polyhedral; Very firm consistence; 0-
	2%, fine gravelly, 2-6mm, Sand, coarse fragments; Few (2 - 10 %), Calcareous, , Soft 
	segregations; 
	Morphological Notes
	Observation Notes
	SLIGHT DOMING OF COL'S IN B21:0-35CM SEPERATE DEPOSITIONAL LAYER:                                                       
	Site Notes
	LANDSDOWN

	Project Name:	Regional
	Project Code:	REG	Site ID:	T29	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06	5.6A	 0.029A	 2E	 0.7	 0.23	 0.05	 4.2F	 7C	 7.2F	0.71
	0.06 - 0.2	5.7A	<0.03A	 1.6E	 0.7	 0.12	 0.1	 2.3F	 5C	 4.8F	2.00
	0.2 - 0.38	6.1A	<0.03A
	0.38 - 0.53	6.6A	<0.03A	 2.2E	 1.5	 0.06	 0.3	 2F	 6C	 6.1F	5.00
	0.53 - 0.69	7.2A	 0.089A	 5.8E	 4.1	 0.13	 1.7	 1.6F	 13C	 13.3F	13.08
	0.69 - 0.84	7.6A	 0.119A
	0.84 - 1.02	8.3A	 0.148A
	1.02 - 1.17	8.5A	 0.208A	 6.5E	 3.8	 0.1	 3.3
	1.17 - 1.32	8.8A	 0.327A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06	 0.9D	 7B	 0.015A	 0.08A	<2	 40D	 41	 10	 7
	0.06 - 0.2	 4B	 39D	 41	 14	 7
	0.2 - 0.38
	0.38 - 0.53	 5	 36D	 40	 12	 13
	0.53 - 0.69	 0.012A	 2	 25D	 34	 12	 30
	0.69 - 0.84
	0.84 - 1.02
	1.02 - 1.17	 0.5A
	1.17 - 1.32	 0.01A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.06
	0.06 - 0.2
	0.2 - 0.38
	0.38 - 0.53
	0.53 - 0.69
	0.69 - 0.84
	0.84 - 1.02
	1.02 - 1.17
	1.17 - 1.32

	Project Name:	Regional
	Project Code:	REG	Site ID:	T29	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, 
	pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble
	 salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble
	 salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble
	 salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	19A1	Carbonates - rapid titration
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance