Project Name:	Regional
	Project Code:	REG	Site ID:	T291	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.G. Murtha	Locality:
	Date Desc.:	20/08/80	Elevation:	 15 metres
	Map Ref.:	Sheet No. : 8162   1:100000	Rainfall:	3500
	Northing/Long.:	146.033333333333	Runoff:	Very slow
	Easting/Lat.:	-17.6	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  QA	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Alluvial fan
	1-3%
	Morph. Type:	Lower-slope	Relief:	3 metres
	Elem. Type:	Fan	Slope Category:	Very gently sloped
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Recently cultivated
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Dystrophic Red Dermosol     	Principal Profile Form:	Gn3.71
	ASC Confidence:	Great Soil Group:	No suitable group
	All necessary analytical data are available.
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	Ap	0 - 0.1 m	Brown (10YR4/3-Moist); ; Light clay; Moderate grade of structure, 20-50 mm, Subangular blocky; 
	Moist; Weak consistence; Very few (0 - 2 %), Ferromanganiferous, Medium (2 -6 mm), Nodules; 
	Ap	0.1 - 0.2 m	Brown (10YR4/3-Moist); ; Light clay; Moderate grade of structure, 20-50 mm, Subangular blocky; 
	Moist; Weak consistence; Very few (0 - 2 %), Ferromanganiferous, Medium (2 -6 mm), Nodules; 
	Ap	0.2 - 0.3 m	Brown (10YR4/3-Moist); , 7.5YR54, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, Distinct; 
	Light clay; Moderate grade of structure, 20-50 mm, Subangular blocky; Moist; Weak 
	consistence; Very few (0 - 2 %), Ferromanganiferous, Medium (2 -6 mm), Nodules; Clear change
	 to - 
	B1	0.4 - 0.6 m	Yellowish red (5YR5/6-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, 
	Subangular blocky; Moist; Weak consistence; Very few (0 - 2 %), Ferromanganiferous, Medium 
	(2 -6 mm), Concretions; Diffuse change to - 
	B2	0.6 - 0.9 m	Red (2.5YR4/6-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, Subangular 
	blocky; Wet; Moderately plastic; Normal plasticity; Few (2 - 10 %), Ferromanganiferous, Medium 
	(2 -6 mm), Concretions; Diffuse change to - 
	BC	0.9 - 1.2 m	Red (2.5YR4/6-Moist); , 7.5YR66, 2-10% , 0-5mm, Faint; , 2-10% , 0-5mm, Faint; Medium clay; 
	Strong grade of structure, 10-20 mm, Subangular blocky; Wet; Moderately plastic; Normal 
	plasticity; Few (2 - 10 %), Ferromanganiferous, Medium (2 -6 mm), Concretions; 
	BC	1.2 - 1.5 m	Yellowish red (5YR5/8-Moist); , 10YR68, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, 
	Distinct; Medium clay; Strong grade of structure, 10-20 mm, Subangular blocky; Moist; Weak 
	consistence; Few (2 - 10 %), Ferromanganiferous, Medium (2 -6 mm), Concretions; 
	BC	1.5 - 1.8 m	Yellowish red (5YR5/8-Moist); , 10YR68, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, 
	Distinct; Medium clay; Strong grade of structure, 10-20 mm, Subangular blocky; Moist; Weak 
	consistence; 
	Morphological Notes
	Observation Notes
	FREE WATER IN PROFIE FROM 60-120CM                                                                                      
	Site Notes
	MOURILYAN

	Project Name:	Regional
	Project Code:	REG	Site ID:	T291	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)

	Project Name:	Regional
	Project Code:	REG	Site ID:	T291	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.8A	 0.041A	 0.03H	<0.01	 0.12	 0.03	 2.4F	 2.56A	 2.6F	1.17
	 8.2C	0.37
	0.1 - 0.2	4.8A	 0.038A
	0.2 - 0.4	4.7A	 0.044A	 0.07H	<0.01	 0.07	 0.03	 2.3F	 2.5A	 2.5F	1.20
	 6.9C	0.43
	0.4 - 0.6	4.6A	 0.047A
	0.6 - 0.9	4.6A	 0.002A	<0.02H	<0.01	 0.5	 0.03	 1.7F	 1.7A	 2.3F	1.76
	 3.1C	0.97
	0.9 - 1.2	4.6A	 0.044A
	1.2 - 1.5	4.7A	 0.056A
	1.5 - 1.8	4.8A	 0.062A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.26D	 53B	 0.11A	 0.12A	 0.51A	 0	 14A	 24	 12	 49
	0.1 - 0.2	 0	 14A	 26	 12	 49
	0.2 - 0.4	 1.13D	 53B	 0.11A	 0	 13A	 26	 12	 49
	0.4 - 0.6	 0	 12A	 28	 12	 48
	0.6 - 0.9	 0.23D	 0.045A	 0.53A	 0	 12A	 30	 10	 48
	0.9 - 1.2	 9B	 0	 9A	 28	 11	 52
	1.2 - 1.5
	1.5 - 1.8	 0	 4A	 28	 25	 44
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.4
	0.4 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8

	Project Name:	Regional
	Project Code:	REG	Site ID:	T291	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	MIN_EC	Exchange Capacity - Minerology
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)
	XRD_C_Ch2	Chloritized 2:1 minerals - X-Ray Diffraction
	XRD_C_Gb	Gibbsite - X-Ray Diffraction
	XRD_C_Gt	Geothite - X-Ray Diffraction
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_K2O	K2O - X-Ray Diffraction or Clay Fraction (air dry)
	XRD_C_Ka	Kaolin - X-Ray Diffraction