Project Name:	Regional
	Project Code:	REG	Site ID:	T307	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.G. Murtha	Locality:
	Date Desc.:	11/11/81	Elevation:	 10 metres
	Map Ref.:	Sheet No. : 7965   1:100000	Rainfall:	0
	Northing/Long.:	144.383333333333	Runoff:	No Data
	Easting/Lat.:	-16.25	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qa	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Dystrophic Red Kandosol     	Principal Profile Form:	Um
	ASC Confidence:	Great Soil Group:	No suitable group
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.14 m	Dark greyish brown (10YR4/2-Moist); ; Sandy clay loam (Light); Moderate grade of structure, 5-10 
	mm, Cast; Earthy fabric; Moist; Weak consistence; Many, fine (1-2mm) roots; Clear change to - 
	B11	0.14 - 0.3 m	Yellowish brown (10YR5/5-Moist); ; Sandy clay loam (Light); Massive grade of structure; Earthy 
	fabric; Moist; Weak consistence; Common, fine (1-2mm) roots; Diffuse change to - 
	B12	0.3 - 0.4 m	Yellowish brown (10YR5/6-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; 
	Moist; Weak consistence; Few, fine (1-2mm) roots; 
	B13	0.4 - 0.6 m	Strong brown (7.5YR5/6-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; 
	Moist; Weak consistence; Few, fine (1-2mm) roots; Diffuse change to - 
	B2	0.6 - 0.9 m	Yellowish red (5YR5/8-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; 
	Moist; Weak consistence; Few, fine (1-2mm) roots; 
	B2	0.9 - 1.2 m	Yellowish red (5YR5/8-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; 
	Moist; Weak consistence; Diffuse change to - 
	B3	1.2 - 1.5 m	Reddish yellow (5YR6/8-Moist); , 10YR64, 10-20% , 5-15mm, Faint; , 10-20% , 5-15mm, Faint; 
	Sandy clay loam (Light); Massive grade of structure; Earthy fabric; Moist; Weak consistence; 2-
	10%, medium gravelly, 6-20mm, Quartz, coarse fragments; 
	1.5 - 1.8 m	Reddish yellow (5YR6/8-Moist); , 10YR64, 10-20% , 5-15mm, Faint; , 10-20% , 5-15mm, Faint; 
	Sandy clay loam (Light); Massive grade of structure; Earthy fabric; Weak consistence; 2-10%, 
	medium gravelly, 6-20mm, Quartz, coarse fragments; 
	1.8 - 2.1 m	Reddish yellow (5YR6/8-Moist); , 10YR64, 10-20% , 5-15mm, Faint; , 10-20% , 5-15mm, Faint; 
	Sandy clay loam (Light); Massive grade of structure; Earthy fabric; Weak consistence; 2-10%, 
	medium gravelly, 6-20mm, Quartz, coarse fragments; 
	Morphological Notes
	Observation Notes
	Site Notes
	DAINTREE

	Project Name:	Regional
	Project Code:	REG	Site ID:	T307	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.14	4.8A	 0.023A	 0.11H	 0.07	 0.07	 0.05	 1.5F	 2.04A	 1.8F	2.45
	 3C	1.67
	0.14 - 0.3	4.9A	 0.014A
	0.3 - 0.4	4.9A	 0.014A	<0.02H	<0.01	 0.06	 0.03	 1.1F	 1.35A	 1.2F	2.22
	 1C	3.00
	0.4 - 0.6	4.8A	 0.011A
	0.6 - 0.9	4.9A	 0.011A	<0.02H	<0.01	 0.05	 0.02	 0.8F	 0.93A	 0.9F	2.15
	 1C	2.00
	0.9 - 1.2	4.8A	 0.011A
	1.2 - 1.5	4.8A	 0.011A
	1.5 - 1.8	4.9A	 0.008A
	1.8 - 2.1	5A	 0.011A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.14	 1.37D	 14B	 0.009A	 0.11A	 0.68A	 0	 34A	 38	 15	 13
	0.14 - 0.3	 0.73D	 9B	 0.06A
	0.3 - 0.4	 0.28D	 9B	 0	 30A	 39	 16	 15
	0.4 - 0.6	 0.15D	 7B	 0.02A
	0.6 - 0.9	 9B	 0.005A	 0.65A	 0	 37A	 37	 14	 12
	0.9 - 1.2
	1.2 - 1.5	 8	 34A	 40	 13	 13
	1.5 - 1.8
	1.8 - 2.1	 20	 50A	 24	 9	 18
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.14
	0.14 - 0.3
	0.3 - 0.4
	0.4 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2.1

	Project Name:	Regional
	Project Code:	REG	Site ID:	T307	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)