Project Name:	Regional
	Project Code:	REG	Site ID:	T324	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	01/12/81	Elevation:	 15 metres
	Map Ref.:	Sheet No. : 7965   1:100000	Rainfall:	0
	Northing/Long.:	145.366666666667	Runoff:	No Data
	Easting/Lat.:	-16.4666666666667	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qa	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Dystrophic Yellow Dermosol     	Principal Profile Form:	Uf6.34
	ASC Confidence:	Great Soil Group:	No suitable group
	All necessary analytical data are available.
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	Ap	0 - 0.1 m	Dark greyish brown (2.5Y4/2-Moist); ; Medium heavy clay; Moderate grade of structure, 5-10 mm, 
	Subangular blocky; Smooth-ped fabric; Moist; 
	Ap	0.1 - 0.3 m	Dark greyish brown (2.5Y4/2-Moist); ; Medium heavy clay; Moderate grade of structure, 5-10 mm, 
	Subangular blocky; Smooth-ped fabric; Moist; Clear change to - 
	B21	0.3 - 0.6 m	Olive yellow (2.5Y6/6-Moist); ; Medium heavy clay; Moderate grade of structure, 5-10 mm, 
	Subangular blocky; Smooth-ped fabric; Moist; Few (2 - 10 %), Ferromanganiferous, Medium (2 -6 
	mm), Nodules; 
	B21	0.6 - 0.9 m	Light olive brown (2.5Y5/6-Moist); ; Medium heavy clay; Moderate grade of structure, 5-10 mm, 
	Subangular blocky; Smooth-ped fabric; Moist; Few (2 - 10 %), Ferromanganiferous, Medium (2 -6 
	mm), Nodules; Diffuse change to - 
	B22	0.9 - 1.2 m	Brownish yellow (10YR6/6-Moist); , 2.5YR48, 2-10% , 0-5mm, Faint; , 2-10% , 0-5mm, Faint; 
	Medium heavy clay; Moderate grade of structure, 5-10 mm, Subangular blocky; Smooth-ped 
	fabric; Moist; Few (2 - 10 %), Ferromanganiferous, Medium (2 -6 mm), Nodules; Diffuse change 
	to - 
	B22	1.2 - 1.5 m	Brownish yellow (10YR6/6-Moist); , 2.5YR48, 10-20% , 0-5mm, Distinct; , 10-20% , 0-5mm, 
	Distinct; Medium heavy clay; Moderate grade of structure, 5-10 mm, Subangular blocky; Smooth-
	ped fabric; Moist; 2-10%, Quartz, coarse fragments; Few (2 - 10 %), Ferromanganiferous, Medium
	 (2 -6 mm), Nodules; Gradual change to - 
	1.5 - 1.8 m	Olive yellow (2.5Y6/6-Moist); , 5YR58, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, Distinct; 
	Sandy medium clay; Weak grade of structure, 5-10 mm, Subangular blocky; Smooth-ped fabric; 
	10-20%, Quartz, coarse fragments; Common (10 - 20 %), Ferromanganiferous, Medium (2 -6 
	mm), Nodules; Diffuse change to - 
	B3	1.8 - 2.1 m	Olive yellow (2.5Y6/6-Moist); , 5YR58, 20-50% , 5-15mm, Distinct; , 20-50% , 5-15mm, Distinct; 
	Sandy medium clay; Weak grade of structure, 5-10 mm, Subangular blocky; Smooth-ped fabric; 
	Moist; 20-50%, Quartz, coarse fragments; Common (10 - 20 %), Ferromanganiferous, Medium (2 -
	6 mm), Nodules; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Regional
	Project Code:	REG	Site ID:	T324	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	MOSSMAN

	Project Name:	Regional
	Project Code:	REG	Site ID:	T324	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.8A	 0.035A	 3.09H	 0.2	 0.34	 0.07	 0.3F	 4.81A	 4F	1.46
	 4C	1.75
	0.1 - 0.3	5.8A	 0.026A
	0.3 - 0.6	5.5A	 0.041A	 1.39H	 0.03	 0.11	 0.06	 1.1F	 2.45A	 2.7F	2.45
	0.6 - 0.9	5.6A	 0.032A
	0.9 - 1.2	5.4A	 0.029A	 1.44H	 0.09	 0.09	 0.05	 0.6F	 2.38A	 2.3F	2.10
	 4C	1.25
	1.2 - 1.5	5.2A	 0.026A
	1.5 - 1.8	5.4A	 0.014A
	1.8 - 2.1	5.3A	 0.011A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.05D	 68B	 0.05A	 0.09A	 1.52A	 0	 11A	 28	 34	 27
	0.1 - 0.3	 72B
	0.3 - 0.6	 0.44D	 12B	 0.05A	 0	 7A	 26	 34	 33
	0.6 - 0.9	 4B	 0	 10A	 27	 31	 32
	0.9 - 1.2	 0.019A	 2.86A	 1	 14A	 28	 26	 32
	1.2 - 1.5
	1.5 - 1.8	 3	 20A	 32	 19	 30
	1.8 - 2.1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.3
	0.3 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2.1

	Project Name:	Regional
	Project Code:	REG	Site ID:	T324	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	MIN_EC	Exchange Capacity - Minerology
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)
	XRD_C_Ch2	Chloritized 2:1 minerals - X-Ray Diffraction
	XRD_C_Gb	Gibbsite - X-Ray Diffraction
	XRD_C_Gt	Geothite - X-Ray Diffraction
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_K2O	K2O - X-Ray Diffraction or Clay Fraction (air dry)
	XRD_C_Ka	Kaolin - X-Ray Diffraction