Project Name:	Regional
	Project Code:	REG	Site ID:	T326	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	01/12/81	Elevation:	 10 metres
	Map Ref.:	Sheet No. : 7964   1:100000	Rainfall:	0
	Northing/Long.:	145.466666666667	Runoff:	No Data
	Easting/Lat.:	-16.5416666666667	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qa	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Magnesic Brown Dermosol     	Principal Profile Form:	Uf6.34
	ASC Confidence:	Great Soil Group:	No suitable group
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:
	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Panicum species
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark greyish brown (2.5Y4/2-Moist); Light grey (10YR7/2-Dry); ; Light clay; Moderate grade of 
	structure, 5-10 mm, Cast; Moist; Weak consistence; Clear change to - 
	B21	0.1 - 0.3 m	Olive yellow (2.5Y6/6-Moist); ; Light medium clay; Strong grade of structure, 5-10 mm, 
	Subangular blocky; Moist; Weak consistence; Gradual change to - 
	B22	0.3 - 0.5 m	Olive yellow (2.5Y6/6-Moist); , 2.5YR48, 2-10% , 0-5mm, Faint; , 2-10% , 0-5mm, Faint; Medium 
	clay; Strong grade of structure, 5-10 mm, Subangular blocky; Moist; Weak consistence; Diffuse 
	change to - 
	B22	0.5 - 0.6 m	Olive yellow (2.5Y6/6-Moist); , 2.5YR48, 10-20% , 0-5mm, Distinct; , 10-20% , 0-5mm, Distinct; 
	Medium clay; Strong grade of structure, 5-10 mm, Subangular blocky; Moist; Weak consistence; 
	B23	0.6 - 0.9 m	Pale yellow (5Y7/4-Moist); , 2.5YR48, 10-20% , 5-15mm, Prominent; , 10-20% , 5-15mm, 
	Prominent; Medium clay; Strong grade of structure, 5-10 mm, Subangular blocky; Moist; Weak 
	consistence; Few (2 - 10 %), Ferromanganiferous, Medium (2 -6 mm), Nodules; Gradual change 
	to - 
	D	0.9 - 1.2 m	Pale yellow (5Y7/3-Moist); , 5YR56, 20-50% , 5-15mm, Distinct; , 20-50% , 5-15mm, Distinct; 
	Medium clay; Strong grade of structure, 10-20 mm, Subangular blocky; Moist; Weak 
	consistence; Few (2 - 10 %), Ferromanganiferous, Medium (2 -6 mm), Nodules; Diffuse change 
	to - 
	1.2 - 1.5 m	Grey (2.5Y5/1-Moist); , 7.5YR66, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, Distinct; Heavy 
	clay; Strong grade of structure, 20-50 mm, Angular blocky; Very strong consistence; Few (2 - 10 
	%), Ferromanganiferous, Medium (2 -6 mm), Nodules; 
	1.5 - 1.8 m	Grey (2.5Y5/1-Moist); , 7.5YR66, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, Distinct; Heavy 
	clay; Strong grade of structure, 20-50 mm, Angular blocky; Very strong consistence; Few (2 - 10 
	%), Ferromanganiferous, Medium (2 -6 mm), Nodules; 
	1.8 - 2.1 m	Grey (2.5Y5/1-Moist); , 7.5YR66, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, Distinct; Heavy 
	clay; Strong grade of structure, 20-50 mm, Angular blocky; Very strong consistence; Few (2 - 10 
	%), Ferromanganiferous, Medium (2 -6 mm), Nodules; 
	Morphological Notes

	Project Name:	Regional
	Project Code:	REG	Site ID:	T326	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Observation Notes
	STRONG COARSE SLICKENSIDES FROM 150-180CM:                                                                              
	Site Notes

	Project Name:	Regional
	Project Code:	REG	Site ID:	T326	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.1A	 0.032A	 0.82H	 1.14	 0.14	 0.16	 1.4F	 3.81A	 3.7F	4.20
	0.1 - 0.3	5.7A	 0.014A
	0.3 - 0.5	6A	 0.011A	 0.03H	 1.75	 0.05	 0.15	 0.5F	 3.27A	 2.5F	4.59
	0.5 - 0.6	5.9A	 0.026A
	0.6 - 0.9	6A	 0.014A	 0.01H	 2.51	 0.05	 0.19	 0.3F	 3.18A	 3.1F	5.97
	0.9 - 1.2	5.9A	 0.026A
	1.2 - 1.5	5.8A	 0.13A	 1.16H	 11.5	 0.07	 1.24	 0.6F	 13.5A	 14.6F	9.19
	1.5 - 1.8	6.9A	 0.336A
	1.8 - 2.1	7.8A	 0.458A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.19D	 5B	 0.01A	 0.15A	 1.94A	<1	 2A	 30	 43	 24
	0.1 - 0.3	 6B	 0	 1A	 20	 41	 38
	0.3 - 0.5	 0.19D	 3B	 0.05A	<1	 2A	 19	 42	 36
	0.5 - 0.6	 7B
	0.6 - 0.9	 7B	 0.005A	 1.92A	<1	 3A	 30	 34	 32
	0.9 - 1.2
	1.2 - 1.5	 0	 2A	 12	 46	 40
	1.5 - 1.8
	1.8 - 2.1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.3
	0.3 - 0.5
	0.5 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2.1

	Project Name:	Regional
	Project Code:	REG	Site ID:	T326	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)