Project Name:	Regional
	Project Code:	REG	Site ID:	T33	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.F. Isbell	Locality:	Southern corner of Brolga and Double Barrel 
	Creek:48M from Double Barrel Creek:
	Date Desc.:	16/09/64	Elevation:	No Data
	Map Ref.:	Sheet No. : 8258   1:100000	Rainfall:	870
	Northing/Long.:	146.85	Runoff:	Moderately rapid
	Easting/Lat.:	-19.6666666666667	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qa	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Levee	Slope Category:	Very gently sloped
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Dermosol     	Principal Profile Form:	Gn3.15
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Heteropogon contortus
	Mid Strata - , , . *Species includes - Planchonia careya
	Tall Strata - Tree, , Sparse. *Species includes - Eucalyptus alba, Eucalyptus tessellaris, Eucalyptus tereticornis
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.13 m	Very dark brown (10YR2/2-Moist); Dark grey (10YR4/1-Dry); , 0-0% ; , 0-0% ; Loam; Weak grade of
	 structure, 5-10 mm, Angular blocky; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-
	1mm) macropores, Dry; Strong consistence; Clear change to - 
	A2	0.13 - 0.3 m	Dark brown (10YR3/3-Moist); Brown (10YR5/3-Dry); , 0-0% ; , 0-0% ; Loam (Heavy); Weak grade of
	 structure, 20-50 mm, Angular blocky; Dry; Strong consistence; 0-2%, fine gravelly, 2-6mm, 
	Sand, coarse fragments; Clear change to - 
	B1	0.3 - 0.46 m	Brown (7.5YR4/4-Moist); Reddish yellow (7.5YR6/5-Dry); , 0-0% ; , 0-0% ; Light clay; Moderate 
	grade of structure, 20-50 mm, Angular blocky; Common (1-5 per 100mm2) Very fine (0.075-1mm)
	 macropores, Dry; Very strong consistence; 0-2%, fine gravelly, 2-6mm, Sand, coarse fragments;
	 Gradual change to - 
	B21	0.46 - 0.71 m	Reddish brown (5YR4/4-Moist); , 0-0% ; , 0-0% ; Medium clay; Moderate grade of structure, 20-50
	 mm, Angular blocky; Smooth-ped fabric; Dry; Very strong consistence; 0-2%, fine gravelly, 2-
	6mm, Sand, coarse fragments; Field pH 6.5 (pH meter, 0.71); Gradual change to - 
	B22	0.71 - 0.91 m	Reddish brown (5YR4/4-Moist); , 2.5YR46; , 10YR43; Medium clay; Moderate grade of structure, 
	20-50 mm, Angular blocky; Dry; Very strong consistence; 2-10%, coarse gravelly, 20-60mm, 
	rounded, Gravel, coarse fragments; Field pH 6.2 (pH meter, 0.91); Gradual change to - 
	BC	0.91 - 1.14 m	Yellowish red (5YR4/6-Moist); , 0-0% ; , 0-0% ; Sandy medium clay; Very firm consistence; 10-
	20%, coarse gravelly, 20-60mm, Gravel, coarse fragments; Gradual change to - 
	C	1.14 - 1.37 m	Yellowish red (5YR4/6-Moist); , 0-0% ; , 0-0% ; Sandy clay loam (Light); Firm consistence; 2-
	10%, fine gravelly, 2-6mm, Sand, coarse fragments; 
	1.37 - 1.47 m	; 
	Morphological Notes
	Large gravel fragement stopped auger at 137 CM'S:
	Observation Notes
	Site Notes

	Project Name:	Regional
	Project Code:	REG	Site ID:	T33	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	LANDSDOWN

	Project Name:	Regional
	Project Code:	REG	Site ID:	T33	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	6.3A	 0.089A	 9.6E	 2	 0.7	 0.35	 4.5F	 17C	 17.2F	2.06
	0.13 - 0.3	6.3A	 0.029A
	0.3 - 0.46	6.5A	 0.029A	 6.4E	 2	 0.33	 0.42	 2.6F	 12C	 11.8F	3.50
	0.46 - 0.71	6.4A	 0.029A	 6.4E	 2	 0.3	 0.25	 3.3F	 12C	 12.3F	2.08
	0.71 - 0.91	6.5A	 0.029A
	0.91 - 1.14	6.6A	 0.029A
	1.14 - 1.37	6.6A	 0.029A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13	 1.6D	 100B	 0.045A	 0.12A	 0	 16D	 42	 24	 19
	0.13 - 0.3	 0.7D	 52B	 0.05A
	0.3 - 0.46	 0	 18D	 36	 23	 23
	0.46 - 0.71	 0.025A	 0	 21D	 32	 20	 28
	0.71 - 0.91
	0.91 - 1.14	 0.023A
	1.14 - 1.37
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13
	0.13 - 0.3
	0.3 - 0.46
	0.46 - 0.71
	0.71 - 0.91
	0.91 - 1.14
	1.14 - 1.37

	Project Name:	Regional
	Project Code:	REG	Site ID:	T33	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, 
	pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble
	 salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble
	 salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble
	 salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance