Project Name:	Regional
	Project Code:	REG	Site ID:	T334	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.J. Coventry	Locality:
	Date Desc.:	04/10/73	Elevation:	No Data
	Map Ref.:	Sheet No. : 7956   1:100000	Rainfall:	600
	Northing/Long.:	145.194444444444	Runoff:	No Data
	Easting/Lat.:	-20.7277777777778	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	N/A
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Mesotrophic Red Kandosol     	Principal Profile Form:	Gn2.42
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - None recorded
	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Grevillea parallela, Acacia species
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus whitei, Eucalyptus papuana
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark reddish brown (5YR3/3-Moist); Reddish brown (5YR4/4-Dry); , 0-0% ; , 0-0% ; Sandy loam; 
	Massive grade of structure; Dry; Weak consistence; Many, fine (1-2mm) roots; 
	A1	0.1 - 0.2 m	Dark reddish brown (5YR3/3-Moist); Reddish brown (5YR4/4-Dry); , 0-0% ; , 0-0% ; Sandy loam 
	(Light); Massive grade of structure; Dry; Weak consistence; Many, fine (1-2mm) roots; Gradual 
	change to - 
	A3	0.2 - 0.3 m	Dark reddish brown (5YR3/4-Moist); Yellowish red (5YR4/8-Dry); , 0-0% ; , 0-0% ; Sandy loam 
	(Heavy); Massive grade of structure; Dry; Weak consistence; Common, fine (1-2mm) roots; 
	Gradual change to - 
	B11	0.3 - 0.6 m	Red (2.5YR4/8-Moist); Red (2.5YR4/8-Dry); , 2.5YR36, 0-2% , 5-15mm, Faint; , 0-2% , 5-15mm, 
	Faint; Sandy clay loam; Massive grade of structure; Dry; Weak consistence; Few, fine (1-2mm) 
	roots; Gradual change to - 
	B12	0.6 - 0.9 m	Red (2.5YR4/8-Moist); , 2.5YR36, 2-10% , 5-15mm, Distinct; , 2-10% , 5-15mm, Distinct; Sandy 
	clay loam (Heavy); Massive grade of structure; Dry; Strong consistence; 
	B12	0.9 - 1.2 m	Dark red (2.5YR3/7-Moist); , 2.5YR36, 2-10% , 5-15mm, Distinct; , 2-10% , 5-15mm, Distinct; 
	Sandy clay loam (Heavy); Massive grade of structure; Dry; Strong consistence; Gradual change 
	to - 
	B21	1.2 - 1.5 m	Dark red (2.5YR3/7-Moist); , 0-0% ; , 0-0% ; Sandy medium clay; Massive grade of structure; Dry; 
	Strong consistence; 
	B21	1.5 - 1.8 m	Dark red (2.5YR3/7-Moist); , 2.5YR64, 2-10% , 0-5mm, Distinct; , 2-10% , 0-5mm, Distinct; Sandy
	 medium clay; Massive grade of structure; Dry; Strong consistence; Gradual change to - 
	B22	1.8 - 2.1 m	Dark red (2.5YR3/7-Moist); , 10YR57, 10-20% , 15-30mm, Distinct; , 10-20% , 15-30mm, Distinct;
	 Sandy medium clay; Massive grade of structure; Dry; Strong consistence; Many (20 - 50 %), 
	Argillaceous, , Nodules; 
	B22	2.1 - 2.4 m	Dark red (2.5YR3/7-Moist); , 10YR57, 10-20% , 15-30mm, Distinct; , 10-20% , 15-30mm, Distinct;
	 Sandy medium clay; Massive grade of structure; Dry; Strong consistence; Many (20 - 50 %), 
	Argillaceous, , Nodules; 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T334	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B22	2.4 - 2.7 m	Dark red (2.5YR3/7-Moist); , 10YR57, 10-20% , 15-30mm, Distinct; , 10-20% , 15-30mm, Distinct;
	 Sandy medium clay; Massive grade of structure; Dry; Strong consistence; Many (20 - 50 %), 
	Argillaceous, , Nodules; 
	B22	2.7 - 3 m	Dark red (2.5YR3/7-Moist); , 10YR57, 10-20% , 15-30mm, Distinct; , 2.5YR63, 10-20% , 15-
	30mm, Distinct; Sandy medium clay; Massive grade of structure; Dry; Strong consistence; Many 
	(20 - 50 %), Argillaceous, , Nodules; 
	B22	3 - 3.5 m	Dark red (2.5YR3/7-Moist); , 10YR57, 10-20% , 15-30mm, Distinct; , 2.5YR63, 10-20% , 15-
	30mm, Distinct; Sandy medium clay; Massive grade of structure; Dry; Strong consistence; Many 
	(20 - 50 %), Argillaceous, , Nodules; Gradual change to - 
	BC	3.5 - 4 m	Yellowish brown (10YR5/6-Moist); , 2.5YR48, 10-20% , 15-30mm, Distinct; , 2.5YR62, 10-20% , 
	15-30mm, Distinct; Sandy medium clay; Massive grade of structure; Dry; Strong consistence; 
	Few (2 - 10 %), Argillaceous, Medium (2 -6 mm), Nodules; Gradual change to - 
	C1	4 - 4.5 m	Yellowish brown (10YR5/7-Moist); , 2.5YR36, 10-20% , 15-30mm, Prominent; , 10-20% , 15-
	30mm, Prominent; Sandy medium clay; Massive grade of structure; Dry; Very strong 
	consistence; 
	C1	4.5 - 5 m	Yellowish brown (10YR5/7-Moist); , 2.5YR36, 10-20% , 15-30mm, Prominent; , 10-20% , 15-
	30mm, Prominent; Sandy medium clay; Massive grade of structure; Dry; Very strong 
	consistence; 
	C1	5 - 5.33 m	 (N6/0-Moist); , 2.5YR36, 10-20% , 15-30mm, Prominent; , 10-20% , 15-30mm, Prominent; 
	Massive grade of structure; Dry; Very strong consistence; 
	Morphological Notes
	Observation Notes
	SOME BIOTUBATION IN A1 AND A3 HORIZONS.                                                                                 
	Site Notes

	Project Name:	Regional
	Project Code:	REG	Site ID:	T334	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.1A	 0.48A	 2.62H	 1.36	 0.38	 0.04	 0.19F	 4.97A	 4.6F	0.80
	 4.97C
	0.1 - 0.2	6A
	0.2 - 0.3	6A	 0.03A
	0.3 - 0.6	5.9A	 0.03A	 1.94H	 1.6	 0.39	 0.03	 0.19F	 3.77A	 4.2F	0.80
	 3.77C
	0.6 - 0.9	5.6A	 0.024A	 1.54H	 1.7	 0.07	 0.04	 0.13F	 3.4A	 3.5F	1.18
	 3.4C
	0.9 - 1.2	6.2A	 0.016A
	1.2 - 1.5	6.4A	 0.16A	 1.11H	 2.14	 0.04	 0.08	 0.27F	 4.07A	 3.6F	1.97
	 4.07C
	1.5 - 1.8	6.6A	 0.018A
	1.8 - 2.1	6.7A	 0.021A	 0.73H	 2.18	 0.04	 0.17	 0.17F	 3.71A	 3.3F	4.58
	 3.71C
	2.1 - 2.4	6.4A	 0.025A
	2.4 - 2.7	6.7A	 0.023A
	2.7 - 3	6.9A	 0.023A
	3 - 3.5	6.7A	 0.024A
	3.5 - 4	7A	 0.019A
	4 - 4.5	7A	 0.025A
	4.5 - 5	7A	 0.026A
	5 - 5.33	6.9A	 0.043A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.98D	 5B	 0.014A	 0.058A	 0.13A	 0	 31A	 39	 12	 19
	0.1 - 0.2	 0	 28A	 37	 11	 24
	0.2 - 0.3	 0.49D	 2B	 0.041A	 0	 29A	 36	 15	 21
	0.3 - 0.6	 0.39D	 3B	 0.009A	 0.028A	 0.13A	 0	 27A	 32	 10	 31
	0.6 - 0.9	 0.009A	 0.12A	 0	 24A	 30	 11	 36
	0.9 - 1.2	 1	 24A	 27	 9	 40
	1.2 - 1.5	 0.009A	 0.12A	 1	 22A	 27	 9	 42
	1.5 - 1.8	 1	 25A	 26	 8	 42
	1.8 - 2.1	 1	 23A	 26	 9	 42
	2.1 - 2.4	 2	 25A	 25	 9	 41
	2.4 - 2.7	 1	 24A	 26	 11	 39
	2.7 - 3	 1	 26A	 28	 10	 36
	3 - 3.5	 1	 27A	 27	 9	 36
	3.5 - 4	 2	 33A	 27	 9	 32
	4 - 4.5	 1	 32A	 30	 9	 29
	4.5 - 5	 1	 34A	 28	 9	 29
	5 - 5.33	 3	 32A	 30	 9	 29
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2

	Project Name:	Regional
	Project Code:	REG	Site ID:	T334	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2.1
	2.1 - 2.4
	2.4 - 2.7
	2.7 - 3
	3 - 3.5
	3.5 - 4
	4 - 4.5
	4.5 - 5
	5 - 5.33

	Project Name:	Regional
	Project Code:	REG	Site ID:	T334	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)