Project Name:	Regional
	Project Code:	REG	Site ID:	T361	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	25/11/83	Elevation:	 70 metres
	Map Ref.:	Sheet No. : 8061   1:100000	Rainfall:	2250
	Northing/Long.:	145.916666666667	Runoff:	Moderately rapid
	Easting/Lat.:	-18.1458333333333	Drainage:	Well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  QA	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Rolling low hills 30-90m 10-	Pattern Type:	Low hills
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Fan	Slope Category:	Gently inclined
	Slope:	10 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melacic Magnesic Red Kandosol     	Principal Profile Form:	Dr2.51
	ASC Confidence:	Great Soil Group:	Red earth
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Mid Strata - Tree, 6.01-12m, Isolated clumps. *Species includes - Casuarina littoralis
	Tall Strata - Tree, 20.01-35m, Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Black (10YR2/1-Moist); Mottles, 0-0% ; Mottles, 0-0% ; Sandy clay loam (Light); Massive grade of
	 structure; Earthy fabric; Weak consistence; Many, medium (2-5mm) roots; 
	A1	0.1 - 0.2 m	Black (10YR2/1-Moist); Mottles, 0-0% ; Mottles, 0-0% ; Sandy clay loam (Light); Massive grade of
	 structure; Earthy fabric; Weak consistence; Many, medium (2-5mm) roots; 
	A1	0.2 - 0.3 m	Black (10YR2/1-Moist); Mottles, 0-0% ; Mottles, 0-0% ; Sandy clay loam (Light); Massive grade of
	 structure; Earthy fabric; Weak consistence; Many, medium (2-5mm) roots; Diffuse, Broken 
	change to - 
	A3	0.3 - 0.45 m	Very dark grey (5YR3/1-Moist); Mottles, 0-0% ; Mottles, 0-0% ; Sandy clay loam; Massive grade of
	 structure; Earthy fabric; Weak consistence; Common, fine (1-2mm) roots; Clear, Wavy change 
	to - 
	B1	0.45 - 0.5 m	Reddish brown (5YR4/3-Moist); Mottles, 0-0% ; Mottles, 0-0% ; Clay loam, sandy; Massive grade 
	of structure; Earthy fabric; Firm consistence; Few, fine (1-2mm) roots; Clear, Wavy change to - 
	B2	0.5 - 0.6 m	Red (2.5YR4/8-Moist); Mottles, 0-0% ; Mottles, 0-0% ; Medium clay; Massive grade of structure; 
	Earthy fabric; Firm consistence; 20-50%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, 
	coarse fragments; 
	B2	0.6 - 0.9 m	Red (2.5YR4/8-Moist); Mottles, 0-0% ; Mottles, 0-0% ; Medium clay; Massive grade of structure; 
	Earthy fabric; Firm consistence; 20-50%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, 
	coarse fragments; 
	B2	0.9 - 1.2 m	Red (2.5YR4/8-Moist); Mottles, 0-0% ; Mottles, 0-0% ; Medium clay; Massive grade of structure; 
	Earthy fabric; Firm consistence; 20-50%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, 
	coarse fragments; 
	B2	1.2 - 1.5 m	Red (2.5YR4/8-Moist); Mottles, 0-0% ; Mottles, 0-0% ; Medium clay; Massive grade of structure; 
	Earthy fabric; Firm consistence; 20-50%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, 
	coarse fragments; 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T361	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B2	1.5 - 1.8 m	Red (2.5YR4/8-Moist); Mottles, 0-0% ; Mottles, 0-0% ; Medium clay; Massive grade of structure; 
	Earthy fabric; Firm consistence; 20-50%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, 
	coarse fragments; 
	B2	1.8 - 2 m	Red (2.5YR4/8-Moist); Mottles, 0-0% ; Mottles, 0-0% ; Medium clay; Massive grade of structure; 
	Earthy fabric; Firm consistence; 20-50%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, 
	coarse fragments; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Regional
	Project Code:	REG	Site ID:	T361	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.4A	 0.07A	 2.5H	 1	 0.18	 0.03	 0.76F	 4.2A	 4.5F	0.71
	 24.2C	0.12
	0.1 - 0.2	5.1A	 0.06A
	0.2 - 0.3	5A	 0.04A	 0.11H	 0.23	<0.02	 0.03	 2.46F	 2.5A	 2.9F	1.20
	 17.1C	0.18
	0.3 - 0.45	4.9A	 0.043A
	0.45 - 0.5	5.1A	 0.027A
	0.5 - 0.6	5.3A	 0.017A	<0.02H	 0.66	<0.02	<0.02	 0.71F	 1.9A	 1.4F
	 3.5C
	0.6 - 0.9	5.4A	 0.014A	<0.02H	 0.83	<0.02	<0.02	 0.25F	 1.4A	 1.1F
	 2C
	0.9 - 1.2	5.5A	 0.012A
	1.2 - 1.5	5.5A	 0.011A	<0.02H	 1.13	<0.02	<0.02	 0.12F	 2.4A	 1.3F
	 3.2C
	1.5 - 1.8	5.6A	 0.01A
	1.8 - 2	5.6A	 0.009A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 9.01C	 9B	 0.03A	 0.34A	 0.19A	 13	 39A	 12	 16	 33
	0.1 - 0.2	 9B	 7	 33A	 12	 14	 41
	0.2 - 0.3	 5.19C	 5B	 0.021A	 0.21A	 0.16A	 9	 33A	 12	 10	 45
	0.3 - 0.45	 4C	 3B	 0.14A	 18	 35A	 10	 7	 48
	0.45 - 0.5	 3B	 19	 34A	 12	 5	 50
	0.5 - 0.6	 0.65C	 2B	 0.011A	 0.04A	 0.13A	 22	 36A	 10	 4	 50
	0.6 - 0.9	 20	 35A	 9	 2	 54
	0.9 - 1.2	 22	 36A	 7	 1	 56
	1.2 - 1.5	 0.11C	 0.008A	 0.06A	 22	 26A	 6	 1	 66
	1.5 - 1.8	 19	 29A	 6	 3	 62
	1.8 - 2	 7	 30A	 5	 5	 60
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.45
	0.45 - 0.5
	0.5 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2

	Project Name:	Regional
	Project Code:	REG	Site ID:	T361	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_FE	Total element - Fe(%) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6B3	Total organic carbon - high frequency induction furnace, infrared
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	9H1	Phosphate retention
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)