Project Name:	Regional
	Project Code:	REG	Site ID:	T363	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	24/11/83	Elevation:	 20 metres
	Map Ref.:	Sheet No. : 8161   1:100000	Rainfall:	2250
	Northing/Long.:	146.129166666667	Runoff:	Slow
	Easting/Lat.:	-18.4527777777778	Drainage:	Moderately well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  QA	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Fan	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Yellow Kandosol     	Principal Profile Form:	Gn2.21
	ASC Confidence:	Great Soil Group:	Yellow earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Mid Strata - Tree, 6.01-12m, Isolated clumps. *Species includes - Casuarina littoralis
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus alba
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.04 m	Very dark grey (10YR3/1-Moist); Mottles, 0-0% ; Mottles, 0-0% ; Sandy clay loam (Light); Massive 
	grade of structure; Earthy fabric; Moderately moist; Very weak consistence; 2-10%, fine gravelly, 
	2-6mm, angular, dispersed, Quartz, coarse fragments; Common, very fine (0-1mm) roots; Clear, 
	Wavy change to - 
	A3	0.04 - 0.1 m	Brown (10YR4/3-Moist); Mottles, 0-0% ; Mottles, 0-0% ; Clay loam, sandy; Massive grade of 
	structure; Earthy fabric; Moderately moist; Weak consistence; 2-10%, fine gravelly, 2-6mm, 
	angular, dispersed, Quartz, coarse fragments; Common, very fine (0-1mm) roots; 
	A3	0.1 - 0.15 m	Brown (10YR4/3-Moist); Mottles, 0-0% ; Mottles, 0-0% ; Clay loam, sandy; Massive grade of 
	structure; Earthy fabric; Moderately moist; Weak consistence; 2-10%, fine gravelly, 2-6mm, 
	angular, dispersed, Quartz, coarse fragments; Common, very fine (0-1mm) roots; Gradual, Wavy 
	change to - 
	B1	0.15 - 0.2 m	Yellowish brown (10YR5/4-Moist); Mottles, 0-0% ; Mottles, 0-0% ; Clay loam, sandy; Massive 
	grade of structure; Earthy fabric; Moderately moist; Weak consistence; 2-10%, fine gravelly, 2-
	6mm, angular, dispersed, Quartz, coarse fragments; Few, medium (2-5mm) roots; 
	B1	0.2 - 0.27 m	Yellowish brown (10YR5/4-Moist); Mottles, 0-0% ; Mottles, 0-0% ; Clay loam, sandy; Massive 
	grade of structure; Earthy fabric; Moderately moist; Weak consistence; 2-10%, fine gravelly, 2-
	6mm, angular, dispersed, Quartz, coarse fragments; Few, medium (2-5mm) roots; Gradual, Wavy
	 change to - 
	B2	0.27 - 0.3 m	Olive yellow (2.5Y6/6-Moist); Mottles, 0-0% ; Mottles, 0-0% ; Sandy medium clay (Light); Massive 
	grade of structure; Earthy fabric; Moderately moist; Weak consistence; 20-50%, medium 
	gravelly, 6-20mm, subangular, dispersed, Quartz, coarse fragments; Few, medium (2-5mm) 
	roots; 
	B2	0.3 - 0.6 m	Olive yellow (2.5Y6/6-Moist); Mottles, 0-0% ; Mottles, 0-0% ; Sandy medium clay (Light); Massive 
	grade of structure; Earthy fabric; Moderately moist; Weak consistence; 20-50%, medium 
	gravelly, 6-20mm, subangular, dispersed, Quartz, coarse fragments; Few, medium (2-5mm) 
	roots; 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T363	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B2	0.6 - 0.65 m	Olive yellow (2.5Y6/6-Moist); Mottles, 0-0% ; Mottles, 0-0% ; Sandy medium clay (Light); Massive 
	grade of structure; Earthy fabric; Moderately moist; Weak consistence; 20-50%, medium 
	gravelly, 6-20mm, subangular, dispersed, Quartz, coarse fragments; Few, medium (2-5mm) 
	roots; Clear, Wavy change to - 
	D1	0.65 - 0.9 m	Light yellowish brown (2.5Y6/4-Moist); Mottles, 0-0% ; Mottles, 0-0% ; Clayey sand; Massive 
	grade of structure; Earthy fabric; Moderately moist; Weak consistence; 2-10%, fine gravelly, 2-
	6mm, angular, dispersed, Quartz, coarse fragments; Few, fine (1-2mm) roots; Clear, Wavy 
	change to - 
	D2	0.9 - 1.2 m	Light yellowish brown (2.5Y6/4-Moist); Mottles, 0-0% ; Mottles, 0-0% ; Clayey coarse sand; 
	Single grain grade of structure; Sandy (grains prominent) fabric; Moderately moist; Loose 
	consistence; 50-90%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; 
	Few, very fine (0-1mm) roots; 
	D2	1.2 - 1.5 m	Light yellowish brown (2.5Y6/4-Moist); Mottles, 0-0% ; Mottles, 0-0% ; Clayey coarse sand; 
	Single grain grade of structure; Sandy (grains prominent) fabric; Moderately moist; Loose 
	consistence; 50-90%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; 
	Few, very fine (0-1mm) roots; 
	Morphological Notes
	Observation Notes
	300-600MM ROUNDED GRAVEL OCCUR'S AT BASE:                                                                               
	Site Notes

	Project Name:	Regional
	Project Code:	REG	Site ID:	T363	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04	5.9A	 0.039A	 2.6H	 1.24	 0.31	 0.03	 0.24F	 4.5A	 4.4F	0.67
	 8.1C	0.37
	0.04 - 0.1	6A	 0.021A
	0.1 - 0.15	5.7A	 0.016A	 0.9H	 0.65	 0.11	 0.02	 0.89F	 2.8A	 2.6F	0.71
	 5.4C	0.37
	0.15 - 0.2	6A	 0.01A
	0.2 - 0.27	6A	 0.013A
	0.27 - 0.3	5.8A	 0.015A
	0.3 - 0.6	5.9A	 0.011A	 0.7H	 0.75	 0.14	 0.04	 1.54F	 3.2A	 3.2F	1.25
	 5.7C	0.70
	0.6 - 0.65	5.5A	 0.009A
	0.65 - 0.9	5.9A	 0.008A
	0.9 - 1.2	6A	 0.008A
	1.2 - 1.5	6.1A	 0.009A	 0.8H	 1.02	 0.12	 0.04	 0.58F	 2.6A	 2.6F	1.54
	 3.9C	1.03
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04	 2.44C	 7B	 0.015A	 0.13A	 3A	 10	 40A	 25	 21	 14
	0.04 - 0.1	 7	 34A	 27	 23	 16
	0.1 - 0.15	 1.18C	 5B	 0.07A	 6	 32A	 27	 24	 17
	0.15 - 0.2	 6	 28A	 28	 24	 20
	0.2 - 0.27	 0.71C	 0.05A	 30A	 27	 23	 20
	0.27 - 0.3	 8	 31A	 26	 21	 22
	0.3 - 0.6	 0.45C	 3B	 0.011A	 3.08A	 15	 38A	 21	 17	 24
	0.6 - 0.65	 27	 45A	 17	 13	 24
	0.65 - 0.9	 9	 52A	 19	 11	 18
	0.9 - 1.2	 4	 58A	 18	 10	 14
	1.2 - 1.5	 0.12C	 23	 58A	 16	 10	 15
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.04
	0.04 - 0.1
	0.1 - 0.15
	0.15 - 0.2
	0.2 - 0.27
	0.27 - 0.3
	0.3 - 0.6
	0.6 - 0.65
	0.65 - 0.9
	0.9 - 1.2
	1.2 - 1.5

	Project Name:	Regional
	Project Code:	REG	Site ID:	T363	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_FE	Total element - Fe(%) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	9H1	Phosphate retention
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)