Project Name:	Regional
	Project Code:	REG	Site ID:	T371	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	22/11/83	Elevation:	 20 metres
	Map Ref.:	Sheet No. : 8161   1:100000	Rainfall:	2250
	Northing/Long.:	146.056944444445	Runoff:	Very slow
	Easting/Lat.:	-18.3361111111111	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  QA	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0.5 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Subnatric Grey Sodosol     	Principal Profile Form:	Dy3.41
	ASC Confidence:	Great Soil Group:	Soloth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Melaleuca viridiflora, Angophora costata
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.07 m	Grey (10YR5/1-Moist); Mottles, 0-0% ; Mottles, 0-0% ; Sandy clay loam (Light); Massive grade of 
	structure; Earthy fabric; Moderately moist; Very weak consistence; Few, very fine (0-1mm) roots; 
	Clear, Smooth change to - 
	A2cb	0.07 - 0.1 m	Light grey (10YR7/2-Moist); White (10YR8/2-Dry); Mottles, 10YR78, 10-20% , 5-15mm, Distinct; 
	Mottles, 10-20% , 5-15mm, Distinct; Fine sandy clay loam; Massive grade of structure; Earthy 
	fabric; Moderately moist; Very weak consistence; Few, very fine (0-1mm) roots; 
	A2cb	0.1 - 0.2 m	Light grey (10YR7/2-Moist); White (10YR8/2-Dry); Mottles, 10YR78, 10-20% , 5-15mm, Distinct; 
	Mottles, 10-20% , 5-15mm, Distinct; Fine sandy clay loam; Massive grade of structure; Earthy 
	fabric; Moderately moist; Very weak consistence; Few, very fine (0-1mm) roots; Clear, Wavy 
	change to - 
	B1	0.2 - 0.25 m	Light brownish grey (10YR6/2-Moist); Mottles, 10YR68, 20-50% , 5-15mm, Distinct; Mottles, 20-
	50% , 5-15mm, Distinct; Light medium clay; Moderate grade of structure, 5-10 mm, Subangular 
	blocky; Smooth-ped fabric; Moderately moist; Firm consistence; Few, fine (1-2mm) roots; 
	Diffuse, Smooth change to - 
	B21	0.25 - 0.3 m	Light brownish grey (2.5Y6/2-Moist); Mottles, 10YR68, 10-20% , 0-5mm, Distinct; Mottles, 10-
	20% , 0-5mm, Distinct; Medium clay; Moderate grade of structure, 10-20 mm, Angular blocky; 
	Smooth-ped fabric; Moderately moist; Very firm consistence; Few, fine (1-2mm) roots; 
	B21	0.3 - 0.6 m	Light brownish grey (2.5Y6/2-Moist); Mottles, 10YR68, 10-20% , 0-5mm, Distinct; Mottles, 10-
	20% , 0-5mm, Distinct; Medium clay; Moderate grade of structure, 10-20 mm, Angular blocky; 
	Smooth-ped fabric; Moderately moist; Very firm consistence; Few, fine (1-2mm) roots; Diffuse, 
	Broken change to - 
	B2b	0.6 - 0.9 m	Grey (5Y6/1-Moist); Mottles, 10YR58, 2-10% , 0-5mm, Distinct; Mottles, 2-10% , 0-5mm, Distinct;
	 Heavy clay; Moderate grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; 
	Moderately moist; Very strong consistence; 20-50%, coarse gravelly, 20-60mm, subangular, 
	dispersed, Quartz, coarse fragments; 
	B2b	0.9 - 1 m	Grey (5Y6/1-Moist); Mottles, 10YR58, 2-10% , 0-5mm, Distinct; Mottles, 2-10% , 0-5mm, Distinct;
	 Heavy clay; Moderate grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; 
	Moderately moist; Very strong consistence; 20-50%, coarse gravelly, 20-60mm, subangular, 
	dispersed, Quartz, coarse fragments; 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T371	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Observation Notes
	ROUNDED GN GV STOPPED AUGER:VERY DENSE B23/D ALSO BLEACHED VERTICALLY:                                                  
	Site Notes
	Morphological Notes

	Project Name:	Regional
	Project Code:	REG	Site ID:	T371	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.07	5.5A	 0.04A	 1.57H	 0.67	 0.15	 0.06	 0.09F	 2.9A	 2.5F	2.07
	 3.4C	1.76
	0.07 - 0.1	5.4A	 0.024A
	0.1 - 0.2	5.4A	 0.015A	 0.5H	 0.53	 0.07	 0.1	 0.14F	 2A	 1.3F	5.00
	 1C	10.00
	0.2 - 0.25	5.8A	 0.017A	 1.1H	 1.6	 0.1	 0.23	 0.45F	 4.1A	 3.5F	5.61
	 4.7C	4.89
	0.25 - 0.3	5.7A	 0.018A
	0.3 - 0.6	5.6A	 0.024A	 1.71H	 3.46	 0.06	 0.5	 1.18F	 7A	 6.9F	7.14
	 8.9C	5.62
	0.6 - 0.9	5.8A	 0.052A
	0.9 - 1	5.8A	 0.058A	 2.43H	 5.49	 0.04	 1.28	 0.88F	 10.7A	 10.1F	11.96
	 11.5C	11.13
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.07	 1.23C	 5B	 0.004A	 0.06A	 2.61A	 1	 26A	 37	 29	 8
	0.07 - 0.1	 8	 24A	 39	 31	 7
	0.1 - 0.2	 0.25C	 5B	 1	 25A	 38	 29	 9
	0.2 - 0.25	 0.27C	 2B	 0.02A	 1	 21A	 28	 24	 28
	0.25 - 0.3	 1	 17A	 21	 24	 38
	0.3 - 0.6	 0.28C	 2B	 0.003A	 1.86A	 2	 16A	 23	 25	 36
	0.6 - 0.9	 1	 14A	 29	 27	 31
	0.9 - 1	 0.12C	 0.001A	 2.3A	 1	 12A	 27	 31	 30
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.07
	0.07 - 0.1
	0.1 - 0.2
	0.2 - 0.25
	0.25 - 0.3
	0.3 - 0.6
	0.6 - 0.9
	0.9 - 1

	Project Name:	Regional
	Project Code:	REG	Site ID:	T371	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_FE	Total element - Fe(%) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	9H1	Phosphate retention
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)