Project Name:	Regional
	Project Code:	REG	Site ID:	T377	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	23/11/83	Elevation:	 30 metres
	Map Ref.:	Sheet No. : 8061   1:100000	Rainfall:	2250
	Northing/Long.:	145.970833333333	Runoff:	Very slow
	Easting/Lat.:	-18.2458333333333	Drainage:	Moderately well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  QA	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	5 metres
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mesotrophic Dermosolic Redoxic Hydrosol     	Principal Profile Form:	Uf6.41
	ASC Confidence:	Great Soil Group:	No suitable group
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Imperata cylindrica
	Tall Strata - Tree, 20.01-35m, Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Very dark greyish brown (10YR3/2-Moist); Light brownish grey (10YR6/2-Dry); Mottles, 0-0% ; 
	Mottles, 0-0% ; Silty medium clay; Moderate grade of structure, 2-5 mm, Subangular blocky; 
	Smooth-ped fabric; Moderately moist; Very weak consistence; Many, fine (1-2mm) roots; 
	A1	0.1 - 0.12 m	Very dark greyish brown (10YR3/2-Moist); Light brownish grey (10YR6/2-Dry); Mottles, 0-0% ; 
	Mottles, 0-0% ; Silty medium clay; Moderate grade of structure, 2-5 mm, Subangular blocky; 
	Smooth-ped fabric; Moderately moist; Very weak consistence; Many, fine (1-2mm) roots; Clear, 
	Smooth change to - 
	B21	0.12 - 0.2 m	Brownish yellow (10YR6/8-Moist); Mottles, 10YR62, 20-50% , 5-15mm, Distinct; Mottles, 20-50%
	 , 5-15mm, Distinct; Medium clay; Moderate grade of structure, 5-10 mm, Subangular blocky; 
	Smooth-ped fabric; Moderately moist; Weak consistence; Many, fine (1-2mm) roots; 
	B21	0.2 - 0.25 m	Brownish yellow (10YR6/8-Moist); Mottles, 10YR62, 20-50% , 5-15mm, Distinct; Mottles, 20-50%
	 , 5-15mm, Distinct; Medium clay; Moderate grade of structure, 5-10 mm, Subangular blocky; 
	Smooth-ped fabric; Moderately moist; Weak consistence; Many, fine (1-2mm) roots; Clear, 
	Smooth change to - 
	B22	0.25 - 0.3 m	Light brownish grey (10YR6/2-Moist); Mottles, 10YR68, 10-20% , 5-15mm, Distinct; Mottles, 10-
	20% , 5-15mm, Distinct; Medium clay; Moderate grade of structure, 5-10 mm, Subangular blocky;
	 Smooth-ped fabric; Moderately moist; Firm consistence; Many, fine (1-2mm) roots; 
	B22	0.3 - 0.5 m	Light brownish grey (10YR6/2-Moist); Mottles, 10YR68, 10-20% , 5-15mm, Distinct; Mottles, 10-
	20% , 5-15mm, Distinct; Medium clay; Moderate grade of structure, 5-10 mm, Subangular blocky;
	 Smooth-ped fabric; Moderately moist; Firm consistence; Many, fine (1-2mm) roots; Diffuse, 
	Wavy change to - 
	B23/2b	0.5 - 0.6 m	Light brownish grey (10YR6/2-Moist); White (10YR8/1-Dry); Mottles, 10YR68, 10-20% , 5-15mm, 
	Distinct; Mottles, 10-20% , 5-15mm, Distinct; Medium heavy clay; Moderate grade of structure, 5-
	10 mm, Subangular blocky; Smooth-ped fabric; Moderately moist; Firm consistence; Common 
	(10 - 20 %), Manganiferous, Medium (2 -6 mm), Soft segregations; Common, fine (1-2mm) roots; 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T377	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B23/2b	0.6 - 0.9 m	Light brownish grey (10YR6/2-Moist); White (10YR8/1-Dry); Mottles, 10YR68, 10-20% , 5-15mm, 
	Distinct; Mottles, 10-20% , 5-15mm, Distinct; Medium heavy clay; Moderate grade of structure, 5-
	10 mm, Subangular blocky; Smooth-ped fabric; Moderately moist; Firm consistence; Common 
	(10 - 20 %), Manganiferous, Medium (2 -6 mm), Soft segregations; Common, fine (1-2mm) roots; 
	Diffuse, Wavy change to - 
	B24/2b	0.9 - 1.2 m	Light brownish grey (10YR6/2-Moist); Mottles, 10YR68, 10-20% , 0-5mm, Distinct; Mottles, 10-
	20% , 0-5mm, Distinct; Heavy clay; Moderate grade of structure, 10-20 mm, Angular blocky; 
	Smooth-ped fabric; Moderately moist; Very firm consistence; Very few (0 - 2 %), Manganiferous, 
	Fine (0 - 2 mm), Soft segregations; Common, fine (1-2mm) roots; Diffuse, Wavy change to - 
	B25/2b	1.2 - 1.5 m	Light brownish grey (10YR6/2-Moist); Mottles, 10YR68, 20-50% , 15-30mm, Prominent; Mottles, 
	20-50% , 15-30mm, Prominent; Heavy clay; Moderate grade of structure, 5-10 mm, Subangular 
	blocky; Smooth-ped fabric; Moderately moist; Strong consistence; Common (10 - 20 %), 
	Manganiferous, Medium (2 -6 mm), Soft segregations; Few, fine (1-2mm) roots; 
	B25/2b	1.5 - 1.8 m	Light brownish grey (10YR6/2-Moist); Mottles, 10YR68, 20-50% , 15-30mm, Prominent; Mottles, 
	20-50% , 15-30mm, Prominent; Heavy clay; Moderate grade of structure, 5-10 mm, Subangular 
	blocky; Smooth-ped fabric; Moderately moist; Strong consistence; Common (10 - 20 %), 
	Manganiferous, Medium (2 -6 mm), Soft segregations; Few, fine (1-2mm) roots; 
	B25/2b	1.8 - 2 m	Light brownish grey (10YR6/2-Moist); Mottles, 10YR68, 20-50% , 15-30mm, Prominent; Mottles, 
	20-50% , 15-30mm, Prominent; Heavy clay; Moderate grade of structure, 5-10 mm, Subangular 
	blocky; Smooth-ped fabric; Moderately moist; Strong consistence; Common (10 - 20 %), 
	Manganiferous, Medium (2 -6 mm), Soft segregations; Few, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	VERTICAL MOTTLING IN 12-20CM DEPTH:MN DOMINATE IN Y MOTTLE:                                                             
	Site Notes

	Project Name:	Regional
	Project Code:	REG	Site ID:	T377	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.9A	 0.045A	 3.43H	 1.8	 0.28	 0.24	 0.68F	 6.9A	 6.4F	3.48
	 13.5C	1.78
	0.1 - 0.12	5.7A	 0.036A
	0.12 - 0.2	5.7A	 0.03A	 1.38H	 1.46	 0.07	 0.25	 1.23F	 5.3A	 4.4F	4.72
	 10.3C	2.43
	0.2 - 0.25	5.8A	 0.031A
	0.25 - 0.3	5.8A	 0.029A
	0.3 - 0.5	6A	 0.021A	 0.69H	 1.4	 0.1	 0.31	 1.17F	 4.1A	 3.5F	7.56
	 7.4C	4.19
	0.5 - 0.6	6.2A	 0.018A
	0.6 - 0.9	6.3A	 0.018A	 0.68H	 1.67	 0.07	 0.45	 1.23F	 4.5A	 4.4F	10.00
	 9.1C	4.95
	0.9 - 1.2	6.4A	 0.019A	 0.67H	 2.19	 0.08	 0.26	 0.89F	 4.8A	 4.1F	5.42
	 4.4C	5.91
	1.2 - 1.5	6.1A	 0.033A	 0.7H	 2.11	 0.07	 0.76	 1.49F	 5.8A	 5.1F	13.10
	 6.5C	11.69
	1.5 - 1.8	5.8A	 0.051A	 1.26F	 5.4C
	1.8 - 2	5.6A	 0.072A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 2.71C	 13B	 0.02A	 0.19A	 2.2A	 0	 4A	 24	 42	 30
	0.1 - 0.12	 2
	0.12 - 0.2	 1.06C	 4B	 0.011A	 0.08A	 2.04A	 0	 2A	 22	 43	 33
	0.2 - 0.25	 0	 2A	 23	 40	 34
	0.25 - 0.3	 0	 2A	 23	 40	 35
	0.3 - 0.5	 0.39C	 2	 3A	 25	 35	 37
	0.5 - 0.6	 2	 4A	 24	 34	 38
	0.6 - 0.9	 0.31C	 0.008A	 1.26A	 2	 3A	 23	 33	 41
	0.9 - 1.2	 3	 7A	 24	 32	 37
	1.2 - 1.5	 0.1C	 0.003A	 1.58A	 5	 10A	 23	 31	 35
	1.5 - 1.8	 1	 7A	 33	 30	 31
	1.8 - 2	 0	 6A	 39	 26	 30
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.12
	0.12 - 0.2
	0.2 - 0.25
	0.25 - 0.3
	0.3 - 0.5
	0.5 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8

	Project Name:	Regional
	Project Code:	REG	Site ID:	T377	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	1.8 - 2

	Project Name:	Regional
	Project Code:	REG	Site ID:	T377	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_FE	Total element - Fe(%) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6B3	Total organic carbon - high frequency induction furnace, infrared
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	9H1	Phosphate retention
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)