Project Name:	Regional
	Project Code:	REG	Site ID:	T39	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.F. Isbell	Locality:	5.3KM north east of BlooT bury on Midge Pt. 
	Road:approx 274M past houseon right:
	Date Desc.:	07/10/64	Elevation:	 152 metres
	Map Ref.:	Sheet No. : 8656   1:100000	Rainfall:	1524
	Northing/Long.:	148.629166666667	Runoff:	Moderately rapid
	Easting/Lat.:	-20.6708333333333	Drainage:	No Data
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Pla	Substrate Material:	Existing vertical exposure, 0.8 m 
	deep,Andesite 
	Land Form
	Rel/Slope Class: 	Rolling rises 9-30m 10-32%	Pattern Type:	Low hills
	Morph. Type:	No Data	Relief:	30 metres
	Elem. Type:	Hillcrest	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Eutrophic Brown Dermosol     	Principal Profile Form:	Gn3.21
	ASC Confidence:	Great Soil Group:	Prairie soil
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - None recorded
	Mid Strata - Tree, 1.01-3m, Very sparse. *Species includes - Planchonia careya
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus tessellaris, Eucalyptus tereticornis, Eucalyptus 
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.13 m	Very dark brown (10YR2/2-Moist); Very dark grey (10YR3/1-Dry); , 0-0% ; , 0-0% ; Loam (Heavy); 
	Strong grade of structure, 5-10 mm, Angular blocky; Strong grade of structure, 2-5 mm, Granular;
	 Moist; Weak consistence; 0-2%, medium gravelly, 6-20mm, Gravel, coarse fragments; Gradual 
	change to - 
	A2	0.13 - 0.28 m	Dark brown (7.5YR3/4-Moist); Strong brown (7.5YR4/6-Dry); , 7.5YR42, 2-10% , Distinct; , 
	7.5YR45, 2-10% , Distinct; Clay loam (Heavy); Strong grade of structure, 5-10 mm, Angular 
	blocky; Strong grade of structure, 2-5 mm, Granular; Moist; Weak consistence; 2-10%, coarse 
	gravelly, 20-60mm, Gravel, coarse fragments; Many (20 - 50 %), Ferromanganiferous, Fine (0 - 2 
	mm), ; Gradual change to - 
	B1	0.28 - 0.48 m	Strong brown (7.5YR4/5-Moist); Strong brown (7.5YR4/8-Dry); , 0-0% ; , 0-0% ; Light clay; 
	Moderate grade of structure, 5-10 mm, Angular blocky; Smooth-ped fabric; Moist; Weak 
	consistence; 0-2%, fine gravelly, 2-6mm, Gravel, coarse fragments; Common (10 - 20 %), 
	Ferromanganiferous, Fine (0 - 2 mm), ; Gradual change to - 
	B2	0.48 - 0.66 m	Strong brown (7.5YR4/6-Moist); , 2.5YR58, 2-10% , Faint; , 2-10% , Faint; Light medium clay; 
	Moderate grade of structure, 5-10 mm, Angular blocky; Smooth-ped fabric; Moist; Firm 
	consistence; 2-10%, Sand, coarse fragments; Few (2 - 10 %), Ferromanganiferous, , ; Gradual 
	change to - 
	C	0.66 - 0.79 m	Strong brown (7.5YR4/8-Moist); , 2.5YR58, 10-20% , Distinct; , 10-20% , Distinct; Light clay; 10-
	20%, Sand, coarse fragments; 
	0.79 - 0.89 m	; 
	Morphological Notes
	Much soft weathered volcanic rock:
	Observation Notes
	SOME MIXING OF A AN B HORIZON IN A2:B1 HAS PATCHES OF DB CL/LC FROM UPPER HORIZON:                                      
	Site Notes

	Project Name:	Regional
	Project Code:	REG	Site ID:	T39	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	BLOOMSBURY

	Project Name:	Regional
	Project Code:	REG	Site ID:	T39	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	6.2A	 0.029A	 10.8B	 4.3	 0.14	 0.01	 22C	0.05
	0.13 - 0.28	5.9A	 0.029A
	0.28 - 0.48	6.1A	<0.03A	 6.4B	 3.9	 0.06	 0.01	 14C	0.07
	0.48 - 0.66	6.2A	<0.03A	 9.2B	 5.6	 0.05	 0.02	 16C	0.13
	0.66 - 0.79	6.5A	<0.03A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13	 3.51D	 11B	 0.039A	 0.13A	 4	 33D	 29	 20	 20
	0.13 - 0.28	 0.74D	 5B	 0.035A	 0.04A	 8	 22D	 19	 18	 40
	0.28 - 0.48	 1B	 0.023A	 3	 18D	 20	 21	 39
	0.48 - 0.66	 0.014A	 1	 12D	 16	 16	 53
	0.66 - 0.79	<1B	 0.008A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13
	0.13 - 0.28
	0.28 - 0.48
	0.48 - 0.66
	0.66 - 0.79

	Project Name:	Regional
	Project Code:	REG	Site ID:	T39	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance