Project Name:	Regional
	Project Code:	REG	Site ID:	T393	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	M.D. Laffan	Locality:
	Date Desc.:	21/06/84	Elevation:	 800 metres
	Map Ref.:	Sheet No. : 8063   1:100000	Rainfall:	1500
	Northing/Long.:	145.576944444444	Runoff:	No Data
	Easting/Lat.:	-17.3	Drainage:	Rapidly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 CZA	Substrate Material:	Basalt 
	Land Form
	Rel/Slope Class: 	Steep low hills 30-90m 32-56%	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	53 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Dermosol     	Principal Profile Form:	Gn3.22
	ASC Confidence:	Great Soil Group:	Euchrozem
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:	Low Strata - Sod grass, 0.26-0.5m, Closed or dense. *Species includes - None recorded
	Surface Coarse Fragments:	2-10%, medium gravelly, 6-20mm, subangular, Sand
	Profile Morphology
	A	0 - 0.1 m	Dark brown (7.5YR3/2-Moist); , 0-0% ; , 0-0% ; Clay loam (Heavy); Moderate grade of structure, 2-
	5 mm, Subangular blocky; Smooth-ped fabric; Moist; Weak consistence; 0-2%, medium gravelly,
	 6-20mm, subangular, dispersed, Sand, coarse fragments; Clear change to - 
	B2	0.1 - 0.2 m	Dark brown (7.5YR3/3-Moist); , 0-0% ; , 0-0% ; Light clay; Moderate grade of structure, 5-10 mm, 
	Subangular blocky; Smooth-ped fabric; Moist; Weak consistence; 0-2%, medium gravelly, 6-
	20mm, subangular, dispersed, Sand, coarse fragments; 
	B2	0.2 - 0.3 m	Dark brown (7.5YR3/3-Moist); , 0-0% ; , 0-0% ; Light clay; Moderate grade of structure, 5-10 mm, 
	Subangular blocky; Smooth-ped fabric; Moist; Weak consistence; 0-2%, medium gravelly, 6-
	20mm, subangular, dispersed, Sand, coarse fragments; 
	B2	0.3 - 0.4 m	Dark brown (7.5YR3/3-Moist); , 0-0% ; , 0-0% ; Light clay; Moderate grade of structure, 5-10 mm, 
	Subangular blocky; Smooth-ped fabric; Moist; Weak consistence; 0-2%, medium gravelly, 6-
	20mm, subangular, dispersed, Sand, coarse fragments; Clear change to - 
	B3	0.4 - 0.6 m	Dark brown (7.5YR3/3-Moist); , 7.5YR58, 2-10% , 5-15mm, Distinct; , 2-10% , 5-15mm, Distinct; 
	Light clay; Moderate grade of structure, 5-10 mm, Subangular blocky; Smooth-ped fabric; Moist; 
	Weak consistence; 0-2%, medium gravelly, 6-20mm, subangular, dispersed, Sand, coarse 
	fragments; Clear change to - 
	BC	0.6 - 0.9 m	Dark brown (7.5YR3/4-Moist); , 7.5YR58, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, 
	Distinct; Sandy clay loam; Weak grade of structure, 2-5 mm, Subangular blocky; Smooth-ped 
	fabric; Moist; Weak consistence; 20-50%, medium gravelly, 6-20mm, subangular, dispersed, 
	Sand, coarse fragments; Gradual change to - 
	C1	0.9 - 1.2 m	Dark brown (7.5YR3/3-Moist); , 0-0% ; , 0-0% ; Sandy clay loam; Single grain grade of structure; 
	Smooth-ped fabric; Moist; Weak consistence; 90-100%, coarse gravelly, 20-60mm, subangular, 
	dispersed, Sand, coarse fragments; 
	Morphological Notes
	Observation Notes
	FORMERLY RAINFOREST (5B):PARENT MATERIAL MODERATELY WEATHERED BASALTIC SCORIA:                                  
	        
	Site Notes

	Project Name:	Regional
	Project Code:	REG	Site ID:	T393	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6D	 0.107A	 27.9H	 6.7	 2.2	 0.06	 0.15F	 17A	 37F	0.35
	7.1A	 48C	0.13
	0.1 - 0.2	7.2A	 0.065A
	0.2 - 0.3	6D	 0.054A	 28.6H	 5.06	 2.4	 0.22	 0.03F	 21.7A	 36.3F	1.01
	7.5A	 46C	0.48
	0.3 - 0.4	7.7A	 0.046A
	0.4 - 0.6	6.3D	 0.034A	 22.7H	 6.52	 3.47	 0.18	 0.61F	 14.8A	 33.5F	1.22
	8A	 37C	0.49
	0.6 - 0.9	7.9A	 0.04A
	0.9 - 1.2	8.1A	 0.036A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 4.92C	 130B	 0.37A	 6	 26A	 16	 20	 37
	0.1 - 0.2	 3.78C
	0.2 - 0.3	 99B	 7	 25A	 21	 22	 33
	0.3 - 0.4
	0.4 - 0.6	 0.45C	 35	 45A	 24	 16	 16
	0.6 - 0.9	 20	 43A	 23	 17	 18
	0.9 - 1.2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.6
	0.6 - 0.9
	0.9 - 1.2

	Project Name:	Regional
	Project Code:	REG	Site ID:	T393	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_FE	Total element - Fe(%) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4C1	pH of 1:5 soil/1M potassium chloride extract - direct
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6B3	Total organic carbon - high frequency induction furnace, infrared
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	9H1	Phosphate retention
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)