Project Name:	Regional
	Project Code:	REG	Site ID:	T397	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	M.D. Laffan	Locality:
	Date Desc.:	10/10/84	Elevation:	No Data
	Map Ref.:	Sheet No. : 7963   1:100000	Rainfall:	1400
	Northing/Long.:	145.463888888889	Runoff:	No Data
	Easting/Lat.:	-17.3166666666667	Drainage:	Poorly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  QA	Substrate Material:	Undisturbed soil core, Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	<1 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melacic Dermosolic Redoxic Hydrosol     	Principal Profile Form:	Uf6.41
	ASC Confidence:	Great Soil Group:	Humic gley
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - Sod grass, , . *Species includes - None recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.1 m	Black (10YR2/1-Moist); , 2.5YR36, 2-10% , 0-5mm, Faint; , 2-10% , 0-5mm, Faint; Silty light clay 
	(Heavy); Moderate grade of structure, 10-20 mm, Polyhedral; Moderate grade of structure, 5-10 
	mm, Granular; Smooth-ped fabric; Moist; Firm consistence; Many, fine (1-2mm) roots; 
	A11	0.1 - 0.2 m	Black (10YR2/1-Moist); , 2.5YR36, 2-10% , 0-5mm, Faint; , 2-10% , 0-5mm, Faint; Silty light clay 
	(Heavy); Moderate grade of structure, 10-20 mm, Polyhedral; Moderate grade of structure, 5-10 
	mm, Granular; Smooth-ped fabric; Moist; Firm consistence; Many, fine (1-2mm) roots; Gradual, 
	Smooth change to - 
	A12	0.2 - 0.3 m	Very dark grey (10YR3/1-Moist); , 2.5YR36, 10-20% , 0-5mm, Distinct; , 10-20% , 0-5mm, 
	Distinct; Silty light clay (Heavy); Moderate grade of structure, 10-20 mm, Subangular blocky; 
	Moderate grade of structure, 5-10 mm, Granular; Smooth-ped fabric; Moist; Firm consistence; 
	Many, fine (1-2mm) roots; Gradual, Smooth change to - 
	AB	0.3 - 0.4 m	Dark grey (10YR4/1-Moist); , 2.5YR36, 20-50% , 0-5mm, Distinct; , 20-50% , 0-5mm, Distinct; 
	Silty medium clay; Moderate grade of structure, 20-50 mm, Prismatic; Moderate grade of 
	structure, 5-10 mm, Angular blocky; Smooth-ped fabric; Moist; Firm consistence; Common, fine 
	(1-2mm) roots; Gradual, Smooth change to - 
	B1g	0.4 - 0.6 m	Grey (10YR5/1-Moist); , 7.5YR58, 20-50% , 0-5mm, Distinct; , 20-50% , 0-5mm, Distinct; Medium
	 clay; Strong grade of structure, 20-50 mm, Prismatic; Moderate grade of structure, 5-10 mm, 
	Angular blocky; Smooth-ped fabric; Moist; Firm consistence; Common, very fine (0-1mm) roots; 
	B1g	0.6 - 0.75 m	Grey (10YR5/1-Moist); , 7.5YR58, 20-50% , 0-5mm, Distinct; , 20-50% , 0-5mm, Distinct; Medium
	 clay; Strong grade of structure, 20-50 mm, Prismatic; Moderate grade of structure, 5-10 mm, 
	Angular blocky; Smooth-ped fabric; Moist; Firm consistence; Common, very fine (0-1mm) roots; 
	Gradual, Smooth change to - 
	B2g	0.75 - 0.9 m	Greyish brown (10YR5/2-Moist); , 7.5YR58, 20-50% , 0-5mm, Distinct; , 20-50% , 0-5mm, 
	Distinct; Sandy medium clay; Moderate grade of structure, 20-50 mm, Prismatic; Moderate grade
	 of structure, 5-10 mm, Angular blocky; Smooth-ped fabric; Moist; Firm consistence; Few 
	cutans, <10% of ped faces or walls coated, faint; Few, very fine (0-1mm) roots; 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T397	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B2g	0.9 - 1.2 m	Greyish brown (10YR5/2-Moist); , 7.5YR58, 20-50% , 0-5mm, Distinct; , 20-50% , 0-5mm, 
	Distinct; Sandy medium clay; Moderate grade of structure, 20-50 mm, Prismatic; Moderate grade
	 of structure, 5-10 mm, Angular blocky; Smooth-ped fabric; Moist; Firm consistence; Few 
	cutans, <10% of ped faces or walls coated, faint; Few, very fine (0-1mm) roots; Gradual, Wavy 
	change to - 
	B3g	1.2 - 1.5 m	Grey (10YR6/1-Moist); , 7.5YR58, 20-50% , 5-15mm, Distinct; , 20-50% , 5-15mm, Distinct; 
	Sandy light clay (Light); Moderate grade of structure, 20-50 mm, Prismatic; Moderate grade of 
	structure, 5-10 mm, Angular blocky; Smooth-ped fabric; Moist; Very firm consistence; 2-10%, 
	fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; Few cutans, <10% of ped faces or 
	walls coated, faint; Few, very fine (0-1mm) roots; 
	B3g	1.5 - 1.8 m	Grey (10YR6/1-Moist); , 7.5YR58, 20-50% , 5-15mm, Distinct; , 20-50% , 5-15mm, Distinct; 
	Sandy light clay (Light); Moderate grade of structure, 20-50 mm, Prismatic; Moderate grade of 
	structure, 5-10 mm, Angular blocky; Smooth-ped fabric; Moist; Very firm consistence; 2-10%, 
	fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; Few cutans, <10% of ped faces or 
	walls coated, faint; Few, very fine (0-1mm) roots; 
	B3g	1.8 - 1.9 m	Grey (10YR6/1-Moist); , 7.5YR58, 20-50% , 5-15mm, Distinct; , 20-50% , 5-15mm, Distinct; 
	Sandy light clay (Light); Moderate grade of structure, 20-50 mm, Prismatic; Moderate grade of 
	structure, 5-10 mm, Angular blocky; Smooth-ped fabric; Moist; Very firm consistence; 2-10%, 
	fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; Few cutans, <10% of ped faces or 
	walls coated, faint; Few, very fine (0-1mm) roots; Clear, Wavy change to - 
	2Bgb	1.9 - 2.1 m	Grey (10YR5/1-Moist); , 7.5YR58, 20-50% , 5-15mm, Distinct; , 20-50% , 5-15mm, Distinct; Silty 
	light clay (Heavy); Moderate grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; 
	Moist; Very firm consistence; Few cutans, <10% of ped faces or walls coated, faint; Few, very 
	fine (0-1mm) roots; 
	Morphological Notes
	Observation Notes
	PARENT MATERIAL RECENT ALLUVIUM FROM RHYOLITE AN MINOR GRANITE OVERLYING GRANITIC ALLUVIUM AT 
	75CM:                     
	Site Notes
	CARRINGTON

	Project Name:	Regional
	Project Code:	REG	Site ID:	T397	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	3.9D	 0.094A	 2.7H	 1.9	 0.48	 0.07	 2.73F	 7.5A	 7.9F	0.93
	5A	 21C	0.33
	0.1 - 0.2	5.2A	 0.033A
	0.2 - 0.3	3.9D	 0.027A	 1.55H	 1.67	 0.28	 0.17	 3.02F	 5.5A	 6.7F	3.09
	5.3A	 15C	1.13
	0.3 - 0.4	5.5A	 0.019A
	0.4 - 0.6	3.9D	 0.017A	 0.87H	 1.67	 0.26	 0.15	 2.18F	 4.5A	 5.1F	3.33
	5.6A	 8C	1.88
	0.6 - 0.75	5.7A	 0.016A
	0.75 - 0.9	4.1D	 0.016A	 0.49H	 1.34	 0.15	 0.13	 1.11F	 3.1A	 3.2F	4.19
	5.8A	 6C	2.17
	0.9 - 1.2	5.7A	 0.023A
	1.2 - 1.5	5.6A	 0.027A
	1.5 - 1.8	5.8A	 0.029A
	1.8 - 1.9	6A	 0.024A
	1.9 - 2.1	6.2A	 0.028A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 4.75C	 34B	 0.046A	 0.33A	 2.3A	 0	 2A	 10	 34	 54
	0.1 - 0.2
	0.2 - 0.3	 8B	 0	 6A	 14	 38	 42
	0.3 - 0.4
	0.4 - 0.6	 0.61C	 0.01A	 2.74A	 0	 5A	 19	 35	 41
	0.6 - 0.75
	0.75 - 0.9	 0.27C	 0.009A	 2.88A	 0	 18A	 30	 21	 32
	0.9 - 1.2
	1.2 - 1.5	 17	 50A	 14	 9	 27
	1.5 - 1.8
	1.8 - 1.9
	1.9 - 2.1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.6
	0.6 - 0.75
	0.75 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 1.9
	1.9 - 2.1

	Project Name:	Regional
	Project Code:	REG	Site ID:	T397	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4C1	pH of 1:5 soil/1M potassium chloride extract - direct
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6B3	Total organic carbon - high frequency induction furnace, infrared
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	9H1	Phosphate retention
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)