Project Name:	Regional
	Project Code:	REG	Site ID:	T4	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.F. Isbell	Locality:
	Date Desc.:	17/12/63	Elevation:	No Data
	Map Ref.:	Sheet No. : 8060   1:100000	Rainfall:	0
	Northing/Long.:	145.508333333333	Runoff:	Rapid
	Easting/Lat.:	-18.9166666666667	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 SDk	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	No Data	Relief:	23 metres
	Elem. Type:	Hillcrest	Slope Category:	Level
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Subnatric Brown Sodosol     	Principal Profile Form:	Dy2.4
	ASC Confidence:	Great Soil Group:	Solodized solonetz
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (10YR3/3-Moist); Brown (10YR5/3-Dry); , 0-0% ; , 0-0% ; Sandy loam; Massive grade 
	of structure; Dry; Strong consistence; 2-10%, medium gravelly, 6-20mm, Gravel, coarse 
	fragments; 
	A2	0.1 - 0.15 m	Brown (10YR4/3-Moist); Pale brown (10YR6/3-Dry); , 0-0% ; , 0-0% ; Sandy clay loam; Massive 
	grade of structure; Dry; Strong consistence; 20-50%, medium gravelly, 6-20mm, Gravel, coarse 
	fragments; Few (2 - 10 %), Ferromanganiferous, , Nodules; Clear change to - 
	B21	0.15 - 0.3 m	Brown (7.5YR4/2-Moist); , 0-0% ; , 0-0% ; Medium clay; Moderate grade of structure, 100-200 
	mm, Columnar; Dry; Very strong consistence; 20-50%, medium gravelly, 6-20mm, Gravel, coarse
	 fragments; Few (2 - 10 %), Ferromanganiferous, , Nodules; Abrupt change to - 
	B22	0.3 - 0.45 m	Brown (7.5YR4/2-Moist); , 0-0% ; , 0-0% ; Medium clay; Weak grade of structure, 20-50 mm, 
	Subangular blocky; Dry; Very strong consistence; 2-10%, medium gravelly, 6-20mm, Gravel, 
	coarse fragments; Common cutans, 10-50% of ped faces or walls coated, prominent; Gradual 
	change to - 
	B23	0.45 - 0.6 m	Strong brown (7.5YR4/5-Moist); , 0-0% ; , 0-0% ; Medium clay; Weak grade of structure, 20-50 
	mm, Subangular blocky; Dry; Very strong consistence; Gradual change to - 
	B23	0.6 - 0.81 m	Strong brown (7.5YR4/5-Moist); , 0-0% ; , 0-0% ; Medium clay; Weak grade of structure, 20-50 
	mm, Subangular blocky; Dry; Very strong consistence; Gradual change to - 
	BC	0.81 - 0.91 m	; 
	Morphological Notes
	BC	As above with weathered parent material.
	Observation Notes
	WEATHERED FELSPATHIC SANDSTONE FROM 60CM                                                                                
	Site Notes
	BLUE RANGE RD.

	Project Name:	Regional
	Project Code:	REG	Site ID:	T4	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.9A	 0.11A	 3.2B	 3.2	 0.38	 0.1	 8C	1.25
	0.1 - 0.15	5.5A	 0.16A	 1.6B	 4.4	 0.2	 0.3	 6C	5.00
	0.15 - 0.3	5.5A	 0.52A	 1.6B	 8.5	 0.2	 1.4	 12C	11.67
	0.3 - 0.45	7.3A	 0.729A	 1.6B	 9.5	 0.16	 2	 13C	15.38
	0.45 - 0.6	8.1A	 0.699A	 2B	 9	 0.16	 2	 11C	18.18
	0.6 - 0.81	8.3A	 0.66A	 1.5B	 9	 0.1	 2.2	 10C	22.00
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.35D	 10B	 0.034A	 0.09A	 1.04A	 20	 30D	 39	 12	 19
	0.1 - 0.15	 0.76D	 7B	 0.05A	 30	 26D	 38	 15	 21
	0.15 - 0.3	 0.66D	 8B	 0.026A	 0.06A	 1.55A	 25	 12D	 14	 14	 60
	0.3 - 0.45	 0.01A	 4B
	0.45 - 0.6	 0.04A	 4B	 0.022A	 1.8A	 10	 11D	 20	 10	 59
	0.6 - 0.81	 0.03A	 4B	 0.019A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.15
	0.15 - 0.3
	0.3 - 0.45
	0.45 - 0.6
	0.6 - 0.81

	Project Name:	Regional
	Project Code:	REG	Site ID:	T4	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	17A1	Total potassium - X-ray fluorescence
	19A1	Carbonates - rapid titration
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	MIN_EC	Exchange Capacity - Minerology
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_K2O	K2O - X-Ray Diffraction or Clay Fraction (air dry)
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction
	XRD_C_Vm	Vermiculte - X-Ray Diffraction