Project Name:	Regional
	Project Code:	REG	Site ID:	T40	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.F. Isbell	Locality:	Mirani/Calen Road:3.2KM north of Kungurri 
	School:1KM north of crest:0.6KM north of farm house:
	Date Desc.:	10/12/64	Elevation:	No Data
	Map Ref.:	Sheet No. : 8655   1:100000	Rainfall:	1778
	Northing/Long.:	148.729166666667	Runoff:	Rapid
	Easting/Lat.:	-21.0583333333333	Drainage:	No Data
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Plv	Substrate Material:	Existing vertical exposure, 0.9 m 
	deep,Andesite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Mountains
	Morph. Type:	Crest	Relief:	152 metres
	Elem. Type:	Hillcrest	Slope Category:	Steep
	Slope:	0 % 	Aspect:	350 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Dermosol     	Principal Profile Form:	Gn3.21
	ASC Confidence:	Great Soil Group:	Prairie soil
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Closed or dense. *Species includes - Panicum maximum var. trichoglume
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.18 m	Dark brown (10YR3/3-Moist); , 0-0% ; , 0-0% ; Clay loam (Light); Weak grade of structure, 5-10 
	mm, Angular blocky; Weak consistence; 2-10%, Gravel, coarse fragments; Gradual change to - 
	A2	0.18 - 0.33 m	Dark yellowish brown (10YR3/4-Moist); , 0-0% ; , 0-0% ; Clay loam (Heavy); Moderate grade of 
	structure, 5-10 mm, Angular blocky; Weak consistence; Few (2 - 10 %), Ferromanganiferous, 
	Fine (0 - 2 mm), Nodules; Gradual change to - 
	B21	0.33 - 0.53 m	Strong brown (7.5YR4/6-Moist); , 0-0% ; , 0-0% ; Light clay; Strong grade of structure, 5-10 mm, 
	Angular blocky; Smooth-ped fabric; Weak consistence; 2-10%, Sand, coarse fragments; Few (2 
	- 10 %), Ferromanganiferous, Fine (0 - 2 mm), Concretions; Gradual change to - 
	B22	0.53 - 0.76 m	Strong brown (7.5YR4/6-Moist); , 2.5YR46, 2-10% , 5-15mm, Distinct; , 2-10% , 5-15mm, 
	Distinct; Light medium clay; Strong grade of structure, 5-10 mm, Angular blocky; Smooth-ped 
	fabric; Moderately plastic; Normal plasticity; 2-10%, rounded, Sand, coarse fragments; Few (2 - 
	10 %), Ferromanganiferous, , ; Field pH 6 (pH meter); Clear change to - 
	0.76 - 0.91 m	; 
	Morphological Notes
	YB w'd an.+ some b.mn.segr.on cleavge planes:structured mc:
	Observation Notes
	Site Notes
	MACKAY

	Project Name:	Regional
	Project Code:	REG	Site ID:	T40	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.18	6.6A	 0.077A	 12.8B	 3.2	 0.35	 0.1	 23C	0.43
	0.18 - 0.33	6.3A	 0.077A
	0.33 - 0.53	6.1A	 0.041A	 13.2B	 7.1	 0.12	 0.14	 22C	0.64
	0.53 - 0.76	5.6A	 0.041A
	0.76 - 0.91	5.6A	 0.035A	 15B	 18	 0.21	 1.5
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.18	 2.29D	 27B	 0.116A	 0.22A	 0.45A	 7D	 33	 30	 30
	0.18 - 0.33	 1.57D	 0.18A
	0.33 - 0.53	 0.44D	 0.062A	 0.59A	 0.28A	 0	 9D	 29	 24	 38
	0.53 - 0.76
	0.76 - 0.91	 1B	 0.063A	 0.44A	 32D	 34	 18	 17
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.18
	0.18 - 0.33
	0.33 - 0.53
	0.53 - 0.76
	0.76 - 0.91

	Project Name:	Regional
	Project Code:	REG	Site ID:	T40	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	MIN_EC	Exchange Capacity - Minerology
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction
	XRD_C_Vm	Vermiculte - X-Ray Diffraction