Project Name:	Regional
	Project Code:	REG	Site ID:	T420	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	01/09/85	Elevation:	 670 metres
	Map Ref.:	Sheet No. : 7962   1:100000	Rainfall:	797
	Northing/Long.:	145.080555555556	Runoff:	No Data
	Easting/Lat.:	-17.7055555555556	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Fan	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Red Kandosol     	Principal Profile Form:	Gn2.1
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus dichromophloia
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.06 m	Dark reddish brown (2.5YR3/4-Moist); Red (2.5YR5/6-Dry); ; Sandy clay loam (Light); Massive 
	grade of structure; Earthy fabric; Dry; Many, fine (1-2mm) roots; Clear, Smooth change to - 
	A3	0.06 - 0.12 m	Dark red (2.5YR3/6-Moist); ; Sandy clay loam (Heavy); Massive grade of structure; Earthy fabric; 
	Dry; Many, fine (1-2mm) roots; Clear, Smooth change to - 
	B1	0.12 - 0.22 m	Dark red (2.5YR3/6-Moist); Red (2.5YR4/6-Dry); ; Clay loam; Massive grade of structure; Earthy 
	fabric; Dry; Few, fine (1-2mm) roots; Gradual, Smooth change to - 
	B21	0.22 - 0.4 m	Dark red (10R3/6-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Dry; Few, fine (1-
	2mm) roots; Gradual, Smooth change to - 
	B22	0.4 - 0.7 m	Dark red (10R3/6-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Dry; Few, fine (1-
	2mm) roots; Gradual, Smooth change to - 
	B23	0.7 - 1 m	Dark red (2.5YR3/6-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Dry; 0-2%, fine 
	gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; Few, fine (1-2mm) roots; 
	B23	1 - 1.3 m	Dark red (2.5YR3/6-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Dry; 0-2%, fine 
	gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; Few, fine (1-2mm) roots; 
	Gradual, Smooth change to - 
	B24	1.3 - 1.6 m	Dark red (2.5YR3/6-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; Dry; 0-2%, fine 
	gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; Few (2 - 10 %), Ferruginous, 
	Fine (0 - 2 mm), Nodules; 
	B24	1.6 - 1.8 m	Dark red (2.5YR3/6-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; Dry; 0-2%, fine 
	gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; Few (2 - 10 %), Ferruginous, 
	Fine (0 - 2 mm), Nodules; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Regional
	Project Code:	REG	Site ID:	T420	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06	6.9A	 0.033A	 3.2H	 0.95	 0.29	 0.03	 0.02F	 4.2A	 4.5F	0.71
	 4C	0.75
	0.06 - 0.12	6.54A	 0.029A
	0.12 - 0.22	7.2A	 0.019A
	0.22 - 0.4	6.8A	 0.011A	 1.15H	 0.6	 0.2	 0.02	 0.05F	 2A	 2F	1.00
	 2C
	0.4 - 0.7	7.12A	 0.012A
	0.7 - 1	7.06A	 0.014A	 1.75H	 0.78	 0.33	 0.02	<0.02F	 2A	 2.9F	1.00
	 3C	0.67
	1 - 1.3	7.13A	 0.011A
	1.3 - 1.6	6.54A	 0.016A	 1.33H	 0.61	 0.17	 0.02	 0.9F	 2.5A	 3F	0.80
	 3C	0.67
	1.6 - 1.8	6.95A	 0.011A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06	 1.21C	 6A	 0.016A	 0.05A	 0.16A	 2	 35D	 45	 3	 17
	 7B
	0.06 - 0.12	 2	 33D	 44	 3	 20
	0.12 - 0.22	 2	 32D	 43	 5	 20
	0.22 - 0.4	 0.24C	 3A	 0.01A	<0.01A	 0.18A	 2	 30D	 41	 4	 25
	 4B
	0.4 - 0.7	 2	 26D	 26	 3	 45
	0.7 - 1	 0.15C	 3A	 0.015A	<0.01A	 0.26A	 2	 22D	 24	 4	 50
	 3B
	1 - 1.3	 3	 22D	 29	 5	 45
	1.3 - 1.6	 0.08C	 4B	 0.012A	 0.21A
	1.6 - 1.8	 12	 27D	 32	 4	 37
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.06
	0.06 - 0.12
	0.12 - 0.22
	0.22 - 0.4
	0.4 - 0.7
	0.7 - 1
	1 - 1.3
	1.3 - 1.6
	1.6 - 1.8

	Project Name:	Regional
	Project Code:	REG	Site ID:	T420	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_FE	Total element - Fe(%) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	9H1	Phosphate retention
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance