Project Name:	Regional
	Project Code:	REG	Site ID:	T437	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	M.G. Cannon	Locality:	6.5KM E.S.E. of Murrigal siding between Bedford 
	Creek and Murray River:
	Date Desc.:	23/09/85	Elevation:	No Data
	Map Ref.:	Sheet No. : 8061   1:100000	Rainfall:	4000
	Northing/Long.:	145.969444444444	Runoff:	No runoff
	Easting/Lat.:	-18.0777777777778	Drainage:	Rapidly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qr	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Beach ridge plain
	Morph. Type:	Ridge	Relief:	4 metres
	Elem. Type:	Beach ridge	Slope Category:	Level
	Slope:	<1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melacic Regolithic Chernic Tenosol     	Principal Profile Form:	Uc5.2
	ASC Confidence:	Great Soil Group:	Earthy sand
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, Mid-dense. *Species includes - Eucalyptus pellita
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Black (10YR2/1-Moist); ; Loamy sand (Sapric); Weak grade of structure, <2 mm, Cast; Earthy 
	fabric; Dry; Loose consistence; Common, very fine (0-1mm) roots; Diffuse change to - 
	0.1 - 0.2 m	Black (10YR2/1-Moist); ; Loamy sand (Sapric); Weak grade of structure, <2 mm, Cast; Earthy 
	fabric; Loose consistence; Common, very fine (0-1mm) roots; Diffuse change to - 
	0.2 - 0.3 m	Black (10YR2/1-Moist); ; Loamy sand (Sapric); Massive grade of structure; Earthy fabric; Loose 
	consistence; Few, very fine (0-1mm) roots; Diffuse change to - 
	A3	0.3 - 0.47 m	Very dark grey (10YR3/1-Moist); ; Loamy sand; Massive grade of structure; Earthy fabric; Dry; 
	Loose consistence; Few, fine (1-2mm) roots; Diffuse, Tongued change to - 
	AB	0.47 - 0.77 m	Light brownish grey (10YR6/2-Moist); , 10YR76, 20-50% , 15-30mm, Distinct; , 20-50% , 15-
	30mm, Distinct; Clayey sand; Massive grade of structure; Smooth-ped fabric; Dry; Loose 
	consistence; Few, very fine (0-1mm) roots; Diffuse, Tongued change to - 
	B21	0.77 - 1.03 m	Yellow (10YR7/8-Moist); , 7.5YR68, 2-10% , 5-15mm, Distinct; , 10YR62, 2-10% , 5-15mm, 
	Distinct; Clayey sand; Massive grade of structure; Smooth-ped fabric; Dry; Loose consistence; 
	Diffuse change to - 
	1.03 - 1.33 m	Yellow (10YR7/8-Moist); , 7.5YR68, 2-10% , 5-15mm, Distinct; , 10YR81, 2-10% , 5-15mm, 
	Distinct; Clayey sand; Massive grade of structure; Smooth-ped fabric; Loose consistence; 
	Diffuse change to - 
	B22c	1.33 - 1.6 m	White (10YR8/1-Moist); , 10YR78, 10-20% , 15-30mm, Distinct; , 10YR68, 10-20% , 15-30mm, 
	Distinct; Clayey sand; Massive grade of structure; Smooth-ped fabric; Dry; Loose consistence; 
	Diffuse change to - 
	B23c	1.6 - 1.7 m	Yellow (10YR7/8-Moist); , 7.5YR68, 10-20% , 15-30mm, Distinct; , 10YR81, 10-20% , 15-30mm, 
	Distinct; Clayey sand; Massive grade of structure; Smooth-ped fabric; Dry; Loose consistence; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Regional
	Project Code:	REG	Site ID:	T437	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	SE OF TULL601

	Project Name:	Regional
	Project Code:	REG	Site ID:	T437	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.16A	 0.047A	 0.27H	 0.31	 0.13	 0.1	 2.44F	 2.8A	 3.3F	3.57
	 10C	1.00
	0.1 - 0.2	5A	 0.037A
	0.2 - 0.3	5.07A	 0.034A
	0.3 - 0.47	4.9A	 0.017A	<0.02H	 0.02	 0.02	 0.05	 1.46F	 1.8A	 1.6F	2.78
	 5C	1.00
	0.47 - 0.77
	0.77 - 1.03	5.38A	 0.011A	<0.02H	 0.31	 0.02	 0.06	 0.64F	 1.7A	 1.1F	3.53
	 1C	6.00
	1.03 - 1.33	5.44A	 0.01A
	1.33 - 1.6	5.01A	 0.022A	<0.02H	 0.31	 0.02	 0.07	 0.65F	 2.1A	 1.1F	3.33
	 1C	7.00
	1.6 - 1.7	5.56A	 0.013A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 4.52C	 4A	 0.012A	 0.15A	 0.46A	 0	 46D	 35	 7	 12
	 5B
	0.1 - 0.2	 0	 37D	 45	 7	 11
	0.2 - 0.3	 0	 39D	 43	 7	 11
	0.3 - 0.47	 1.97C	 4B	 0.008A	 0.06A	 0.49A	 0	 43D	 42	 4	 11
	0.47 - 0.77
	0.77 - 1.03	 0.17C	 2A	 0.006A	<0.01A	 0.5A	 1	 39D	 16	 4	 12
	 6B
	1.03 - 1.33	 1	 32D	 51	 5	 12
	1.33 - 1.6	 0.09C	 2A	 0.006A	 0.49A	 1	 38D	 47	 3	 12
	 3B
	1.6 - 1.7	 1	 34D	 52	 2	 12
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.47
	0.47 - 0.77
	0.77 - 1.03
	1.03 - 1.33
	1.33 - 1.6
	1.6 - 1.7

	Project Name:	Regional
	Project Code:	REG	Site ID:	T437	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_FE	Total element - Fe(%) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	9H1	Phosphate retention
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance