Project Name:	Regional
	Project Code:	REG	Site ID:	T441	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	23/09/85	Elevation:	No Data
	Map Ref.:	Sheet No. : 8062   1:100000	Rainfall:	3500
	Northing/Long.:	145.831944444444	Runoff:	Very slow
	Easting/Lat.:	-17.8930555555556	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qa	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Open depression (vale)	Relief:	No Data
	Elem. Type:	Drainage depression	Slope Category:	Level
	Slope:	<1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm, Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melacic Dystrophic Yellow Kandosol     	Principal Profile Form:	Gn2.61
	ASC Confidence:	Great Soil Group:	No suitable group
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Tristania sauveolens
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.1 m	Black (10YR2/1-Moist); ; Loam (Sapric); Weak grade of structure, 2-5 mm, Cast; Common (1-5 
	per 100mm2) Very fine (0.075-1mm) macropores, Moist; Very weak consistence; 
	0.1 - 0.22 m	Black (10YR2/1-Moist); ; Loam (Sapric); Weak grade of structure, 2-5 mm, Cast; Common (1-5 
	per 100mm2) Very fine (0.075-1mm) macropores, Very weak consistence; Diffuse change to - 
	A3	0.22 - 0.47 m	Dark greyish brown (10YR4/2-Moist); ; Sandy clay loam; Massive grade of structure; Common (1-
	5 per 100mm2) Very fine (0.075-1mm) macropores, Moist; Weak consistence; Clear change to - 
	AB	0.47 - 0.61 m	Brownish yellow (10YR6/6-Moist); , 10YR42, 20-50% , 5-15mm, Distinct; , 20-50% , 5-15mm, 
	Distinct; Clay loam, sandy; Massive grade of structure; Common (1-5 per 100mm2) Very fine 
	(0.075-1mm) macropores, Moist; Weak consistence; Clear change to - 
	B21	0.61 - 0.9 m	Olive yellow (2.5Y6/6-Moist); , 2.5YR58, 2-10% , 0-5mm, Distinct; , 2-10% , 0-5mm, Distinct; 
	Light medium clay; Massive grade of structure; Common (1-5 per 100mm2) Very fine (0.075-
	1mm) macropores, Moist; Weak consistence; Gradual change to - 
	B22	0.9 - 1.24 m	Olive yellow (2.5Y6/6-Moist); , 2.5YR58, 2-10% , 0-5mm, Distinct; , 2-10% , 0-5mm, Distinct; 
	Sandy medium clay; Massive grade of structure; Common (1-5 per 100mm2) Very fine (0.075-
	1mm) macropores, Moist; Weak consistence; Diffuse change to - 
	B23	1.24 - 1.54 m	Olive yellow (2.5Y6/6-Moist); , 10R48, 2-10% , 0-5mm, Prominent; , 2-10% , 0-5mm, Prominent; 
	Medium clay; Moderate grade of structure, 2-5 mm, Angular blocky; Few (<1 per 100mm2) Very 
	fine (0.075-1mm) macropores, Moist; Weak consistence; 0-2%, fine gravelly, 2-6mm, angular, 
	dispersed, Quartz, coarse fragments; Diffuse change to - 
	B24	1.54 - 1.8 m	Light brownish grey (2.5Y6/3-Moist); , 10R48, 10-20% , 0-5mm, Prominent; , 10-20% , 0-5mm, 
	Prominent; Medium clay; Strong grade of structure, 2-5 mm, Angular blocky; Few (<1 per 
	100mm2) Very fine (0.075-1mm) macropores, Moist; Weak consistence; 0-2%, fine gravelly, 2-
	6mm, angular, dispersed, Quartz, coarse fragments; 
	Morphological Notes
	Observation Notes
	HUMIC WORM CASTS TO 90CM                                                                                                
	Site Notes

	Project Name:	Regional
	Project Code:	REG	Site ID:	T441	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)

	Project Name:	Regional
	Project Code:	REG	Site ID:	T441	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.95A	 0.064A	<0.02H	 0.24	 0.11	 0.16	 2.67F	 2A	 3.2F	8.00
	 13C	1.23
	0.1 - 0.22	4.98A	 0.031A
	0.22 - 0.47	5.09A	 0.022A	<0.02H	 0.06	 0.03	<0.02	 1.56F	 2.4A	 1.7F
	 6C
	0.47 - 0.61	5.15A	 0.015A
	0.61 - 0.9	5.01A	 0.015A	<0.02H	 0.05	<0.02	<0.02	 1.54F	 2.3A	 1.7F
	 4C
	0.9 - 1.24	4.8A	 0.018A
	1.24 - 1.54	4.85A	 0.018A	<0.02H	 0.07	<0.02	<0.02	 1.02F	 2A	 1.2F
	 2C
	1.54 - 1.8	4.82A	 0.017A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 5.42C	 10A	 0.043A	 0.26A	 0.13A	 1	 35D	 18	 11	 36
	 11B
	0.1 - 0.22	 1	 41D	 16	 9	 34
	0.22 - 0.47	 1.86C	 6B	 0.03A	 0.09A	 0.11A	 3	 36D	 19	 10	 35
	0.47 - 0.61	 2	 36D	 17	 10	 37
	0.61 - 0.9	 0.75C	<1A	 0.026A	 0.02A	 0.11A	 4	 36D	 16	 8	 40
	 5B
	0.9 - 1.24	 8	 39D	 17	 8	 36
	1.24 - 1.54	 0.21C	<1A	 0.026A	 0.15A	 6	 39D	 17	 6	 38
	 7B
	1.54 - 1.8	 4	 30D	 14	 13	 42
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.22
	0.22 - 0.47
	0.47 - 0.61
	0.61 - 0.9
	0.9 - 1.24
	1.24 - 1.54
	1.54 - 1.8

	Project Name:	Regional
	Project Code:	REG	Site ID:	T441	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_FE	Total element - Fe(%) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	9H1	Phosphate retention
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance