Project Name:	Regional
	Project Code:	REG	Site ID:	T442	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	M.G. Cannon	Locality:	1.2KM down Scougall Road off Tully Cardstone Road:
	Date Desc.:	23/09/85	Elevation:	No Data
	Map Ref.:	Sheet No. : 8062   1:100000	Rainfall:	3500
	Northing/Long.:	145.845833333333	Runoff:	Slow
	Easting/Lat.:	-17.9041666666667	Drainage:	Well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qa	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	<1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Dystrophic Red Dermosol     	Principal Profile Form:	Gn3.11
	ASC Confidence:	Great Soil Group:	No suitable group
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:
	Tall Strata - Tree, 12.01-20m, Closed or dense. *Species includes - Acacia species, Acacia mangium
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.12 m	Dark brown (7.5YR3/2-Moist); ; Clay loam; Moderate grade of structure, 2-5 mm, Cast; Few (<1 
	per 100mm2) Very fine (0.075-1mm) macropores, Very few (0 - 2 %), Manganiferous, Fine (0 - 2 
	mm), Nodules; Common, fine (1-2mm) roots; Diffuse change to - 
	A12	0.12 - 0.25 m	Dark reddish brown (2.5YR3/3-Moist); ; Clay loam (Light); Weak grade of structure, 2-5 mm, 
	Subangular blocky; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Very few (0 - 2 %), 
	Manganiferous, Fine (0 - 2 mm), Nodules; Common, very fine (0-1mm) roots; Gradual change to -
	 
	A3	0.25 - 0.38 m	Reddish brown (2.5YR4/4-Moist); , 2.5YR33, 10-20% , 15-30mm, Distinct; , 10-20% , 15-30mm, 
	Distinct; Clay loam; Weak grade of structure, 2-5 mm, Subangular blocky; Few (<1 per 100mm2) 
	Very fine (0.075-1mm) macropores, Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Nodules; 
	Few, very fine (0-1mm) roots; Diffuse change to - 
	B1	0.38 - 0.5 m	Dark red (2.5YR3/6-Moist); ; Light clay; Weak grade of structure, 5-10 mm, Subangular blocky; 
	Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Very few (0 - 2 %), Manganiferous, 
	Fine (0 - 2 mm), Nodules; Few, very fine (0-1mm) roots; Gradual change to - 
	B21	0.5 - 0.8 m	Red (2.5YR4/8-Moist); ; Light medium clay; Moderate grade of structure, 2-5 mm, Subangular 
	blocky; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Few (2 - 10 %), Manganiferous,
	 Medium (2 -6 mm), Nodules; Few, very fine (0-1mm) roots; Diffuse change to - 
	B22	0.8 - 1.1 m	Red (2.5YR4/8-Moist); ; Light medium clay; Moderate grade of structure, 5-10 mm, Subangular 
	blocky; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Few (2 - 10 %), Manganiferous,
	 Medium (2 -6 mm), Nodules; Few, very fine (0-1mm) roots; Diffuse change to - 
	B23	1.1 - 1.4 m	Red (2.5YR5/8-Moist); , 10YR78, 0-2% , 0-5mm, Faint; , 0-2% , 0-5mm, Faint; Medium clay; 
	Moderate grade of structure, 5-10 mm, Subangular blocky; Few (<1 per 100mm2) Very fine 
	(0.075-1mm) macropores, Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), Nodules; 
	1.4 - 1.6 m	Red (2.5YR5/8-Moist); , 10YR78, 2-10% , 0-5mm, Faint; , 2-10% , 0-5mm, Faint; Medium clay; 
	Weak grade of structure, 10-20 mm, Prismatic; Strong grade of structure, 5-10 mm, Subangular 
	blocky; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, 10-20%, medium gravelly, 6-
	20mm, rounded, dispersed, Clay, coarse fragments; Very few (0 - 2 %), Manganiferous, Medium 
	(2 -6 mm), Nodules; Diffuse change to - 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T442	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B24	1.6 - 1.8 m	Red (2.5YR5/8-Moist); , 10YR78, 2-10% , 0-5mm, Distinct; , 2-10% , 0-5mm, Distinct; Medium 
	clay; Weak grade of structure, 10-20 mm, Prismatic; Strong grade of structure, 5-10 mm, 
	Subangular blocky; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, 10-20%, medium 
	gravelly, 6-20mm, rounded, dispersed, Clay, coarse fragments; 
	Morphological Notes
	Observation Notes
	Site Notes
	CARDSTONE RD

	Project Name:	Regional
	Project Code:	REG	Site ID:	T442	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.12	4.45A	 0.177A	 0.23H	 0.54	 0.08	 0.12	 2.91F	 3A	 3.9F	4.00
	 13C	0.92
	0.12 - 0.25	4.88A	 0.053A
	0.25 - 0.38	5.09A	 0.027A	<0.02H	 0.07	 0.02	 0.03	 1.25F	 2.3A	 1.4F	1.30
	 6C	0.50
	0.38 - 0.5	5.1A	 0.022A
	0.5 - 0.8	5.04A	 0.022A	<0.02H	 0.2	<0.02	 0.02	 0.19F	 1.7A	 0.5F	1.18
	 3C	0.67
	0.8 - 1.1	4.97A	 0.023A
	1.1 - 1.4	4.95A	 0.021A	<0.02H	 0.14	<0.02	 0.03	 0.19F	 1.1A	 0.4F	2.73
	 2C	1.50
	1.4 - 1.6	5.05A	 0.018A
	1.6 - 1.8	4.96A	 0.018A	<0.02H	 0.12	<0.02	 0.03	 1.85F	 1A	 2F	3.00
	 3C	1.00
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.12	 5.25C	 7A	 0.044A	 0.27A	 0.17A	 2	 16D	 21	 14	 49
	 10B
	0.12 - 0.25	 0	 16D	 22	 12	 50
	0.25 - 0.38	 2C	 5B	 0.032A	 0.07A	 0.15A	 0	 16D	 22	 12	 50
	0.38 - 0.5	 0	 14D	 22	 11	 53
	0.5 - 0.8	 0.58C	 1A	 0.023A	 0.01A	 0.18A	 0	 12D	 20	 10	 58
	 5B
	0.8 - 1.1	 0	 10D	 19	 14	 58
	1.1 - 1.4	 0.29C	 4B	 0.02A	 0.25A	 0	 12D	 20	 10	 58
	1.4 - 1.6	 0	 8D	 22	 19	 51
	1.6 - 1.8	 5A	 0.017A	 0.37A	 0	 7D	 23	 21	 49
	 5B
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.12
	0.12 - 0.25
	0.25 - 0.38
	0.38 - 0.5
	0.5 - 0.8
	0.8 - 1.1
	1.1 - 1.4
	1.4 - 1.6
	1.6 - 1.8

	Project Name:	Regional
	Project Code:	REG	Site ID:	T442	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_FE	Total element - Fe(%) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6B3	Total organic carbon - high frequency induction furnace, infrared
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	9H1	Phosphate retention
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance