Project Name:	Regional
	Project Code:	REG	Site ID:	T45	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.F. Isbell	Locality:	South turnoff 6.9KM from Torrens Creek/Hazlerigg 
	Road:70M along south track:
	Date Desc.:	13/05/65	Elevation:	 457 metres
	Map Ref.:	Sheet No. : 7956   1:100000	Rainfall:	559
	Northing/Long.:	145.083333333333	Runoff:	Moderately rapid
	Easting/Lat.:	-20.7916666666667	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qs	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial fan
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Red Kandosol     	Principal Profile Form:	Gn2.11
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Heteropogon contortus, Plectrachne pungens
	Mid Strata - Tree, 1.01-3m, Very sparse. *Species includes - Acacia coriacea
	Tall Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus similis, Eucalyptus dichromophloia, Eucalyptus 
	drepanophylla
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark reddish brown (2.5YR3/4-Moist); Reddish brown (2.5YR4/4-Dry); ; Sandy loam (Heavy); 
	Massive grade of structure; Dry; Very firm consistence; Field pH 5.5 (pH meter); Gradual change 
	to - 
	B1	0.1 - 0.3 m	Dark red (10R3/6-Moist); Red (10R4/6-Dry); ; Sandy loam (Heavy); Massive grade of structure; 
	Earthy fabric; Dry; Very firm consistence; Gradual change to - 
	B21	0.3 - 0.51 m	Dark red (10R3/6-Moist); Red (10R4/6-Dry); ; Sandy clay loam (Heavy); Massive grade of 
	structure; Earthy fabric; Dry; Very firm consistence; Gradual change to - 
	B22	0.51 - 0.76 m	Dark red (10R3/6-Moist); Red (10R4/6-Dry); ; Sandy clay loam (Light); Massive grade of structure; 
	Earthy fabric; Dry; Strong consistence; Gradual change to - 
	B23	0.76 - 1.07 m	Dark red (10R3/6-Moist); Red (10R4/6-Dry); ; Sandy medium clay; Massive grade of structure; 
	Earthy fabric; Dry; Strong consistence; Field pH 6 (pH meter, 1.02); Gradual change to - 
	B23	1.07 - 1.37 m	Dark red (10R3/6-Moist); Red (10R4/6-Dry); ; Sandy medium clay; Massive grade of structure; 
	Earthy fabric; Dry; Strong consistence; Gradual change to - 
	B3	1.37 - 1.68 m	Red (10R4/6-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Dry; Strong 
	consistence; 
	B3	1.68 - 1.98 m	Red (10R4/6-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Dry; Strong 
	consistence; 
	Morphological Notes
	Observation Notes
	SMALL FRAGEMENT OF FE.SANDSTONE IN 51-76CM HORIZON:                                                                     
	Site Notes
	TORRENS CK.

	Project Name:	Regional
	Project Code:	REG	Site ID:	T45	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.2A	<0.03A	 1.2B	 0.5	 0.18	 0.1	 2C	5.00
	0.1 - 0.3	6.5A	<0.03A
	0.3 - 0.51	6.4A	<0.02A	 1.3B	 0.6	 0.12	 0.2	 2C	10.00
	0.51 - 0.76	6.4A	<0.03A
	0.76 - 1.07	6.2A	<0.03A	 1B	 0.8	 0.08	 0.1	 3C	3.33
	1.07 - 1.37	6.1A	<0.03A
	1.37 - 1.68	6.1A	<0.03A
	1.68 - 1.98	6A	<0.03A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.67D	 4B	 0.019A	 0.04A	 0.04A	 58D	 21	 8	 16
	0.1 - 0.3	 0.2D	 0.02A
	0.3 - 0.51	 4B	<2	 61D	 17	 3	 17
	0.51 - 0.76
	0.76 - 1.07	 0.047A	 0.04A	 54D	 17	 5	 24
	1.07 - 1.37	 2B
	1.37 - 1.68
	1.68 - 1.98	 2B	 43D	 22	 6	 27
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.3
	0.3 - 0.51
	0.51 - 0.76
	0.76 - 1.07
	1.07 - 1.37
	1.37 - 1.68
	1.68 - 1.98

	Project Name:	Regional
	Project Code:	REG	Site ID:	T45	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	MIN_EC	Exchange Capacity - Minerology
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	XRD_C_Hm	Hematite - X-Ray Diffraction
	XRD_C_K2O	K2O - X-Ray Diffraction or Clay Fraction (air dry)
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction