Project Name:	Regional
	Project Code:	REG	Site ID:	T461	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.D. Smith	Locality:
	Date Desc.:	02/11/84	Elevation:	<1 metres
	Map Ref.:	Sheet No. : 8061   1:100000	Rainfall:	0
	Northing/Long.:	145.754166666667	Runoff:	Very slow
	Easting/Lat.:	-18	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qa	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Alluvial fan
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Fan	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:	Stable, No sheet erosion (sheet) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Acidic Dermosolic Redoxic Hydrosol     	Principal Profile Form:	Uf6.41
	ASC Confidence:	Great Soil Group:	No suitable group
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.13 m	Black (2.5Y2/0-Moist); ; Light medium clay (Sapric); Strong grade of structure, 5-10 mm, Angular
	 blocky; Moderate grade of structure, 2-5 mm, Cast; Clear change to - 
	A3	0.13 - 0.23 m	Grey (2.5Y5/1-Moist); , 10YR58, 2-10% , 0-5mm, Distinct; , 2-10% , 0-5mm, Distinct; Medium 
	heavy clay; Moderate grade of structure, 5-10 mm, Angular blocky; Clear change to - 
	B21	0.23 - 0.4 m	Light grey (2.5Y7/1-Moist); , 10YR78, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, Distinct; 
	Medium heavy clay; Moderate grade of structure, 50-100 mm, Prismatic; Strong grade of 
	structure, 5-10 mm, Angular blocky; 
	0.4 - 0.6 m	Light grey (2.5Y7/1-Moist); , 10YR78, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, Distinct; 
	Medium heavy clay; Moderate grade of structure, 50-100 mm, Prismatic; Strong grade of 
	structure, 5-10 mm, Angular blocky; 
	0.6 - 0.9 m	Light grey (2.5Y7/1-Moist); , 10YR78, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, Distinct; 
	Medium heavy clay; Moderate grade of structure, 50-100 mm, Prismatic; Strong grade of 
	structure, 5-10 mm, Angular blocky; Clear change to - 
	B22	0.9 - 1.35 m	Light grey (2.5Y7/1-Moist); , 10YR68, 20-50% , 30-mm, Prominent; , 20-50% , 30-mm, Prominent;
	 Medium heavy clay; Moderate grade of structure, 5-10 mm, Subangular blocky; Clear change to - 
	D1	1.35 - 1.45 m	Pale yellow (2.5Y7/4-Moist); ; Loamy coarse sand; Single grain grade of structure; 
	Morphological Notes
	Observation Notes
	ANAL BY DPI                                                                                                             
	Site Notes

	Project Name:	Regional
	Project Code:	REG	Site ID:	T461	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.4A	 0.15A	 3.5B	 1.5	 0.39	 0.46	 2.58F	 17.5C	2.63
	0.13 - 0.23	5A	 0.05A	 0.79B	 0.86	 0.19	 0.14	 1.9D	 6.9J	2.03
	0.3 - 0.4	5.2A	 0.02A	 0.46B	 0.82	 0.15	 0.11	 1.07D	 3.2J	3.44
	0.4 - 0.6	5.4A	 0.01A	 0.44B	 0.79	 0.06	 0.24
	0.6 - 0.9	5.4A	 0.02A	 0.35B	 1.3	 0.12	 0.37
	0.9 - 1.35	5.4A	 0.01A	 0.37B	 3.1	 0.18	 0.54	 0.62D	 5.1J	10.59
	1.35 - 1.45	5.5A	 0.02A	 0.24B	 2.1	 0.24	 0.43	 0.23D	 2.8J	15.36
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 4.67A	 4A	 0.3A	 1	 10A	 12	 19	 59
	 23B
	0.13 - 0.23	 1.12E	 0.08B	 16C	 18	 18	 47
	0.3 - 0.4	 0.35E	 0.03B	 36C	 22	 14	 27
	0.4 - 0.6	 21C	 28	 19	 32
	0.6 - 0.9	 25C	 20	 9	 46
	0.9 - 1.35	 0.1E	 28C	 29	 13	 29
	1.35 - 1.45	 46C	 23	 13	 18
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.13 - 0.23
	0.3 - 0.4
	0.4 - 0.6
	0.6 - 0.9
	0.9 - 1.35
	1.35 - 1.45

	Project Name:	Regional
	Project Code:	REG	Site ID:	T461	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1	Organic carbon - Walkley and Black
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded