Project Name:	Regional
	Project Code:	REG	Site ID:	T463	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.F. Isbell	Locality:	D.P.I. experiment farm:Leichardt block: site 68:
	Date Desc.:	01/07/86	Elevation:	No Data
	Map Ref.:	Sheet No. : 58   1:5000	Rainfall:	890
	Northing/Long.:	147.3175	Runoff:	Slow
	Easting/Lat.:	-19.81	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 CPg	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Pediment	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	270 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Eutrophic Brown Chromosol     	Principal Profile Form:	Dy3.12
	ASC Confidence:	Great Soil Group:	No suitable group
	All necessary analytical data are available.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.15 m	Dark brown (10YR3/3-Moist); Brown (10YR5/3-Dry); ; Sandy clay loam (Light); Massive grade of 
	structure; Common, fine (1-2mm) roots; Gradual, Smooth change to - 
	A3	0.15 - 0.27 m	Dark yellowish brown (10YR3/4-Moist); Dark yellowish brown (10YR4/4-Dry); ; Sandy clay loam 
	(Heavy); Massive grade of structure; Very few (0 - 2 %), Ferruginous, Fine (0 - 2 mm), Nodules; 
	Few, fine (1-2mm) roots; Clear, Smooth change to - 
	B21	0.27 - 0.42 m	Strong brown (7.5YR5/6-Moist); , 2.5YR48, 2-10% , 0-5mm, Distinct; , 2-10% , 0-5mm, Distinct; 
	Sandy medium clay; Weak grade of structure, 10-20 mm, Subangular blocky; Few (2 - 10 %), 
	Ferruginous, Fine (0 - 2 mm), Nodules; Few, very fine (0-1mm) roots; Diffuse change to - 
	B22	0.42 - 0.57 m	Strong brown (7.5YR5/6-Moist); , 2.5YR48, 2-10% , 0-5mm, Distinct; , 2-10% , 0-5mm, Distinct; 
	Medium clay; Moderate grade of structure, 20-50 mm, Angular blocky; 2-10%, fine gravelly, 2-
	6mm, angular, dispersed, Quartz, coarse fragments; Common (10 - 20 %), Ferruginous, Medium 
	(2 -6 mm), Nodules; Few, very fine (0-1mm) roots; Diffuse change to - 
	B23	0.57 - 0.91 m	Strong brown (7.5YR5/6-Moist); , 2.5YR48, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, 
	Distinct; Medium clay; Weak grade of structure, 10-20 mm, Subangular blocky; 2-10%, medium 
	gravelly, 6-20mm, angular, dispersed, Quartz, coarse fragments; Many (20 - 50 %), Ferruginous, 
	Medium (2 -6 mm), Nodules; Few, very fine (0-1mm) roots; Clear, Wavy change to - 
	B3	0.91 - 1.11 m	Brownish yellow (10YR6/5-Moist); , 5YR48, 2-10% , 0-5mm, Distinct; , 10YR74, 2-10% , 0-5mm, 
	Distinct; Medium clay; Weak grade of structure, 50-100 mm, Lenticular; Moderate grade of 
	structure, 10-20 mm, Subangular blocky; Few, very fine (0-1mm) roots; Gradual change to - 
	BC	1.11 - 1.41 m	Brownish yellow (10YR6/5-Moist); , 10YR72, 10-20% , 5-15mm, Distinct; , 7.5YR56, 10-20% , 5-
	15mm, Distinct; Medium clay; Few (2 - 10 %), Ferruginous, Fine (0 - 2 mm), Soft segregations; 
	Few, very fine (0-1mm) roots; 
	Morphological Notes
	BC	Rock sample from pit:
	Observation Notes
	C HORIZON PROBABLY AT 120CM:                                                                                            
	Site Notes
	BURDEKIN VALLE

	Project Name:	Regional
	Project Code:	REG	Site ID:	T463	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)

	Project Name:	Regional
	Project Code:	REG	Site ID:	T463	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	6.4A	 0.05A	 3.65H	 1.37	 0.14	 0.08	 13.5A	 5.2F	0.59
	 4C	2.00
	0.15 - 0.27	6.6A	 0.03A
	0.27 - 0.42	6.4A	 0.03A	 6.57H	 3.27	 0.06	 0.08	 10.3A	 10F	0.78
	 8C	1.00
	0.42 - 0.57	6.7A	 0.03A
	0.57 - 0.91	6.5A	 0.03A	 7.88H	 4	 0.06	 0.12	 8.2A	 12.1F	1.46
	 9C	1.33
	0.91 - 1.11	7.2A	 0.03A
	1.11 - 1.41	7A	 0.04A	 19.5H	 14.2	 0.03	 0.27	 14.6A	 34F	1.85
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	 9A	 0	 48A	 37	 6	 9
	 5B
	0.15 - 0.27	 7A	 0	 45A	 33	 6	 17
	<3B
	0.27 - 0.42	 0	 37A	 23	 4	 36
	0.42 - 0.57	 0	 34A	 17	 3	 46
	0.57 - 0.91	 0	 34A	 21	 5	 41
	0.91 - 1.11	 0	 14A	 40	 13	 32
	1.11 - 1.41	 0	 17A	 51	 15	 18
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.27
	0.27 - 0.42
	0.42 - 0.57
	0.57 - 0.91
	0.91 - 1.11
	1.11 - 1.41

	Project Name:	Regional
	Project Code:	REG	Site ID:	T463	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J1	Effective CEC
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)