Project Name:	Regional
	Project Code:	REG	Site ID:	T5	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	Locality:
	Date Desc.:	//	Elevation:	No Data
	Map Ref.:	Sheet No. : 8158   1:100000	Rainfall:	0
	Northing/Long.:	146.4875	Runoff:	Rapid
	Easting/Lat.:	-19.7291666666667	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	 SDr	Substrate Material:	Granodiorite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Eutrophic Red Chromosol     	Principal Profile Form:	Dr2.2
	ASC Confidence:	Great Soil Group:	Red-brown earth
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Heteropogon contortus
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Eucalyptus drepanophylla, Eucalyptus dichromophloia, 
	Eucalyptus papuana
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Dark reddish brown (5YR3/3-Moist); Brown (7.5YR5/4-Dry); ; Coarse sandy loam; Massive grade 
	of structure; Moist; Firm consistence; 
	A2	0.1 - 0.18 m	Dark reddish brown (5YR3/4-Moist); Reddish brown (5YR4/4-Dry); ; Clay loam, coarse sandy; 
	Massive grade of structure; Dry; Very strong consistence; Gradual change to - 
	B21	0.18 - 0.36 m	Dark red (2.5YR3/6-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, Subangular 
	blocky; Dry; Weak consistence; Clear change to - 
	BC	0.36 - 0.5 m	Red (2.5YR4/6-Moist); ; Medium clay; Weak grade of structure, 20-50 mm, Subangular blocky; 
	Moist; Weak consistence; 0-2%, Granite, coarse fragments; Gradual change to - 
	C	0.5 - 0.76 m	; Gradual change to - 
	Morphological Notes
	C	Weathered granite with pockets of red medium clay:
	Observation Notes
	C HORIZON: WEATHERED FRIABLE GRANITE ROCK WITH POCKETS RED MEDIUM CLAY:                                                 
	Site Notes
	FANNING RIVER

	Project Name:	Regional
	Project Code:	REG	Site ID:	T5	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.3A	 0.029A	 3.2B	 1	 0.36	 0.2	 6C	3.33
	0.1 - 0.18	6.3A	 0.035A	 3.4B	 1.3	 0.34	 0.2	 5C	4.00
	0.18 - 0.36	6.5A	 0.044A	 7.6B	 2.3	 0.35	 0.4	 12C	3.33
	0.36 - 0.5	6.8A	 0.041A	 8.9B	 3.4	 0.31	 0.05	 12C	0.42
	0.5 - 0.76	6.9A	 0.047A	 6.8B	 3.5	 0.29	 0.7	 11C	6.36
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.87D	 11B	 0.01A	 0.05A	 2.14A	 10	 63D	 20	 7	 10
	0.1 - 0.18	 0.45D	 7B	 0.004A	 0.04A	 2.06A	 5	 58D	 19	 7	 16
	0.18 - 0.36	 0.67D	 3B	 0.005A	 0.06A	 1.45A	 3	 30D	 10	 10	 50
	0.36 - 0.5	 3B	 0.005A	 1.42A	 23	 29D	 14	 11	 45
	0.5 - 0.76	 15B	 0.01A	 1.55A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.18
	0.18 - 0.36
	0.36 - 0.5
	0.5 - 0.76

	Project Name:	Regional
	Project Code:	REG	Site ID:	T5	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	MIN_EC	Exchange Capacity - Minerology
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_K2O	K2O - X-Ray Diffraction or Clay Fraction (air dry)
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_St	Smectite - X-Ray Diffraction