Project Name:	Regional
	Project Code:	REG	Site ID:	T50	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R.F. Isbell	Locality:	Adjacent to Otterburn siding 3.2KM east of Mirani:
	Date Desc.:	06/07/65	Elevation:	 30 metres
	Map Ref.:	Sheet No. : 8655   1:100000	Rainfall:	1400
	Northing/Long.:	148.883333333333	Runoff:	Very slow
	Easting/Lat.:	-21.1625	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qa	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	No Data	Relief:	0 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Chomosolic Oxyaquic Hydrosol     	Principal Profile Form:	Dy3.33
	ASC Confidence:	Great Soil Group:	Solodic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Imperata cylindrica
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Melaleuca viridiflora
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus tessellaris
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.09 m	Dark greyish brown (10YR4/2-Moist); Light brownish grey (10YR6/2-Dry); , 10YR58, 0-2% , 0-
	5mm, Faint; , 0-2% , 0-5mm, Faint; Sandy loam; Weak grade of structure, 5-10 mm, Subangular 
	blocky; Firm consistence; Clear change to - 
	A2	0.09 - 0.18 m	Grey (10YR5/1-Moist); Light grey (10YR7/1-Dry); , 10YR58, 2-10% , 0-5mm, Faint; , 2-10% , 0-
	5mm, Faint; Sandy loam; Massive grade of structure; Firm consistence; Very few (0 - 2 %), 
	Manganiferous, Medium (2 -6 mm), Nodules; Abrupt change to - 
	B21	0.18 - 0.33 m	Grey (10YR5/1-Moist); , 10YR56, 10-20% , 0-5mm, Distinct; , 10-20% , 0-5mm, Distinct; Heavy 
	clay; Weak grade of structure, 20-50 mm, Subangular blocky; Very plastic; Normal plasticity; 
	Gradual change to - 
	B22	0.33 - 0.56 m	Greyish brown (10YR5/2-Moist); , 10YR44, 10-20% , 0-5mm, Faint; , 10-20% , 0-5mm, Faint; 
	Heavy clay; Weak grade of structure, 20-50 mm, Subangular blocky; Very plastic; Normal 
	plasticity; 
	B22	0.56 - 0.76 m	Greyish brown (10YR5/2-Moist); , 10YR44, 10-20% , 0-5mm, Faint; , 10-20% , 0-5mm, Faint; 
	Heavy clay; Weak grade of structure, 20-50 mm, Subangular blocky; Very plastic; Normal 
	plasticity; Gradual change to - 
	BC	0.76 - 0.97 m	Greyish brown (10YR5/2-Moist); , 10YR44, 10-20% , 0-5mm, Distinct; , 10-20% , 0-5mm, 
	Distinct; Medium clay; Massive grade of structure; Very plastic; Normal plasticity; Very few (0 - 2
	 %), Manganiferous, Medium (2 -6 mm), Nodules; Very few (0 - 2 %), Calcareous, , Soft 
	segregations; Gradual change to - 
	BC	0.97 - 1.17 m	Grey (10YR5/1-Moist); , 10YR58, 2-10% , 0-5mm, Distinct; , 2-10% , 0-5mm, Distinct; Medium 
	clay; Very plastic; Normal plasticity; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), 
	Nodules; Common (10 - 20 %), Calcareous, , Soft segregations; Gradual change to - 
	C	1.17 - 1.32 m	Light brownish grey (10YR6/2-Moist); , 10YR58, 2-10% , 0-5mm, Distinct; , 2-10% , 0-5mm, 
	Distinct; Sandy medium clay; Weak consistence; Very few (0 - 2 %), Manganiferous, Medium (2 -
	6 mm), Nodules; Very few (0 - 2 %), Calcareous, , Soft segregations; Clear change to - 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T50	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	D	1.32 - 1.47 m	Light yellowish brown (10YR6/4-Moist); , 10YR58, 2-10% , 0-5mm, Faint; , 2-10% , 0-5mm, Faint;
	 Sandy clay loam; Very strong consistence; Very few (0 - 2 %), Manganiferous, , Soft 
	segregations; Very few (0 - 2 %), Calcareous, , Nodules; 
	Morphological Notes
	Observation Notes
	Site Notes
	MIRANI

	Project Name:	Regional
	Project Code:	REG	Site ID:	T50	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.09	5.5A	 0.047A	 2.6B	 1.3	 0.19	 0.4	 9C	4.44
	0.09 - 0.18	5.8A	 0.029A	 2.4B	 1.3	 0.1	 0.5	 7C	7.14
	0.18 - 0.33	5.5A	 0.059A	 5B	 6.8	 0.16	 0.3	 18C	1.67
	0.33 - 0.56	5.5A	 0.119A	 6.5B	 8	 0.2	 1.8	 18C	10.00
	0.56 - 0.76	6.3A	 0.229A	 6.5B	 8	 0.1	 2.1	 17C	12.35
	0.76 - 0.97	7.8A	 2.59A	 5B	 6	 0.05	 2	 14C	14.29
	0.97 - 1.17	8.6A	 0.428A	 6.4B	 6.4	 0.06	 2	 15C	13.33
	1.17 - 1.32	8.8A	 0.419A	 8B	 6.9	 0.06	 2	 13C	15.38
	1.32 - 1.47	8.7A	 0.601A	 10.5B	 10	 5.7	 22C	25.91
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.09	 1.35D	 13B	 0.02A	 0.11A	 6D	 41	 34	 20
	0.09 - 0.18	 0.59D	 4B	 0.06A	<2	 8D	 40	 34	 18
	0.18 - 0.33	 0.4D	 0.05A	 3D	 16	 16	 62
	0.33 - 0.56	 2B	 0.009A	 3D	 17	 20	 58
	0.56 - 0.76
	0.76 - 0.97	 11B
	0.97 - 1.17
	1.17 - 1.32	 6B	 0.009A
	1.32 - 1.47
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.09
	0.09 - 0.18
	0.18 - 0.33
	0.33 - 0.56
	0.56 - 0.76
	0.76 - 0.97
	0.97 - 1.17
	1.17 - 1.32
	1.32 - 1.47

	Project Name:	Regional
	Project Code:	REG	Site ID:	T50	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance