Project Name:	Regional
	Project Code:	REG	Site ID:	T61	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.G. Murtha	Locality:	13.3KM southwest of Bobawaba on Rangemeore 
	Road:1.9KM south west of creek at Liechhardt Mill:
	Date Desc.:	04/04/68	Elevation:	 122 metres
	Map Ref.:	Sheet No. : 8458   1:100000	Rainfall:	0
	Northing/Long.:	147.522222222222	Runoff:	No Data
	Easting/Lat.:	-19.9125	Drainage:	No Data
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Cpd	Substrate Material:	Existing vertical exposure, Granodiorite 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	30 metres
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	5 % 	Aspect:	45 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melanic Eutrophic Red Dermosol     	Principal Profile Form:	Dr2.12
	ASC Confidence:	Great Soil Group:	Non-calcic brown 
	All necessary analytical data are available.	soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Heteropogon contortus, Heteropogon triticeus
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus polycarpa, Melaleuca viridiflora
	Surface Coarse Fragments:	2-10%, cobbly, 60-200mm, , 
	Profile Morphology
	A11	0 - 0.1 m	Dark reddish brown (5YR3/2-Moist); Dark brown (7.5YR3/2-Dry); , 0-0% ; , 0-0% ; Loam; Weak 
	grade of structure, 2-5 mm, Subangular blocky; Moderately moist; Weak consistence; Gradual 
	change to - 
	A12	0.1 - 0.2 m	Dark reddish brown (5YR3/2-Moist); , 5YR34, 2-10% ; , 2-10% ; Loam; Weak grade of structure, 
	5-10 mm, Subangular blocky; Moderately moist; Strong consistence; Gradual change to - 
	A3	0.2 - 0.25 m	Dark reddish brown (5YR3/2-Moist); , 2.5YR36; Clay loam; Moderate grade of structure, 5-10 mm,
	 Subangular blocky; Coarse, (10 - 20) mm crack; Moderately moist; Strong consistence; 0-2%, 
	medium gravelly, 6-20mm, Gravel, coarse fragments; Clear change to - 
	B21	0.25 - 0.3 m	Dark red (2.5YR3/6-Moist); , 5YR32, 2-10% ; , 2-10% ; Medium clay; 5-10 mm, Angular blocky; 
	Moderate grade of structure, 2-5 mm, Angular blocky; Coarse, (10 - 20) mm crack; Moderately 
	moist; Strong consistence; Diffuse change to - 
	B22	0.3 - 0.4 m	Dark red (2.5YR3/6-Moist); , 0-0% ; , 0-0% ; Medium clay; 5-10 mm, Angular blocky; Moderate 
	grade of structure, 2-5 mm, Angular blocky; Coarse, (10 - 20) mm crack; Moderately moist; 
	Strong consistence; Diffuse change to - 
	B22	0.4 - 0.5 m	Dark red (2.5YR3/6-Moist); , 0-0% ; , 0-0% ; Light medium clay; Moderate grade of structure, 5-10 
	mm, Angular blocky; Moderately moist; Strong consistence; Gradual change to - 
	BC	0.5 - 0.6 m	Red (2.5YR4/6-Moist); , 0-0% ; , 0-0% ; Light clay (Light); Weak grade of structure, 10-20 mm, 
	Angular blocky; Moist; Weak consistence; Gradual change to - 
	C	0.6 - 0.9 m	Reddish brown (5YR4/4-Moist); ; Sandy clay loam (Light); Massive grade of structure; Moist; Very
	 weak consistence; Diffuse change to - 
	C	0.9 - 1.1 m	Reddish brown (5YR4/4-Moist); ; Sandy loam; Massive grade of structure; Moist; Very weak 
	consistence; 
	Morphological Notes
	Observation Notes
	LARGE WORM CASTS OF A HORIZON MATERIAL 20-40CM:>50CM WEATHERED PARENT MATERIAL INCREASING DOWN
	 PROFILE:                 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T61	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Notes
	BOBAWABA

	Project Name:	Regional
	Project Code:	REG	Site ID:	T61	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.4A	 0.047A	 6.8B	 2.4	 0.65	 0.28	 10C	2.80
	0.1 - 0.2	6.3A	 0.041A	 8.2B	 2.4	 0.51	 0.33	 12C	2.75
	0.2 - 0.25	6.2A	 0.047A	 8.3B	 2.6	 0.47	 0.29	 12C	2.42
	0.25 - 0.3	6.3A	 0.044A	 9.1B	 3.7	 0.31	 0.4	 14C	2.86
	0.3 - 0.4	6.3A	 0.044A	 9.2B	 4.4	 0.46	 0.41	 14C	2.93
	0.4 - 0.5	6.4A	 0.047A	 8.6B	 4.4	 0.15	 0.5	 14C	3.57
	0.5 - 0.6	6.7A	 0.038A
	0.6 - 0.9	7A	 0.041A
	0.9 - 1.1	7.1A	 0.038A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.77D	 32B	 0.056A	 0.11A	 0.98A	<2	 30D	 27	 15	 25
	0.1 - 0.2	 1.35D	 7B	 0.08A	 0	 26D	 28	 17	 27
	0.2 - 0.25	 1.02D	 4B	 0.041A	 0.07A	 0.85A	 0	 22D	 24	 16	 37
	0.25 - 0.3	 0.78D	 2B	 0.039A	 0.06A	 0.54A	 0	 13D	 12	 15	 56
	0.3 - 0.4	 2B	 0.039A	 0.4A	<2	 12D	 10	 19	 60
	0.4 - 0.5	 7B	<2	 13D	 14	 20	 51
	0.5 - 0.6	 20B	 2	 18D	 20	 19	 39
	0.6 - 0.9	 190B
	0.9 - 1.1	 560B	 0.098A	 0.79A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.25
	0.25 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.9
	0.9 - 1.1

	Project Name:	Regional
	Project Code:	REG	Site ID:	T61	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	MIN_EC	Exchange Capacity - Minerology
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_K2O	K2O - X-Ray Diffraction or Clay Fraction (air dry)
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_St	Smectite - X-Ray Diffraction