Project Name:	Regional
	Project Code:	REG	Site ID:	T92	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.G. Murtha	Locality:	2.4KM north of Meadow Bank homestead:12M south 
	west from south west corner of DPI plots:
	Date Desc.:	22/05/69	Elevation:	 730 metres
	Map Ref.:	Sheet No. : 7861   1:100000	Rainfall:	890
	Northing/Long.:	144.966666666667	Runoff:	Moderately rapid
	Easting/Lat.:	-18.7333333333333	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Czm	Substrate Material:	Undisturbed soil core, Basalt 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	0 metres
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Dystrophic Red Ferrosol     	Principal Profile Form:	Gn3.12
	ASC Confidence:	Great Soil Group:	Euchrozem
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus tereticornis
	Surface Coarse Fragments:	2-10%, , , Gravel
	Profile Morphology
	A1	0 - 0.1 m	Dark reddish brown (5YR3/3-Moist); ; Loam (Heavy); Moderate grade of structure, 5-10 mm, 
	Angular blocky; Dry; Very firm consistence; FewGradual change to - 
	A3	0.1 - 0.2 m	Dark reddish brown (5YR3/4-Moist); ; Loam (Heavy); Moderate grade of structure, 5-10 mm, 
	Angular blocky; Dry; Very firm consistence; FewGradual change to - 
	B1	0.2 - 0.3 m	Yellowish red (5YR3/6-Moist); ; Clay loam; Strong grade of structure, 5-10 mm, Angular blocky; 
	Smooth-ped fabric; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Very firm 
	consistence; Diffuse change to - 
	B21	0.3 - 0.6 m	Dark red (2.5YR3/6-Moist); ; Light medium clay; Strong grade of structure, 5-10 mm, Angular 
	blocky; Smooth-ped fabric; Dry; Very firm consistence; 0-2%, Basalt, coarse fragments; Diffuse 
	change to - 
	B22	0.6 - 0.9 m	Dark red (2.5YR3/6-Moist); ; Medium clay; Strong grade of structure, 5-10 mm, Angular blocky; 
	Smooth-ped fabric; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Very firm 
	consistence; 0-2%, Basalt, coarse fragments; 
	B22	0.9 - 1.2 m	Dark red (2.5YR3/6-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, Angular blocky; 
	Dry; Firm consistence; 0-2%, coarse gravelly, 20-60mm, Basalt, coarse fragments; 
	B22	1.2 - 1.5 m	Dark red (2.5YR3/6-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, Angular blocky; 
	Dry; Firm consistence; 2-10%, coarse gravelly, 20-60mm, Basalt, coarse fragments; Diffuse 
	change to - 
	B23	1.5 - 1.8 m	Dark reddish brown (5YR3/4-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, 
	Angular blocky; Dry; Firm consistence; 2-10%, coarse gravelly, 20-60mm, Basalt, coarse 
	fragments; 
	BC	1.8 - 2.1 m	Dark reddish brown (5YR3/4-Moist); ; Light medium clay; Weak grade of structure, 5-10 mm, 
	Angular blocky; Many (>5 per 100mm2) Fine (1-2mm) macropores, Dry; Weak consistence; 
	BC	2.1 - 2.3 m	Dark reddish brown (5YR3/4-Moist); ; Light medium clay; Weak grade of structure, 5-10 mm, 
	Angular blocky; Many (>5 per 100mm2) Fine (1-2mm) macropores, Dry; Weak consistence; 

	Project Name:	Regional
	Project Code:	REG	Site ID:	T92	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	C	2.3 - 2.6 m	; 
	Morphological Notes
	C	Weathered basalt:
	Observation Notes
	180-260CM SOFT WEATHERED BASALT INCREASING DOWN PROFILE:                                                                
	Site Notes
	MEADOW BANK

	Project Name:	Regional
	Project Code:	REG	Site ID:	T92	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.6A	 0.029A	 13.3B	 3.7	 1.3	 0.41
	0.1 - 0.2	6.3A	 0.02A	 11.2B	 2.4	 0.96	 0.39
	0.2 - 0.3	6.3A	 0.023A	 8.3B	 1.9	 0.87	 0.33
	0.3 - 0.6	6.4A	 0.014A	 4.9B	 1.5	 0.71	 0.28
	0.6 - 0.9	6.5A	 0.014A
	0.9 - 1.2	6.6A	 0.011A	 4.3B	 2.1	 0.64	 0.26
	1.2 - 1.5	6.7A	 0.011A
	1.5 - 1.8	6.6A	 0.011A	 4.6B	 3.2	 1.98	 0.44F
	1.8 - 2.1	6.7A	 0.011A
	2.1 - 2.3	6.7A	 0.014A
	2.3 - 2.6	6.7A	 0.014A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 2.22D	 283A	 0.48A	 0.15A	 0.35A	 1D	 11	 29	 58
	 270B
	0.1 - 0.2	 1.59D	 299A	 0.46A	 0.104A	 0.32A	 2D	 7	 18	 54
	 252B
	0.2 - 0.3	 1D	 286A	 0.44A	 0.074A	 0.3A	<2	 2D	 6	 19	 62
	 226B
	0.3 - 0.6	 0.37D	 138A	 0.33A	 0.036A	 0.26A	<2	 1D	 8	 26	 67
	 110B
	0.6 - 0.9
	0.9 - 1.2	 0.08D	 70.9B	 0.34A	 0.012A	 0.19A	 2D	 5	 26	 65
	1.2 - 1.5
	1.5 - 1.8	 0.08D	 92.7B	 0.4A	 0.005A	 0.18A	<2	 3D	 14	 27	 41
	1.8 - 2.1
	2.1 - 2.3	 0.31A	 0.3A	 4D	 15	 26	 43
	2.3 - 2.6
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.5
	1.5 - 1.8
	1.8 - 2.1
	2.1 - 2.3
	2.3 - 2.6

	Project Name:	Regional
	Project Code:	REG	Site ID:	T92	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_FE	Total element - Fe(%) - HF/HClO4 Digest
	12_HF_MN	Total element - Mn(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	17A1	Total potassium - X-ray fluorescence
	2_LOI	Loss on Ignition (%)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	9H1	Phosphate retention
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	XRD_C_Hm	Hematite - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Mh	Meghemite - X-Ray Diffraction